From 0cc8daf2488539f734150e64c799e3a4dd014cd8 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Mon, 19 Jan 2015 11:34:45 +0100
Subject: [PATCH] ARM: BCM5301X: Add DT for Asus RT-AC87U
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
---
 arch/arm/boot/dts/Makefile                  |  3 +-
 arch/arm/boot/dts/bcm4709-asus-rt-ac87u.dts | 44 +++++++++++++++++++++++++++++
 2 files changed, 46 insertions(+), 1 deletion(-)
 create mode 100644 arch/arm/boot/dts/bcm4709-asus-rt-ac87u.dts

--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -64,6 +64,7 @@ dtb-$(CONFIG_ARCH_BCM_5301X) += \
 	bcm47081-asus-rt-n18u.dtb \
 	bcm47081-buffalo-wzr-600dhp2.dtb \
 	bcm47081-buffalo-wzr-900dhp.dtb \
+	bcm4709-asus-rt-ac87u.dtb \
 	bcm4709-netgear-r8000.dtb
 dtb-$(CONFIG_ARCH_BCM_63XX) += bcm963138dvt.dtb
 dtb-$(CONFIG_ARCH_BCM_MOBILE) += bcm28155-ap.dtb \
--- /dev/null
+++ b/arch/arm/boot/dts/bcm4709-asus-rt-ac87u.dts
@@ -0,0 +1,44 @@
+/*
+ * Broadcom BCM470X / BCM5301X ARM platform code.
+ * DTS for Asus RT-AC87U
+ *
+ * Copyright (C) 2015 Rafał Miłecki <zajec5@gmail.com>
+ *
+ * Licensed under the GNU/GPL. See COPYING for details.
+ */
+
+/dts-v1/;
+
+#include "bcm4708.dtsi"
+
+/ {
+	compatible = "asus,rt-ac87u", "brcm,bcm4709", "brcm,bcm4708";
+	model = "Asus RT-AC87U (BCM4709)";
+
+	chosen {
+		bootargs = "console=ttyS0,115200 earlyprintk";
+	};
+
+	memory {
+		reg = <0x00000000 0x08000000
+		       0x88000000 0x08000000>;
+	};
+
+	gpio-keys {
+		compatible = "gpio-keys";
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		wps {
+			label = "WPS";
+			linux,code = <KEY_WPS_BUTTON>;
+			gpios = <&chipcommon 2 GPIO_ACTIVE_LOW>;
+		};
+
+		restart {
+			label = "Reset";
+			linux,code = <KEY_RESTART>;
+			gpios = <&chipcommon 11 GPIO_ACTIVE_LOW>;
+		};
+	};
+};
