From 4a658590f83c1e916ab63ed7fe6f0841924247db Mon Sep 17 00:00:00 2001
From: Hauke Mehrtens <hauke@hauke-m.de>
Date: Fri, 3 Oct 2014 18:37:33 +0200
Subject: [PATCH 2/2] ARM: BCM53XX: set customized AUXCTL

This activated some more features in the l310 cache.

This is based on some vendor code

Signed-off-by: Hauke Mehrtens <hauke@hauke-m.de>
---
 arch/arm/mach-bcm/bcm_5301x.c | 5 ++++-
 1 file changed, 4 insertions(+), 1 deletion(-)

--- a/arch/arm/mach-bcm/bcm_5301x.c
+++ b/arch/arm/mach-bcm/bcm_5301x.c
@@ -50,7 +50,11 @@ static const char __initconst *bcm5301x_
 };
 
 DT_MACHINE_START(BCM5301X, "BCM5301X")
-	.l2c_aux_val	= 0,
+	.l2c_aux_val	= L310_AUX_CTRL_CACHE_REPLACE_RR |
+			  L310_AUX_CTRL_DATA_PREFETCH |
+			  L310_AUX_CTRL_INSTR_PREFETCH |
+			  L310_AUX_CTRL_EARLY_BRESP |
+			  L310_AUX_CTRL_FULL_LINE_ZERO,
 	.l2c_aux_mask	= ~0,
 	.init_early	= bcm5301x_init_early,
 	.dt_compat	= bcm5301x_dt_compat,
