From 6ab7c29099390b3d23c97f14498fd26a5ef6b22b Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Wed, 1 Apr 2015 08:23:04 +0200
Subject: [PATCH] MIPS: BCM47XX: Increase NVRAM buffer size to 64 KiB
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

For years Broadcom devices use 64 KiB NVRAM partition size and some of
them indeed have it filled in more than 50%. This change allows reading
whole NVRAM e.g. on Netgear WNDR4500 and Netgear R8000.

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
Cc: linux-mips@linux-mips.org
Cc: Hauke Mehrtens <hauke@hauke-m.de>
Patchwork: https://patchwork.linux-mips.org/patch/9651/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
---
 arch/mips/bcm47xx/nvram.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/arch/mips/bcm47xx/nvram.c b/arch/mips/bcm47xx/nvram.c
index 2357ea3..2ac7482 100644
--- a/arch/mips/bcm47xx/nvram.c
+++ b/arch/mips/bcm47xx/nvram.c
@@ -20,7 +20,7 @@
 #include <linux/bcm47xx_nvram.h>
 
 #define NVRAM_MAGIC			0x48534C46	/* 'FLSH' */
-#define NVRAM_SPACE			0x8000
+#define NVRAM_SPACE			0x10000
 #define NVRAM_MAX_GPIO_ENTRIES		32
 #define NVRAM_MAX_GPIO_VALUE_LEN	30
 
-- 
1.8.4.5

