--- a/drivers/tty/serial/amba-pl010.c
+++ b/drivers/tty/serial/amba-pl010.c
@@ -48,11 +48,9 @@
 #include <linux/slab.h>
 #include <linux/io.h>
 
-#define UART_NR		8
-
 #define SERIAL_AMBA_MAJOR	204
 #define SERIAL_AMBA_MINOR	16
-#define SERIAL_AMBA_NR		UART_NR
+#define SERIAL_AMBA_NR		CONFIG_SERIAL_AMBA_PL010_NUMPORTS
 
 #define AMBA_ISR_PASS_LIMIT	256
 
@@ -78,9 +76,9 @@ static void pl010_stop_tx(struct uart_po
 	struct uart_amba_port *uap = (struct uart_amba_port *)port;
 	unsigned int cr;
 
-	cr = readb(uap->port.membase + UART010_CR);
+	cr = __raw_readl(uap->port.membase + UART010_CR);
 	cr &= ~UART010_CR_TIE;
-	writel(cr, uap->port.membase + UART010_CR);
+	__raw_writel(cr, uap->port.membase + UART010_CR);
 }
 
 static void pl010_start_tx(struct uart_port *port)
@@ -88,9 +86,9 @@ static void pl010_start_tx(struct uart_p
 	struct uart_amba_port *uap = (struct uart_amba_port *)port;
 	unsigned int cr;
 
-	cr = readb(uap->port.membase + UART010_CR);
+	cr = __raw_readl(uap->port.membase + UART010_CR);
 	cr |= UART010_CR_TIE;
-	writel(cr, uap->port.membase + UART010_CR);
+	__raw_writel(cr, uap->port.membase + UART010_CR);
 }
 
 static void pl010_stop_rx(struct uart_port *port)
@@ -98,9 +96,9 @@ static void pl010_stop_rx(struct uart_po
 	struct uart_amba_port *uap = (struct uart_amba_port *)port;
 	unsigned int cr;
 
-	cr = readb(uap->port.membase + UART010_CR);
+	cr = __raw_readl(uap->port.membase + UART010_CR);
 	cr &= ~(UART010_CR_RIE | UART010_CR_RTIE);
-	writel(cr, uap->port.membase + UART010_CR);
+	__raw_writel(cr, uap->port.membase + UART010_CR);
 }
 
 static void pl010_enable_ms(struct uart_port *port)
@@ -108,18 +106,18 @@ static void pl010_enable_ms(struct uart_
 	struct uart_amba_port *uap = (struct uart_amba_port *)port;
 	unsigned int cr;
 
-	cr = readb(uap->port.membase + UART010_CR);
+	cr = __raw_readl(uap->port.membase + UART010_CR);
 	cr |= UART010_CR_MSIE;
-	writel(cr, uap->port.membase + UART010_CR);
+	__raw_writel(cr, uap->port.membase + UART010_CR);
 }
 
 static void pl010_rx_chars(struct uart_amba_port *uap)
 {
 	unsigned int status, ch, flag, rsr, max_count = 256;
 
-	status = readb(uap->port.membase + UART01x_FR);
+	status = __raw_readl(uap->port.membase + UART01x_FR);
 	while (UART_RX_DATA(status) && max_count--) {
-		ch = readb(uap->port.membase + UART01x_DR);
+		ch = __raw_readl(uap->port.membase + UART01x_DR);
 		flag = TTY_NORMAL;
 
 		uap->port.icount.rx++;
@@ -128,9 +126,9 @@ static void pl010_rx_chars(struct uart_a
 		 * Note that the error handling code is
 		 * out of the main execution path
 		 */
-		rsr = readb(uap->port.membase + UART01x_RSR) | UART_DUMMY_RSR_RX;
+		rsr = __raw_readl(uap->port.membase + UART01x_RSR) | UART_DUMMY_RSR_RX;
 		if (unlikely(rsr & UART01x_RSR_ANY)) {
-			writel(0, uap->port.membase + UART01x_ECR);
+			__raw_writel(0, uap->port.membase + UART01x_ECR);
 
 			if (rsr & UART01x_RSR_BE) {
 				rsr &= ~(UART01x_RSR_FE | UART01x_RSR_PE);
@@ -160,7 +158,7 @@ static void pl010_rx_chars(struct uart_a
 		uart_insert_char(&uap->port, rsr, UART01x_RSR_OE, ch, flag);
 
 	ignore_char:
-		status = readb(uap->port.membase + UART01x_FR);
+		status = __raw_readl(uap->port.membase + UART01x_FR);
 	}
 	spin_unlock(&uap->port.lock);
 	tty_flip_buffer_push(&uap->port.state->port);
@@ -173,7 +171,7 @@ static void pl010_tx_chars(struct uart_a
 	int count;
 
 	if (uap->port.x_char) {
-		writel(uap->port.x_char, uap->port.membase + UART01x_DR);
+		__raw_writel(uap->port.x_char, uap->port.membase + UART01x_DR);
 		uap->port.icount.tx++;
 		uap->port.x_char = 0;
 		return;
@@ -185,7 +183,7 @@ static void pl010_tx_chars(struct uart_a
 
 	count = uap->port.fifosize >> 1;
 	do {
-		writel(xmit->buf[xmit->tail], uap->port.membase + UART01x_DR);
+		__raw_writel(xmit->buf[xmit->tail], uap->port.membase + UART01x_DR);
 		xmit->tail = (xmit->tail + 1) & (UART_XMIT_SIZE - 1);
 		uap->port.icount.tx++;
 		if (uart_circ_empty(xmit))
@@ -203,9 +201,9 @@ static void pl010_modem_status(struct ua
 {
 	unsigned int status, delta;
 
-	writel(0, uap->port.membase + UART010_ICR);
+	__raw_writel(0, uap->port.membase + UART010_ICR);
 
-	status = readb(uap->port.membase + UART01x_FR) & UART01x_FR_MODEM_ANY;
+	status = __raw_readl(uap->port.membase + UART01x_FR) & UART01x_FR_MODEM_ANY;
 
 	delta = status ^ uap->old_status;
 	uap->old_status = status;
@@ -233,7 +231,7 @@ static irqreturn_t pl010_int(int irq, vo
 
 	spin_lock(&uap->port.lock);
 
-	status = readb(uap->port.membase + UART010_IIR);
+	status = __raw_readl(uap->port.membase + UART010_IIR);
 	if (status) {
 		do {
 			if (status & (UART010_IIR_RTIS | UART010_IIR_RIS))
@@ -246,7 +244,7 @@ static irqreturn_t pl010_int(int irq, vo
 			if (pass_counter-- == 0)
 				break;
 
-			status = readb(uap->port.membase + UART010_IIR);
+			status = __raw_readl(uap->port.membase + UART010_IIR);
 		} while (status & (UART010_IIR_RTIS | UART010_IIR_RIS |
 				   UART010_IIR_TIS));
 		handled = 1;
@@ -260,7 +258,7 @@ static irqreturn_t pl010_int(int irq, vo
 static unsigned int pl010_tx_empty(struct uart_port *port)
 {
 	struct uart_amba_port *uap = (struct uart_amba_port *)port;
-	unsigned int status = readb(uap->port.membase + UART01x_FR);
+	unsigned int status = __raw_readl(uap->port.membase + UART01x_FR);
 	return status & UART01x_FR_BUSY ? 0 : TIOCSER_TEMT;
 }
 
@@ -270,7 +268,7 @@ static unsigned int pl010_get_mctrl(stru
 	unsigned int result = 0;
 	unsigned int status;
 
-	status = readb(uap->port.membase + UART01x_FR);
+	status = __raw_readl(uap->port.membase + UART01x_FR);
 	if (status & UART01x_FR_DCD)
 		result |= TIOCM_CAR;
 	if (status & UART01x_FR_DSR)
@@ -296,12 +294,12 @@ static void pl010_break_ctl(struct uart_
 	unsigned int lcr_h;
 
 	spin_lock_irqsave(&uap->port.lock, flags);
-	lcr_h = readb(uap->port.membase + UART010_LCRH);
+	lcr_h = __raw_readl(uap->port.membase + UART010_LCRH);
 	if (break_state == -1)
 		lcr_h |= UART01x_LCRH_BRK;
 	else
 		lcr_h &= ~UART01x_LCRH_BRK;
-	writel(lcr_h, uap->port.membase + UART010_LCRH);
+	__raw_writel(lcr_h, uap->port.membase + UART010_LCRH);
 	spin_unlock_irqrestore(&uap->port.lock, flags);
 }
 
@@ -329,12 +327,12 @@ static int pl010_startup(struct uart_por
 	/*
 	 * initialise the old status of the modem signals
 	 */
-	uap->old_status = readb(uap->port.membase + UART01x_FR) & UART01x_FR_MODEM_ANY;
+	uap->old_status = __raw_readl(uap->port.membase + UART01x_FR) & UART01x_FR_MODEM_ANY;
 
 	/*
 	 * Finally, enable interrupts
 	 */
-	writel(UART01x_CR_UARTEN | UART010_CR_RIE | UART010_CR_RTIE,
+	__raw_writel(UART01x_CR_UARTEN | UART010_CR_RIE | UART010_CR_RTIE,
 	       uap->port.membase + UART010_CR);
 
 	return 0;
@@ -357,10 +355,10 @@ static void pl010_shutdown(struct uart_p
 	/*
 	 * disable all interrupts, disable the port
 	 */
-	writel(0, uap->port.membase + UART010_CR);
+	__raw_writel(0, uap->port.membase + UART010_CR);
 
 	/* disable break condition and fifos */
-	writel(readb(uap->port.membase + UART010_LCRH) &
+	__raw_writel(__raw_readl(uap->port.membase + UART010_LCRH) &
 		~(UART01x_LCRH_BRK | UART01x_LCRH_FEN),
 	       uap->port.membase + UART010_LCRH);
 
@@ -382,7 +380,7 @@ pl010_set_termios(struct uart_port *port
 	/*
 	 * Ask the core to calculate the divisor for us.
 	 */
-	baud = uart_get_baud_rate(port, termios, old, 0, uap->port.uartclk/16); 
+	baud = uart_get_baud_rate(port, termios, old, 0, uap->port.uartclk/16);
 	quot = uart_get_divisor(port, baud);
 
 	switch (termios->c_cflag & CSIZE) {
@@ -445,25 +443,25 @@ pl010_set_termios(struct uart_port *port
 		uap->port.ignore_status_mask |= UART_DUMMY_RSR_RX;
 
 	/* first, disable everything */
-	old_cr = readb(uap->port.membase + UART010_CR) & ~UART010_CR_MSIE;
+	old_cr = __raw_readl(uap->port.membase + UART010_CR) & ~UART010_CR_MSIE;
 
 	if (UART_ENABLE_MS(port, termios->c_cflag))
 		old_cr |= UART010_CR_MSIE;
 
-	writel(0, uap->port.membase + UART010_CR);
+	__raw_writel(0, uap->port.membase + UART010_CR);
 
 	/* Set baud rate */
 	quot -= 1;
-	writel((quot & 0xf00) >> 8, uap->port.membase + UART010_LCRM);
-	writel(quot & 0xff, uap->port.membase + UART010_LCRL);
+	__raw_writel((quot & 0xf00) >> 8, uap->port.membase + UART010_LCRM);
+	__raw_writel(quot & 0xff, uap->port.membase + UART010_LCRL);
 
 	/*
 	 * ----------v----------v----------v----------v-----
 	 * NOTE: MUST BE WRITTEN AFTER UARTLCR_M & UARTLCR_L
 	 * ----------^----------^----------^----------^-----
 	 */
-	writel(lcr_h, uap->port.membase + UART010_LCRH);
-	writel(old_cr, uap->port.membase + UART010_CR);
+	__raw_writel(lcr_h, uap->port.membase + UART010_LCRH);
+	__raw_writel(old_cr, uap->port.membase + UART010_CR);
 
 	spin_unlock_irqrestore(&uap->port.lock, flags);
 }
@@ -545,7 +543,7 @@ static struct uart_ops amba_pl010_pops =
 	.verify_port	= pl010_verify_port,
 };
 
-static struct uart_amba_port *amba_ports[UART_NR];
+static struct uart_amba_port *amba_ports[SERIAL_AMBA_NR];
 
 #ifdef CONFIG_SERIAL_AMBA_PL010_CONSOLE
 
@@ -555,10 +553,10 @@ static void pl010_console_putchar(struct
 	unsigned int status;
 
 	do {
-		status = readb(uap->port.membase + UART01x_FR);
+		status = __raw_readl(uap->port.membase + UART01x_FR);
 		barrier();
 	} while (!UART_TX_READY(status));
-	writel(ch, uap->port.membase + UART01x_DR);
+	__raw_writel(ch, uap->port.membase + UART01x_DR);
 }
 
 static void
@@ -572,8 +570,8 @@ pl010_console_write(struct console *co,
 	/*
 	 *	First save the CR then disable the interrupts
 	 */
-	old_cr = readb(uap->port.membase + UART010_CR);
-	writel(UART01x_CR_UARTEN, uap->port.membase + UART010_CR);
+	old_cr = __raw_readl(uap->port.membase + UART010_CR);
+	__raw_writel(UART01x_CR_UARTEN, uap->port.membase + UART010_CR);
 
 	uart_console_write(&uap->port, s, count, pl010_console_putchar);
 
@@ -582,10 +580,10 @@ pl010_console_write(struct console *co,
 	 *	and restore the TCR
 	 */
 	do {
-		status = readb(uap->port.membase + UART01x_FR);
+		status = __raw_readl(uap->port.membase + UART01x_FR);
 		barrier();
 	} while (status & UART01x_FR_BUSY);
-	writel(old_cr, uap->port.membase + UART010_CR);
+	__raw_writel(old_cr, uap->port.membase + UART010_CR);
 
 	clk_disable(uap->clk);
 }
@@ -594,9 +592,9 @@ static void __init
 pl010_console_get_options(struct uart_amba_port *uap, int *baud,
 			     int *parity, int *bits)
 {
-	if (readb(uap->port.membase + UART010_CR) & UART01x_CR_UARTEN) {
+	if (__raw_readl(uap->port.membase + UART010_CR) & UART01x_CR_UARTEN) {
 		unsigned int lcr_h, quot;
-		lcr_h = readb(uap->port.membase + UART010_LCRH);
+		lcr_h = __raw_readl(uap->port.membase + UART010_LCRH);
 
 		*parity = 'n';
 		if (lcr_h & UART01x_LCRH_PEN) {
@@ -611,8 +609,8 @@ pl010_console_get_options(struct uart_am
 		else
 			*bits = 8;
 
-		quot = readb(uap->port.membase + UART010_LCRL) |
-		       readb(uap->port.membase + UART010_LCRM) << 8;
+		quot = __raw_readl(uap->port.membase + UART010_LCRL) |
+		       __raw_readl(uap->port.membase + UART010_LCRM) << 8;
 		*baud = uap->port.uartclk / (16 * (quot + 1));
 	}
 }
@@ -631,7 +629,7 @@ static int __init pl010_console_setup(st
 	 * if so, search for the first available port that does have
 	 * console support.
 	 */
-	if (co->index >= UART_NR)
+	if (co->index >= SERIAL_AMBA_NR)
 		co->index = 0;
 	uap = amba_ports[co->index];
 	if (!uap)
@@ -673,7 +671,7 @@ static struct uart_driver amba_reg = {
 	.dev_name		= "ttyAM",
 	.major			= SERIAL_AMBA_MAJOR,
 	.minor			= SERIAL_AMBA_MINOR,
-	.nr			= UART_NR,
+	.nr			= SERIAL_AMBA_NR,
 	.cons			= AMBA_CONSOLE,
 };
 
--- a/drivers/tty/serial/Kconfig
+++ b/drivers/tty/serial/Kconfig
@@ -25,10 +25,18 @@ config SERIAL_AMBA_PL010
 	help
 	  This selects the ARM(R) AMBA(R) PrimeCell PL010 UART.  If you have
 	  an Integrator/AP or Integrator/PP2 platform, or if you have a
-	  Cirrus Logic EP93xx CPU, say Y or M here.
+	  Cirrus Logic EP93xx CPU or an Infineon ADM5120 SOC, say Y or M here.
 
 	  If unsure, say N.
 
+config SERIAL_AMBA_PL010_NUMPORTS
+	int "Maximum number of AMBA PL010 serial ports"
+	depends on SERIAL_AMBA_PL010
+	default "8"
+	---help---
+	  Set this to the number of serial ports you want the AMBA PL010 driver
+	  to support.
+
 config SERIAL_AMBA_PL010_CONSOLE
 	bool "Support for console on AMBA serial port"
 	depends on SERIAL_AMBA_PL010=y
