From 138173d4e826587da66c7d321da1a91283222536 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Mon, 1 Dec 2014 07:58:18 +0100
Subject: [PATCH] MIPS: BCM47xx: Move NVRAM header to the include/linux/.
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

There are two reasons for having this header in the common place:
1) Simplifying drivers that read NVRAM entries. We will be able to
   safely call bcm47xx_nvram_* functions without #ifdef-s.
2) Getting NVRAM driver out of MIPS arch code. This is needed to support
   BCM5301X arch which also requires this NVRAM driver. Patch for that
   will follow once we get is reviewed.

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
Acked-by: Hauke Mehrtens <hauke@hauke-m.de>
Cc: linux-mips@linux-mips.org
Cc: Arnd Bergmann <arnd@arndb.de>
Cc: Paul Walmsley <paul@pwsan.com>
Cc: linux-soc@vger.kernel.org
Patchwork: https://patchwork.linux-mips.org/patch/8619/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
---
 arch/mips/bcm47xx/board.c                          |  2 +-
 arch/mips/bcm47xx/nvram.c                          |  2 +-
 arch/mips/bcm47xx/setup.c                          |  1 -
 arch/mips/bcm47xx/sprom.c                          |  1 -
 arch/mips/bcm47xx/time.c                           |  1 -
 arch/mips/include/asm/mach-bcm47xx/bcm47xx.h       |  1 +
 arch/mips/include/asm/mach-bcm47xx/bcm47xx_nvram.h | 21 -------------
 drivers/bcma/driver_mips.c                         |  2 +-
 drivers/net/ethernet/broadcom/b44.c                |  2 +-
 drivers/net/ethernet/broadcom/bgmac.c              |  2 +-
 drivers/ssb/driver_chipcommon_pmu.c                |  2 +-
 drivers/ssb/driver_mipscore.c                      |  2 +-
 include/linux/bcm47xx_nvram.h                      | 34 ++++++++++++++++++++++
 13 files changed, 42 insertions(+), 31 deletions(-)
 delete mode 100644 arch/mips/include/asm/mach-bcm47xx/bcm47xx_nvram.h
 create mode 100644 include/linux/bcm47xx_nvram.h

diff --git a/arch/mips/bcm47xx/board.c b/arch/mips/bcm47xx/board.c
index b3ae068..6e85130 100644
--- a/arch/mips/bcm47xx/board.c
+++ b/arch/mips/bcm47xx/board.c
@@ -1,8 +1,8 @@
 #include <linux/errno.h>
 #include <linux/export.h>
 #include <linux/string.h>
+#include <bcm47xx.h>
 #include <bcm47xx_board.h>
-#include <bcm47xx_nvram.h>
 
 struct bcm47xx_board_type {
 	const enum bcm47xx_board board;
diff --git a/arch/mips/bcm47xx/nvram.c b/arch/mips/bcm47xx/nvram.c
index d805d8a..7c77a88 100644
--- a/arch/mips/bcm47xx/nvram.c
+++ b/arch/mips/bcm47xx/nvram.c
@@ -16,7 +16,7 @@
 #include <linux/kernel.h>
 #include <linux/string.h>
 #include <linux/mtd/mtd.h>
-#include <bcm47xx_nvram.h>
+#include <linux/bcm47xx_nvram.h>
 
 #define NVRAM_MAGIC		0x48534C46	/* 'FLSH' */
 #define NVRAM_SPACE		0x8000
diff --git a/arch/mips/bcm47xx/setup.c b/arch/mips/bcm47xx/setup.c
index e43b504..b26c9c2 100644
--- a/arch/mips/bcm47xx/setup.c
+++ b/arch/mips/bcm47xx/setup.c
@@ -42,7 +42,6 @@
 #include <asm/reboot.h>
 #include <asm/time.h>
 #include <bcm47xx.h>
-#include <bcm47xx_nvram.h>
 #include <bcm47xx_board.h>
 
 union bcm47xx_bus bcm47xx_bus;
diff --git a/arch/mips/bcm47xx/sprom.c b/arch/mips/bcm47xx/sprom.c
index eff9205..c114b02 100644
--- a/arch/mips/bcm47xx/sprom.c
+++ b/arch/mips/bcm47xx/sprom.c
@@ -27,7 +27,6 @@
  */
 
 #include <bcm47xx.h>
-#include <bcm47xx_nvram.h>
 #include <linux/if_ether.h>
 #include <linux/etherdevice.h>
 
diff --git a/arch/mips/bcm47xx/time.c b/arch/mips/bcm47xx/time.c
index 2c85d92..5b46510 100644
--- a/arch/mips/bcm47xx/time.c
+++ b/arch/mips/bcm47xx/time.c
@@ -27,7 +27,6 @@
 #include <linux/ssb/ssb.h>
 #include <asm/time.h>
 #include <bcm47xx.h>
-#include <bcm47xx_nvram.h>
 #include <bcm47xx_board.h>
 
 void __init plat_time_init(void)
diff --git a/arch/mips/include/asm/mach-bcm47xx/bcm47xx.h b/arch/mips/include/asm/mach-bcm47xx/bcm47xx.h
index 7527c1d..8ed77f6 100644
--- a/arch/mips/include/asm/mach-bcm47xx/bcm47xx.h
+++ b/arch/mips/include/asm/mach-bcm47xx/bcm47xx.h
@@ -22,6 +22,7 @@
 #include <linux/ssb/ssb.h>
 #include <linux/bcma/bcma.h>
 #include <linux/bcma/bcma_soc.h>
+#include <linux/bcm47xx_nvram.h>
 
 enum bcm47xx_bus_type {
 #ifdef CONFIG_BCM47XX_SSB
--- a/arch/mips/include/asm/mach-bcm47xx/bcm47xx_nvram.h
+++ b/arch/mips/include/asm/mach-bcm47xx/bcm47xx_nvram.h
@@ -1,21 +1 @@
-/*
- *  Copyright (C) 2005, Broadcom Corporation
- *  Copyright (C) 2006, Felix Fietkau <nbd@openwrt.org>
- *
- *  This program is free software; you can redistribute  it and/or modify it
- *  under  the terms of  the GNU General  Public License as published by the
- *  Free Software Foundation;  either version 2 of the  License, or (at your
- *  option) any later version.
- */
-
-#ifndef __BCM47XX_NVRAM_H
-#define __BCM47XX_NVRAM_H
-
-#include <linux/types.h>
-#include <linux/kernel.h>
-
-int bcm47xx_nvram_init_from_mem(u32 base, u32 lim);
-int bcm47xx_nvram_getenv(const char *name, char *val, size_t val_len);
-int bcm47xx_nvram_gpio_pin(const char *name);
-
-#endif /* __BCM47XX_NVRAM_H */
+#include <linux/bcm47xx_nvram.h>
diff --git a/drivers/bcma/driver_mips.c b/drivers/bcma/driver_mips.c
index 04faf6d..24424f3 100644
--- a/drivers/bcma/driver_mips.c
+++ b/drivers/bcma/driver_mips.c
@@ -21,7 +21,7 @@
 #include <linux/serial_reg.h>
 #include <linux/time.h>
 #ifdef CONFIG_BCM47XX
-#include <bcm47xx_nvram.h>
+#include <linux/bcm47xx_nvram.h>
 #endif
 
 enum bcma_boot_dev {
diff --git a/drivers/net/ethernet/broadcom/b44.c b/drivers/net/ethernet/broadcom/b44.c
index bd5916a..77363d6 100644
--- a/drivers/net/ethernet/broadcom/b44.c
+++ b/drivers/net/ethernet/broadcom/b44.c
@@ -400,7 +400,7 @@ static void b44_set_flow_ctrl(struct b44 *bp, u32 local, u32 remote)
 }
 
 #ifdef CONFIG_BCM47XX
-#include <bcm47xx_nvram.h>
+#include <linux/bcm47xx_nvram.h>
 static void b44_wap54g10_workaround(struct b44 *bp)
 {
 	char buf[20];
diff --git a/drivers/net/ethernet/broadcom/bgmac.c b/drivers/net/ethernet/broadcom/bgmac.c
index 0469f72..be059df 100644
--- a/drivers/net/ethernet/broadcom/bgmac.c
+++ b/drivers/net/ethernet/broadcom/bgmac.c
@@ -18,7 +18,7 @@
 #include <linux/interrupt.h>
 #include <linux/dma-mapping.h>
 #include <linux/platform_data/b53.h>
-#include <bcm47xx_nvram.h>
+#include <linux/bcm47xx_nvram.h>
 
 static const struct bcma_device_id bgmac_bcma_tbl[] = {
 	BCMA_CORE(BCMA_MANUF_BCM, BCMA_CORE_4706_MAC_GBIT, BCMA_ANY_REV, BCMA_ANY_CLASS),
diff --git a/drivers/ssb/driver_chipcommon_pmu.c b/drivers/ssb/driver_chipcommon_pmu.c
index 1173a09..0942841 100644
--- a/drivers/ssb/driver_chipcommon_pmu.c
+++ b/drivers/ssb/driver_chipcommon_pmu.c
@@ -14,7 +14,7 @@
 #include <linux/delay.h>
 #include <linux/export.h>
 #ifdef CONFIG_BCM47XX
-#include <bcm47xx_nvram.h>
+#include <linux/bcm47xx_nvram.h>
 #endif
 
 #include "ssb_private.h"
diff --git a/drivers/ssb/driver_mipscore.c b/drivers/ssb/driver_mipscore.c
index 7b986f9..f87efef 100644
--- a/drivers/ssb/driver_mipscore.c
+++ b/drivers/ssb/driver_mipscore.c
@@ -16,7 +16,7 @@
 #include <linux/serial_reg.h>
 #include <linux/time.h>
 #ifdef CONFIG_BCM47XX
-#include <bcm47xx_nvram.h>
+#include <linux/bcm47xx_nvram.h>
 #endif
 
 #include "ssb_private.h"
diff --git a/include/linux/bcm47xx_nvram.h b/include/linux/bcm47xx_nvram.h
new file mode 100644
index 0000000..b12b07e
--- /dev/null
+++ b/include/linux/bcm47xx_nvram.h
@@ -0,0 +1,34 @@
+/*
+ *  This program is free software; you can redistribute  it and/or modify it
+ *  under  the terms of  the GNU General  Public License as published by the
+ *  Free Software Foundation;  either version 2 of the  License, or (at your
+ *  option) any later version.
+ */
+
+#ifndef __BCM47XX_NVRAM_H
+#define __BCM47XX_NVRAM_H
+
+#include <linux/types.h>
+#include <linux/kernel.h>
+
+#ifdef CONFIG_BCM47XX
+int bcm47xx_nvram_init_from_mem(u32 base, u32 lim);
+int bcm47xx_nvram_getenv(const char *name, char *val, size_t val_len);
+int bcm47xx_nvram_gpio_pin(const char *name);
+#else
+static inline int bcm47xx_nvram_init_from_mem(u32 base, u32 lim)
+{
+	return -ENOTSUPP;
+};
+static inline int bcm47xx_nvram_getenv(const char *name, char *val,
+				       size_t val_len)
+{
+	return -ENOTSUPP;
+};
+static inline int bcm47xx_nvram_gpio_pin(const char *name)
+{
+	return -ENOTSUPP;
+};
+#endif
+
+#endif /* __BCM47XX_NVRAM_H */
-- 
1.8.4.5

