From b9ba09038dab4d824176ea2c2f2b73f49b567217 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Sun, 16 Mar 2014 04:52:01 +0000
Subject: [PATCH 28/57] serial: ralink: the core has a size of 0x100 and not
 0x1000

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 drivers/tty/serial/8250/8250_core.c |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/tty/serial/8250/8250_core.c
+++ b/drivers/tty/serial/8250/8250_core.c
@@ -2635,7 +2635,7 @@ serial8250_pm(struct uart_port *port, un
 static unsigned int serial8250_port_size(struct uart_8250_port *pt)
 {
 	if (pt->port.iotype == UPIO_AU)
-		return 0x1000;
+		return 0x100;
 	if (is_omap1_8250(pt))
 		return 0x16 << pt->port.regshift;
 
