// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qcom-ipq4019.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/soc/qcom,tcsr.h>
#include <dt-bindings/leds/common.h>

/ {
	aliases {
		ethernet0 = &gmac;
		led-boot = &led_blue;
		led-failsafe = &led_red;
		led-running = &led_blue;
		led-upgrade = &led_red;
		label-mac-device = &gmac;
	};

	soc {
		ess-tcsr@1953000 {
			compatible = "qcom,tcsr";
			reg = <0x1953000 0x1000>;
			qcom,ess-interface-select = <TCSR_ESS_PSGMII>;
		};


		tcsr@1949000 {
			compatible = "qcom,tcsr";
			reg = <0x1949000 0x100>;
			qcom,wifi_glb_cfg = <TCSR_WIFI_GLB_CFG>;
		};

		tcsr@194b000 {
			compatible = "qcom,tcsr";
			reg = <0x194b000 0x100>;
			qcom,usb-hsphy-mode-select = <TCSR_USB_HSPHY_HOST_MODE>;
		};

		tcsr@1957000 {
			compatible = "qcom,tcsr";
			reg = <0x1957000 0x100>;
			qcom,wifi_noc_memtype_m0_m2 = <TCSR_WIFI_NOC_MEMTYPE_M0_M2>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&tlmm 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};
};

&tlmm {
	mdio_pins: mdio-pinmux {
		mux-1 {
			pins = "gpio6";
			function = "mdio";
			bias-pull-up;
		};

		mux-2 {
			pins = "gpio7";
			function = "mdc";
			bias-pull-up;
		};
	};

	serial_0_pins: serial0-pinmux {
		pins = "gpio16", "gpio17";
		function = "blsp_uart0";
		bias-disable;
	};

	serial_1_pins: serial1-pinmux {
		pins = "gpio8", "gpio9", "gpio10", "gpio11";
		function = "blsp_uart1";
		bias-disable;
	};

	spi_1_pins: spi-1-pinmux {
		mux-1 {
			pins = "gpio44", "gpio46", "gpio47";
			function = "blsp_spi1";
			bias-disable;
		};

		mux-2 {
			pins = "gpio45", "gpio49";
			function = "gpio";
			bias-pull-up;
			output-high;
		};

		host-interrupt {
			pins = "gpio42";
			function = "gpio";
			input;
		};
	};

	wifi_0_pins: wifi0-pinmux {
		pins = "gpio52";
		function = "gpio";
		drive-strength = <6>;
		bias-pull-up;
		output-high;
	};

	zigbee-0 {
		gpio-hog;
		gpios = <29 GPIO_ACTIVE_HIGH>;
		bias-disable;
		output-low;
	};

	zigbee-1 {
		gpio-hog;
		gpios = <50 GPIO_ACTIVE_HIGH>;
		bias-disable;
		input;
	};

	bluetooth-enable {
		gpio-hog;
		gpios = <32 GPIO_ACTIVE_HIGH>;
		output-high;
	};
};

&ethphy0 {
	status = "disabled";
};

&ethphy1 {
	status = "disabled";
};

&ethphy2 {
	status = "disabled";
};

&watchdog {
	status = "okay";
};

&prng {
	status = "okay";
};

&blsp_dma {
	status = "okay";
};

&cryptobam {
	status = "okay";
	num-channels = <4>;
	qcom,num-ees = <2>;
};

&crypto {
	status = "okay";
};

&blsp1_uart1 {
	status = "okay";
	pinctrl-0 = <&serial_0_pins>;
	pinctrl-names = "default";
};

&blsp1_uart2 {
	status = "okay";
	pinctrl-0 = <&serial_1_pins>;
	pinctrl-names = "default";

	bluetooth {
		compatible = "csr,8811";

		enable-gpios = <&tlmm 32 GPIO_ACTIVE_HIGH>;
	};
};

&blsp1_spi2 {
	status = "okay";
	pinctrl-0 = <&spi_1_pins>;
	pinctrl-names = "default";

	cs-gpios = <&tlmm 45 GPIO_ACTIVE_HIGH>;

	zigbee@0 {
		compatible = "silabs,em3581";
		reg = <0>;
		#address-cells = <1>;
		#size-cells = <0>;
		spi-max-frequency = <12000000>;
	};
};

&blsp1_i2c3 {
	status = "okay";
	pinctrl-0 = <&i2c_0_pins>;
	pinctrl-names = "default";

	// RGB LEDs
	pca9633: led-controller@62 {
		compatible = "nxp,pca9633";
		nxp,hw-blink;
		reg = <0x62>;
		#address-cells = <1>;
		#size-cells = <0>;

		led_red: red@0 {
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_INDICATOR;
			reg = <0>;
		};

		led_green: green@1 {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_INDICATOR;
			reg = <1>;
		};

		led_blue: blue@2 {
			color = <LED_COLOR_ID_BLUE>;
			function = LED_FUNCTION_INDICATOR;
			reg = <2>;
		};
	};
};

&pcie0 {
	status = "okay";

	perst-gpios = <&tlmm 38 GPIO_ACTIVE_LOW>;
	wake-gpios = <&tlmm 40 GPIO_ACTIVE_LOW>;
	clkreq-gpios = <&tlmm 39 GPIO_ACTIVE_LOW>;

	bridge@0,0 {
		reg = <0x00000000 0 0 0 0>;
		#address-cells = <3>;
		#size-cells = <2>;
		ranges;

		wifi2: wifi@1,0 {
			compatible = "qcom,ath10k";
		};
	};
};

&gmac {
	status = "okay";
};

&switch {
	status = "okay";
};

&swport4 {
	status = "okay";
	label = "lan";
};

&swport5 {
	status = "okay";
	label = "wan";
};

&wifi0 {
	status = "okay";
	pinctrl-0 = <&wifi_0_pins>;
	pinctrl-names = "default";

	qcom,coexist-support = <1>;
	qcom,coexist-gpio-pin = <52>;
};

&wifi1 {
	status = "okay";

	ieee80211-freq-limit = <5170000 5330000>;
};

&wifi2 {
	status = "okay";

	ieee80211-freq-limit = <5490000 5835000>;
};
