From 6c70bb5fc9fbb53d7496ddc3d62833c68692970e Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Tue, 23 May 2023 14:11:52 +0100
Subject: [PATCH 0469/1085] i2c-bcm2835: Flush FIFOs cleanly on error

On error condition, note the error return code, but still
handle the FIFOs in the normal way rather than relying on
C_CLEAR flushing everything cleanly.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/i2c/busses/i2c-bcm2835.c | 7 ++-----
 1 file changed, 2 insertions(+), 5 deletions(-)

--- a/drivers/i2c/busses/i2c-bcm2835.c
+++ b/drivers/i2c/busses/i2c-bcm2835.c
@@ -385,10 +385,8 @@ static irqreturn_t bcm2835_i2c_isr(int t
 	bcm2835_debug_add(i2c_dev, val);
 
 	err = val & (BCM2835_I2C_S_CLKT | BCM2835_I2C_S_ERR);
-	if (err) {
+	if (err)
 		i2c_dev->msg_err = err;
-		goto complete;
-	}
 
 	if (val & BCM2835_I2C_S_DONE) {
 		if (!i2c_dev->curr_msg) {
@@ -400,8 +398,6 @@ static irqreturn_t bcm2835_i2c_isr(int t
 
 		if ((val & BCM2835_I2C_S_RXD) || i2c_dev->msg_buf_remaining)
 			i2c_dev->msg_err = BCM2835_I2C_S_LEN;
-		else
-			i2c_dev->msg_err = 0;
 		goto complete;
 	}
 
@@ -465,6 +461,7 @@ static int bcm2835_i2c_xfer(struct i2c_a
 
 	i2c_dev->curr_msg = msgs;
 	i2c_dev->num_msgs = num;
+	i2c_dev->msg_err = 0;
 	reinit_completion(&i2c_dev->completion);
 
 	bcm2835_i2c_start_transfer(i2c_dev);
