/* SPDX-License-Identifier: GPL-2.0-or-later OR MIT
 *
 * Copyright (c) 2018 Peng Zhang <sd20@qxwlan.com>
 *
 */

#include "qcom-ipq4019.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/soc/qcom,tcsr.h>

/ {

	model = "Qxwlan E2600AC";
	compatible = "qcom,ipq4019";

	memory {
		device_type = "memory";
		reg = <0x80000000 0x10000000>; /* 256MB */
	};

	soc {
		tcsr@1949000 {
			compatible = "qcom,tcsr";
			reg = <0x1949000 0x100>;
			qcom,wifi_glb_cfg = <TCSR_WIFI_GLB_CFG>;
		};

		tcsr@194b000 {
			/* select hostmode */
			compatible = "qcom,tcsr";
			reg = <0x194b000 0x100>;
			qcom,usb-hsphy-mode-select = <TCSR_USB_HSPHY_HOST_MODE>;
			status = "okay";
		};

		ess_tcsr@1953000 {
			compatible = "qcom,tcsr";
			reg = <0x1953000 0x1000>;
			qcom,ess-interface-select = <TCSR_ESS_PSGMII>;
		};

		tcsr@1957000 {
			compatible = "qcom,tcsr";
			reg = <0x1957000 0x100>;
			qcom,wifi_noc_memtype_m0_m2 = <TCSR_WIFI_NOC_MEMTYPE_M0_M2>;
		};

		leds {
			compatible = "gpio-leds";

			led1 {
				label = "green:wlan0";
				gpios = <&tlmm 50 GPIO_ACTIVE_LOW>;
			};

			led2 {
				label = "green:wlan1";
				gpios = <&tlmm 36 GPIO_ACTIVE_LOW>;
			};

			led3 {
				function = LED_FUNCTION_USB;
				color = <LED_COLOR_ID_GREEN>;
				gpios = <&tlmm 32 GPIO_ACTIVE_LOW>;
				trigger-sources = <&usb2_port1>, <&usb3_port1>, <&usb3_port2>;
				linux,default-trigger = "usbport";
			};

			led4 {
				label = "green:ctrl1";
				gpios = <&tlmm 51 GPIO_ACTIVE_LOW>;
			};

			led5 {
				label = "green:ctrl2";
				gpios = <&tlmm 30 GPIO_ACTIVE_LOW>;
			};

			led6 {
				label = "green:ctrl3";
				gpios = <&tlmm 31 GPIO_ACTIVE_LOW>;
			};
		};

		keys {
			compatible = "gpio-keys";

			reset {
				label = "reset";
				gpios = <&tlmm 18 GPIO_ACTIVE_LOW>;
				linux,code = <KEY_RESTART>;
			};
		};
	};
};

&watchdog {
	status = "okay";
};

&prng {
	status = "okay";
};

&blsp_dma {
	status = "okay";
};

&crypto {
	status = "okay";
};

&cryptobam {
	status = "okay";
};

&tlmm {
	i2c_0_pins: i2c-0-pinmux {
		mux {
			pins = "gpio20", "gpio21";
			function = "blsp_i2c0";
			bias-disable;
		};
	};

	mdio_pins: mdio_pinmux {
		mux_1 {
			pins = "gpio6";
			function = "mdio";
			bias-pull-up;
		};
		mux_2 {
			pins = "gpio7";
			function = "mdc";
			bias-pull-up;
		};
	};

	serial_0_pins: serial0-pinmux {
		mux {
			pins = "gpio16", "gpio17";
			function = "blsp_uart0";
			bias-disable;
		};
	};

	serial_1_pins: serial1_pinmux {
		mux {
			pins = "gpio8", "gpio9";
			function = "blsp_uart1";
			bias-disable;
		};
	};

	spi_0_pins: spi_0_pinmux {
		pinmux {
			function = "blsp_spi0";
			pins = "gpio13", "gpio14", "gpio15";
			drive-strength = <12>;
			bias-disable;
		};
		pinmux_cs {
			function = "gpio";
			pins = "gpio12";
			drive-strength = <2>;
			bias-disable;
			output-high;
		};
	};
};

&blsp1_uart1 {
	pinctrl-0 = <&serial_0_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&blsp1_uart2 {
	pinctrl-0 = <&serial_1_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&blsp1_i2c3 { /* BLSP1 QUP2 */
	pinctrl-0 = <&i2c_0_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&usb3 {
	status = "okay";
};

&usb3_dwc {
	#address-cells = <1>;
	#size-cells = <0>;

	usb3_port1: port@1 {
		reg = <1>;
		#trigger-source-cells = <0>;
	};

	usb3_port2: port@2 {
		reg = <2>;
		#trigger-source-cells = <0>;
	};
};

&usb3_ss_phy {
	status = "okay";
};

&usb3_hs_phy {
	status = "okay";
};

&usb2 {
	status = "okay";

	usb@6000000 {
		#address-cells = <1>;
		#size-cells = <0>;

		usb2_port1: port@1 {
			reg = <1>;
			#trigger-source-cells = <0>;
		};
	};
};

&usb2_hs_phy {
	status = "okay";
};

&mdio {
	status = "okay";
	pinctrl-0 = <&mdio_pins>;
	pinctrl-names = "default";
};
