From 21d67c2fabfe40baf33202d3287b67b6c16f8382 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ar=C4=B1n=C3=A7=20=C3=9CNAL?= <arinc.unal@arinc9.com>
Date: Mon, 22 Apr 2024 10:15:19 +0300
Subject: [PATCH 12/15] net: dsa: mt7530: get rid of mac_port_validate member
 of mt753x_info
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

The mac_port_validate member of the mt753x_info structure is not being
used, remove it. Improve the member description section in the process.

Signed-off-by: Arınç ÜNAL <arinc.unal@arinc9.com>
---
 drivers/net/dsa/mt7530.h | 10 +++-------
 1 file changed, 3 insertions(+), 7 deletions(-)

--- a/drivers/net/dsa/mt7530.h
+++ b/drivers/net/dsa/mt7530.h
@@ -743,15 +743,14 @@ struct mt753x_pcs {
 
 /* struct mt753x_info -	This is the main data structure for holding the specific
  *			part for each supported device
+ * @id:			Holding the identifier to a switch model
+ * @pcs_ops:		Holding the pointer to the MAC PCS operations structure
  * @sw_setup:		Holding the handler to a device initialization
  * @phy_read_c22:	Holding the way reading PHY port using C22
  * @phy_write_c22:	Holding the way writing PHY port using C22
  * @phy_read_c45:	Holding the way reading PHY port using C45
  * @phy_write_c45:	Holding the way writing PHY port using C45
- * @phy_mode_supported:	Check if the PHY type is being supported on a certain
- *			port
- * @mac_port_validate:	Holding the way to set addition validate type for a
- *			certan MAC port
+ * @mac_port_get_caps:	Holding the handler that provides MAC capabilities
  * @mac_port_config:	Holding the way setting up the PHY attribute to a
  *			certain MAC port
  */
@@ -770,9 +769,6 @@ struct mt753x_info {
 			     int regnum, u16 val);
 	void (*mac_port_get_caps)(struct dsa_switch *ds, int port,
 				  struct phylink_config *config);
-	void (*mac_port_validate)(struct dsa_switch *ds, int port,
-				  phy_interface_t interface,
-				  unsigned long *supported);
 	void (*mac_port_config)(struct dsa_switch *ds, int port,
 				unsigned int mode,
 				phy_interface_t interface);
