From 7388400b8bd42f71d040dbf2fdbdcb834fcc0ede Mon Sep 17 00:00:00 2001
From: Gokul Sriram Palanisamy <gokulsri@codeaurora.org>
Date: Sat, 30 Jan 2021 10:50:13 +0530
Subject: [PATCH] arm64: dts: qcom: Enable Q6v5 WCSS for ipq8074 SoC

Enable remoteproc WCSS PIL driver with glink and ssr subdevices.
Also enables smp2p and mailboxes required for IPC.

Signed-off-by: Gokul Sriram Palanisamy <gokulsri@codeaurora.org>
Signed-off-by: Sricharan R <sricharan@codeaurora.org>
Signed-off-by: Nikhil Prakash V <nprakash@codeaurora.org>
Signed-off-by: Robert Marko <robimarko@gmail.com>
---
 arch/arm64/boot/dts/qcom/ipq8074.dtsi | 81 +++++++++++++++++++++++++++
 1 file changed, 81 insertions(+)

--- a/arch/arm64/boot/dts/qcom/ipq8074.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq8074.dtsi
@@ -142,6 +142,32 @@
 		};
 	};
 
+	wcss: smp2p-wcss {
+		compatible = "qcom,smp2p";
+		qcom,smem = <435>, <428>;
+
+		interrupt-parent = <&intc>;
+		interrupts = <0 322 1>;
+
+		mboxes = <&apcs_glb 9>;
+
+		qcom,local-pid = <0>;
+		qcom,remote-pid = <1>;
+
+		wcss_smp2p_out: master-kernel {
+			qcom,entry-name = "master-kernel";
+			qcom,smp2p-feature-ssr-ack;
+			#qcom,smem-state-cells = <1>;
+		};
+
+		wcss_smp2p_in: slave-kernel {
+			qcom,entry-name = "slave-kernel";
+
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+	};
+
 	soc: soc@0 {
 		#address-cells = <1>;
 		#size-cells = <1>;
@@ -425,6 +451,11 @@
 			reg = <0x01937000 0x21000>;
 		};
 
+		tcsr_q6: syscon@1945000 {
+			compatible = "syscon";
+			reg = <0x01945000 0xe000>;
+		};
+
 		spmi_bus: spmi@200f000 {
 			compatible = "qcom,spmi-pmic-arb";
 			reg = <0x0200f000 0x001000>,
@@ -972,6 +1003,56 @@
 				      "axi_s_sticky";
 			status = "disabled";
 		};
+
+		q6v5_wcss: q6v5_wcss@cd00000 {
+			compatible = "qcom,ipq8074-wcss-pil";
+			reg = <0x0cd00000 0x4040>,
+			      <0x004ab000 0x20>;
+			reg-names = "qdsp6",
+				    "rmb";
+			qca,auto-restart;
+			qca,extended-intc;
+			interrupts-extended = <&intc 0 325 1>,
+					      <&wcss_smp2p_in 0 0>,
+					      <&wcss_smp2p_in 1 0>,
+					      <&wcss_smp2p_in 2 0>,
+					      <&wcss_smp2p_in 3 0>;
+			interrupt-names = "wdog",
+					  "fatal",
+					  "ready",
+					  "handover",
+					  "stop-ack";
+
+			resets = <&gcc GCC_WCSSAON_RESET>,
+				 <&gcc GCC_WCSS_BCR>,
+				 <&gcc GCC_WCSS_Q6_BCR>;
+
+			reset-names = "wcss_aon_reset",
+				      "wcss_reset",
+				      "wcss_q6_reset";
+
+			clocks = <&gcc GCC_PRNG_AHB_CLK>;
+			clock-names = "prng";
+
+			qcom,halt-regs = <&tcsr_q6 0xa000 0xd000 0x0>;
+
+			qcom,smem-states = <&wcss_smp2p_out 0>,
+					   <&wcss_smp2p_out 1>;
+			qcom,smem-state-names = "shutdown",
+						"stop";
+
+			memory-region = <&q6_region>;
+
+			glink-edge {
+				interrupts = <GIC_SPI 321 IRQ_TYPE_EDGE_RISING>;
+				qcom,remote-pid = <1>;
+				mboxes = <&apcs_glb 8>;
+
+				rpm_requests {
+					qcom,glink-channels = "IPCRTR";
+				};
+			};
+		};
 	};
 
 	timer {
