From 7029b92f5fdba739ad2698dc9546e7be03002c51 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Mon, 6 Mar 2017 09:06:18 +0000
Subject: [PATCH 0046/1085] clk-bcm2835: Read max core clock from firmware

The VPU is responsible for managing the core clock, usually under
direction from the bcm2835-cpufreq driver but not via the clk-bcm2835
driver. Since the core frequency can change without warning, it is
safer to report the maximum clock rate to users of the core clock -
I2C, SPI and the mini UART - to err on the safe side when calculating
clock divisors.

If the DT node for the clock driver includes a reference to the
firmware node, use the firmware API to query the maximum core clock
instead of reading the divider registers.

Prior to this patch, a "100KHz" I2C bus was sometimes clocked at about
160KHz. In particular, switching to the 4.9 kernel was likely to break
SenseHAT usage on a Pi3.

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 drivers/clk/bcm/clk-bcm2835.c | 39 ++++++++++++++++++++++++++++++++++-
 1 file changed, 38 insertions(+), 1 deletion(-)

--- a/drivers/clk/bcm/clk-bcm2835.c
+++ b/drivers/clk/bcm/clk-bcm2835.c
@@ -36,6 +36,7 @@
 #include <linux/platform_device.h>
 #include <linux/slab.h>
 #include <dt-bindings/clock/bcm2835.h>
+#include <soc/bcm2835/raspberrypi-firmware.h>
 
 #define CM_PASSWORD		0x5a000000
 
@@ -296,6 +297,8 @@
 #define SOC_BCM2711		BIT(1)
 #define SOC_ALL			(SOC_BCM2835 | SOC_BCM2711)
 
+#define VCMSG_ID_CORE_CLOCK     4
+
 /*
  * Names of clocks used within the driver that need to be replaced
  * with an external parent's name.  This array is in the order that
@@ -314,6 +317,7 @@ static const char *const cprman_parent_n
 struct bcm2835_cprman {
 	struct device *dev;
 	void __iomem *regs;
+	struct rpi_firmware *fw;
 	spinlock_t regs_lock; /* spinlock for all clocks */
 	unsigned int soc;
 
@@ -1039,6 +1043,30 @@ static unsigned long bcm2835_clock_get_r
 	return rate;
 }
 
+static unsigned long bcm2835_clock_get_rate_vpu(struct clk_hw *hw,
+						unsigned long parent_rate)
+{
+	struct bcm2835_clock *clock = bcm2835_clock_from_hw(hw);
+	struct bcm2835_cprman *cprman = clock->cprman;
+
+	if (cprman->fw) {
+		struct {
+			u32 id;
+			u32 val;
+		} packet;
+
+		packet.id = VCMSG_ID_CORE_CLOCK;
+		packet.val = 0;
+
+		if (!rpi_firmware_property(cprman->fw,
+					   RPI_FIRMWARE_GET_MAX_CLOCK_RATE,
+					   &packet, sizeof(packet)))
+			return packet.val;
+	}
+
+	return bcm2835_clock_get_rate(hw, parent_rate);
+}
+
 static void bcm2835_clock_wait_busy(struct bcm2835_clock *clock)
 {
 	struct bcm2835_cprman *cprman = clock->cprman;
@@ -1327,7 +1355,7 @@ static int bcm2835_vpu_clock_is_on(struc
  */
 static const struct clk_ops bcm2835_vpu_clock_clk_ops = {
 	.is_prepared = bcm2835_vpu_clock_is_on,
-	.recalc_rate = bcm2835_clock_get_rate,
+	.recalc_rate = bcm2835_clock_get_rate_vpu,
 	.set_rate = bcm2835_clock_set_rate,
 	.determine_rate = bcm2835_clock_determine_rate,
 	.set_parent = bcm2835_clock_set_parent,
@@ -2303,6 +2331,7 @@ static int bcm2835_clk_probe(struct plat
 	const struct bcm2835_clk_desc *desc;
 	const size_t asize = ARRAY_SIZE(clk_desc_array);
 	const struct cprman_plat_data *pdata;
+	struct device_node *fw_node;
 	size_t i;
 	u32 clk_id;
 	int ret;
@@ -2323,6 +2352,14 @@ static int bcm2835_clk_probe(struct plat
 	if (IS_ERR(cprman->regs))
 		return PTR_ERR(cprman->regs);
 
+	fw_node = of_parse_phandle(dev->of_node, "firmware", 0);
+	if (fw_node) {
+		struct rpi_firmware *fw = rpi_firmware_get(NULL);
+		if (!fw)
+			return -EPROBE_DEFER;
+		cprman->fw = fw;
+	}
+
 	memset(bcm2835_clk_claimed, 0, sizeof(bcm2835_clk_claimed));
 	for (i = 0;
 	     !of_property_read_u32_index(pdev->dev.of_node, "claim-clocks",
