From e7166f2774aafefd29ff26ffbbb7f6d40ac8ea1c Mon Sep 17 00:00:00 2001
From: Nitheesh Sekar <quic_nsekar@quicinc.com>
Date: Mon, 4 Sep 2023 12:06:34 +0530
Subject: [PATCH] arm64: dts: qcom: ipq5018: Add USB related nodes

Add USB phy and controller nodes.

Co-developed-by: Amandeep Singh <quic_amansing@quicinc.com>
Signed-off-by: Amandeep Singh <quic_amansing@quicinc.com>
Signed-off-by: Nitheesh Sekar <quic_nsekar@quicinc.com>
Link: https://lore.kernel.org/r/20230904063635.24975-4-quic_nsekar@quicinc.com
Signed-off-by: Bjorn Andersson <andersson@kernel.org>
---
 arch/arm64/boot/dts/qcom/ipq5018.dtsi | 54 +++++++++++++++++++++++++++
 1 file changed, 54 insertions(+)

--- a/arch/arm64/boot/dts/qcom/ipq5018.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq5018.dtsi
@@ -94,6 +94,19 @@
 		#size-cells = <1>;
 		ranges = <0 0 0 0xffffffff>;
 
+		usbphy0: phy@5b000 {
+			compatible = "qcom,ipq5018-usb-hsphy";
+			reg = <0x0005b000 0x120>;
+
+			clocks = <&gcc GCC_USB0_PHY_CFG_AHB_CLK>;
+
+			resets = <&gcc GCC_QUSB2_0_PHY_BCR>;
+
+			#phy-cells = <0>;
+
+			status = "disabled";
+		};
+
 		tlmm: pinctrl@1000000 {
 			compatible = "qcom,ipq5018-tlmm";
 			reg = <0x01000000 0x300000>;
@@ -156,6 +169,47 @@
 			status = "disabled";
 		};
 
+		usb: usb@8af8800 {
+			compatible = "qcom,ipq5018-dwc3", "qcom,dwc3";
+			reg = <0x08af8800 0x400>;
+
+			interrupts = <GIC_SPI 62 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "hs_phy_irq";
+
+			clocks = <&gcc GCC_USB0_MASTER_CLK>,
+				 <&gcc GCC_SYS_NOC_USB0_AXI_CLK>,
+				 <&gcc GCC_USB0_SLEEP_CLK>,
+				 <&gcc GCC_USB0_MOCK_UTMI_CLK>;
+			clock-names = "core",
+				      "iface",
+				      "sleep",
+				      "mock_utmi";
+
+			resets = <&gcc GCC_USB0_BCR>;
+
+			qcom,select-utmi-as-pipe-clk;
+			#address-cells = <1>;
+			#size-cells = <1>;
+			ranges;
+
+			status = "disabled";
+
+			usb_dwc: usb@8a00000 {
+				compatible = "snps,dwc3";
+				reg = <0x08a00000 0xe000>;
+				clocks = <&gcc GCC_USB0_MOCK_UTMI_CLK>;
+				clock-names = "ref";
+				interrupts = <GIC_SPI 140 IRQ_TYPE_LEVEL_HIGH>;
+				phy-names = "usb2-phy";
+				phys = <&usbphy0>;
+				tx-fifo-resize;
+				snps,is-utmi-l1-suspend;
+				snps,hird-threshold = /bits/ 8 <0x0>;
+				snps,dis_u2_susphy_quirk;
+				snps,dis_u3_susphy_quirk;
+			};
+		};
+
 		intc: interrupt-controller@b000000 {
 			compatible = "qcom,msm-qgic2";
 			reg = <0x0b000000 0x1000>,  /* GICD */
