// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar9344.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/mtd/partitions/uimage.h>

/ {
	chosen {
		bootargs = "console=ttyS0,115200n8";
	};

	aliases {
		led-boot = &led_power_amber;
		led-failsafe = &led_power_amber;
		led-running = &led_power_green;
		led-upgrade = &led_power_amber;
		label-mac-device = &eth0;
	};

	keys {
		compatible = "gpio-keys";

		wps {
			label = "wps";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 21 GPIO_ACTIVE_LOW>;
		};

		rfkill {
			label = "rfkill";
			linux,code = <KEY_RFKILL>;
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};
	};

	leds: leds {
		compatible = "gpio-leds";

		pinctrl-names = "default";
		pinctrl-0 = <&enable_gpio_11>;

		led_power_green: power_green {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
		};

		led_power_amber: power_amber {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_AMBER>;
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};

		wlan2g_green {
			label = "green:wlan2g";
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		wlan5g_blue {
			label = "blue:wlan5g";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		wps_green {
			function = LED_FUNCTION_WPS;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};

		wps_amber {
			function = LED_FUNCTION_WPS;
			color = <LED_COLOR_ID_AMBER>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
		};
	};

	ubi-concat {
		compatible = "mtd-concat";
		devices = <&ubiconcat0 &ubiconcat1>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			ubi@0 {
				label = "ubi";
				reg = <0x0 0x7500000>;
			};
		};
	};
};

&pinmux {
	enable_gpio_11: pinmux_enable_gpio_11 {
		pinctrl-single,bits = <0x8 0x0 0xff000000>;
	};
};

&nand {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "u-boot";
			reg = <0x0 0x40000>;
			read-only;
		};

		partition@40000 {
			label = "u-boot-env";
			reg = <0x40000 0x40000>;
		};

		caldata: partition@80000 {
			label = "caldata";
			reg = <0x80000 0x40000>;
			read-only;

			nvmem-layout {
				compatible = "fixed-layout";
				#address-cells = <1>;
				#size-cells = <1>;

				macaddr_caldata_0: macaddr@0 {
					reg = <0x0 0x6>;
				};

				macaddr_caldata_c: macaddr@c {
					reg = <0xc 0x6>;
				};

				cal_art_1000: cal@1000 {
					reg = <0x1000 0x440>;
				};

				cal_art_5000: cal@5000 {
					reg = <0x5000 0x440>;
				};
			};
		};

		partition@c0000 {
			label = "pot";
			reg = <0xc0000 0x80000>;
		};

		partition@140000 {
			label = "language";
			reg = <0x140000 0x200000>;
		};

		partition@340000 {
			label = "config";
			reg = <0x340000 0x80000>;
		};

		partition@3c0000 {
			label = "traffic_meter";
			reg = <0x3c0000 0x300000>;
		};

		partition@6c0000 {
			label = "firmware";
			reg = <0x6c0000 0x1900000>;

			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			kernel@0 {
				label = "kernel";
				reg = <0x0 0x400000>;
			};

			ubiconcat0: partition@400000 {
				label = "ubiconcat0";
				reg = <0x400000 0x1500000>;
			};
		};

		partition@1fc0000 {
			label = "caldata_backup";
			reg = <0x1fc0000 0x40000>;
			read-only;
		};

		ubiconcat1: partition@2000000 {
			label = "ubiconcat1";
			reg = <0x2000000 0x6000000>;
		};
	};
};

&ref {
	clock-frequency = <40000000>;
};

&builtin_switch {
	resets = <&rst 8>, <&rst 12>;
	reset-names = "switch", "switch-analog";
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		reg = <0>;
		phy-mode = "rgmii";
		qca,mib-poll-interval = <500>;

		qca,ar8327-initvals = <
			0x04 0x07600000
			0x0c 0x01000000
			0x10 0xc1000000
			0x50 0xcc35cc35
			0x54 0xcb37cb37
			0x58 0x00000000
			0x5c 0x00f3cf00
			0x7c 0x0000007e
			0x94 0x0000007e
			>;
	};
};

&eth0 {
	status = "okay";

	/* default for ar934x, except for 1000M */
	pll-data = <0x06000000 0x00000101 0x00001616>;

	nvmem-cells = <&macaddr_caldata_0>;
	nvmem-cell-names = "mac-address";

	phy-mode = "rgmii";
	phy-handle = <&phy0>;
};

&gpio {
	lna0 {
		gpio-hog;
		line-name = "netgear:ext:lna0";
		gpios = <18 GPIO_ACTIVE_HIGH>;
		output-high;
	};

	lna1 {
		gpio-hog;
		line-name = "netgear:ext:lna1";
		gpios = <19 GPIO_ACTIVE_HIGH>;
		output-high;
	};
};

&wmac {
	status = "okay";

	nvmem-cells = <&macaddr_caldata_0>, <&cal_art_1000>;
	nvmem-cell-names = "mac-address", "calibration";
};

&pcie {
	status = "okay";

	ath9k: wifi@0,0 {
		compatible = "pci168c,0033";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&macaddr_caldata_c>, <&cal_art_5000>;
		nvmem-cell-names = "mac-address", "calibration";
		#gpio-cells = <2>;
		gpio-controller;
	};
};
