From 602be52637ecca0b247cf832c8a4ec345844d325 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.com>
Date: Tue, 7 Jan 2025 12:09:48 +0000
Subject: [PATCH] dts: bcm2712: PL011 UARTs are actually r1p5

The ARM PL011 UART instances in BCM2712 are r1p5 spec, which means they
have 32-entry FIFOs. The correct periphid value for this is 0x00341011.
Thanks to N Buchwitz for pointing this out.

Signed-off-by: Phil Elwell <phil@raspberrypi.com>
---
 arch/arm64/boot/dts/broadcom/bcm2712.dtsi | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

--- a/arch/arm64/boot/dts/broadcom/bcm2712.dtsi
+++ b/arch/arm64/boot/dts/broadcom/bcm2712.dtsi
@@ -190,7 +190,7 @@
 			clocks = <&clk_uart>,
 				 <&clk_vpu>;
 			clock-names = "uartclk", "apb_pclk";
-			arm,primecell-periphid = <0x00241011>;
+			arm,primecell-periphid = <0x00341011>;
 			status = "disabled";
 		};
 
@@ -201,7 +201,7 @@
 			clocks = <&clk_uart>,
 				 <&clk_vpu>;
 			clock-names = "uartclk", "apb_pclk";
-			arm,primecell-periphid = <0x00241011>;
+			arm,primecell-periphid = <0x00341011>;
 			status = "disabled";
 		};
 
@@ -212,7 +212,7 @@
 			clocks = <&clk_uart>,
 				 <&clk_vpu>;
 			clock-names = "uartclk", "apb_pclk";
-			arm,primecell-periphid = <0x00241011>;
+			arm,primecell-periphid = <0x00341011>;
 			status = "disabled";
 		};
 
