// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/*
 * Copyright (c) 2020 Rockchip Electronics Co., Ltd.
 *
 * Copyright (c) 2024 FriendlyElec Computer Tech. Co., Ltd.
 * (http://www.friendlyarm.com)
 *
 * Copyright (c) 2024 Tianling Shen <cnsztl@gmail.com>
 */

/dts-v1/;
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/pinctrl/rockchip.h>
#include <dt-bindings/soc/rockchip,vop2.h>
#include "rk3566.dtsi"

/ {
	model = "FriendlyARM NanoPi R3S";
	compatible = "friendlyarm,nanopi-r3s", "rockchip,rk3566";

	aliases {
		ethernet0 = &gmac1;
		mmc0 = &sdmmc0;
		mmc1 = &sdhci;

		led-boot = &power_led;
		led-failsafe = &power_led;
		led-running = &power_led;
		led-upgrade = &power_led;
	};

	chosen: chosen {
		stdout-path = "serial2:1500000n8";
	};

	gpio-keys {
		compatible = "gpio-keys";
		pinctrl-names = "default";
		pinctrl-0 = <&reset_button_pin>;

		button-reset {
			label = "reset";
			gpios = <&gpio0 RK_PC2 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <50>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 = <&power_led_pin>, <&lan_led_pin>, <&wan_led_pin>;

		power_led: led-0 {
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_POWER;
			gpios = <&gpio0 RK_PB7 GPIO_ACTIVE_HIGH>;
		};

		lan_led: led-1 {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_LAN;
			gpios = <&gpio3 RK_PC2 GPIO_ACTIVE_HIGH>;
		};

		wan_led: led-2 {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WAN;
			gpios = <&gpio3 RK_PC3 GPIO_ACTIVE_HIGH>;
		};
	};

	vdd_usbc: vdd-usbc-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vdd_usbc";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
	};

	vcc5v0_sys: vcc5v0-sys-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc5v0_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&vdd_usbc>;
	};

	vcc3v3_sys: vcc3v3-sys-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc3v3_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		vin-supply = <&vcc5v0_sys>;
	};

	vcc5v0_usb: vcc5v0_usb-regulator {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio0 RK_PA6 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&vcc5v0_usb_host_en>;
		regulator-name = "vcc5v0_usb";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&vcc5v0_sys>;
	};
};

&combphy1 {
	status = "okay";
};

&combphy2 {
	status = "okay";
};

&cpu0 {
	cpu-supply = <&vdd_cpu>;
};

&cpu1 {
	cpu-supply = <&vdd_cpu>;
};

&cpu2 {
	cpu-supply = <&vdd_cpu>;
};

&cpu3 {
	cpu-supply = <&vdd_cpu>;
};

&gmac1 {
	assigned-clocks = <&cru SCLK_GMAC1_RX_TX>, <&cru SCLK_GMAC1>;
	assigned-clock-parents = <&cru SCLK_GMAC1_RGMII_SPEED>, <&cru CLK_MAC1_2TOP>;
	assigned-clock-rates = <0>, <125000000>;
	clock_in_out = "output";
	phy-mode = "rgmii-id";
	phy-handle = <&rgmii_phy1>;
	pinctrl-names = "default";
	pinctrl-0 = <&gmac1m0_miim
		     &gmac1m0_tx_bus2_level3
		     &gmac1m0_rx_bus2
		     &gmac1m0_rgmii_clk_level2
		     &gmac1m0_rgmii_bus_level3>;
	snps,reset-gpio = <&gpio4 RK_PC2 GPIO_ACTIVE_LOW>;
	snps,reset-active-low;
	/* Reset time is 20ms, 100ms for rtl8211f */
	snps,reset-delays-us = <0 20000 100000>;
	status = "okay";
};

&gpu {
	mali-supply = <&vdd_gpu>;
	status = "okay";
};

&i2c0 {
	status = "okay";

	vdd_cpu: regulator@1c {
		compatible = "tcs,tcs4525";
		reg = <0x1c>;
		fcs,suspend-voltage-selector = <1>;
		regulator-name = "vdd_cpu";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <800000>;
		regulator-max-microvolt = <1150000>;
		regulator-ramp-delay = <2300>;
		vin-supply = <&vcc5v0_sys>;

		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	rk809: pmic@20 {
		compatible = "rockchip,rk809";
		reg = <0x20>;
		interrupt-parent = <&gpio0>;
		interrupts = <RK_PA3 IRQ_TYPE_LEVEL_LOW>;
		#clock-cells = <1>;
		pinctrl-names = "default";
		pinctrl-0 = <&pmic_int>;
		system-power-controller;
		vcc1-supply = <&vcc3v3_sys>;
		vcc2-supply = <&vcc3v3_sys>;
		vcc3-supply = <&vcc3v3_sys>;
		vcc4-supply = <&vcc3v3_sys>;
		vcc5-supply = <&vcc3v3_sys>;
		vcc6-supply = <&vcc3v3_sys>;
		vcc7-supply = <&vcc3v3_sys>;
		vcc8-supply = <&vcc3v3_sys>;
		vcc9-supply = <&vcc3v3_sys>;
		wakeup-source;

		regulators {
			vdd_logic: DCDC_REG1 {
				regulator-name = "vdd_logic";
				regulator-always-on;
				regulator-boot-on;
				regulator-initial-mode = <0x2>;
				regulator-min-microvolt = <500000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_gpu: DCDC_REG2 {
				regulator-name = "vdd_gpu";
				regulator-always-on;
				regulator-initial-mode = <0x2>;
				regulator-min-microvolt = <500000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_ddr: DCDC_REG3 {
				regulator-name = "vcc_ddr";
				regulator-always-on;
				regulator-boot-on;
				regulator-initial-mode = <0x2>;

				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vdd_npu: DCDC_REG4 {
				regulator-name = "vdd_npu";
				regulator-initial-mode = <0x2>;
				regulator-min-microvolt = <500000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_1v8: DCDC_REG5 {
				regulator-name = "vcc_1v8";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdda0v9_image: LDO_REG1 {
				regulator-name = "vdda0v9_image";
				regulator-min-microvolt = <950000>;
				regulator-max-microvolt = <950000>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdda_0v9: LDO_REG2 {
				regulator-name = "vdda_0v9";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <900000>;
				regulator-max-microvolt = <900000>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdda0v9_pmu: LDO_REG3 {
				regulator-name = "vdda0v9_pmu";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <900000>;
				regulator-max-microvolt = <900000>;

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <900000>;
				};
			};

			vccio_acodec: LDO_REG4 {
				regulator-name = "vccio_acodec";
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vccio_sd: LDO_REG5 {
				regulator-name = "vccio_sd";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc3v3_pmu: LDO_REG6 {
				regulator-name = "vcc3v3_pmu";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcca_1v8: LDO_REG7 {
				regulator-name = "vcca_1v8";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcca1v8_pmu: LDO_REG8 {
				regulator-name = "vcca1v8_pmu";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcca1v8_image: LDO_REG9 {
				regulator-name = "vcca1v8_image";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_3v3: SWITCH_REG1 {
				regulator-name = "vcc_3v3";
				regulator-always-on;
				regulator-boot-on;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc3v3_sd: SWITCH_REG2 {
				regulator-name = "vcc3v3_sd";
				regulator-always-on;
				regulator-boot-on;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};
		};
	};
};

&i2c1 {
	status = "okay";

	hym8563: rtc@51 {
		compatible = "haoyu,hym8563";
		reg = <0x51>;
		#clock-cells = <0>;
		clock-output-names = "hym8563";
		pinctrl-names = "default";
		pinctrl-0 = <&hym8563_int>;
		interrupt-parent = <&gpio0>;
		interrupts = <RK_PD3 IRQ_TYPE_LEVEL_LOW>;
		wakeup-source;
	};
};

&mdio1 {
	rgmii_phy1: ethernet-phy@1 {
		compatible = "ethernet-phy-ieee802.3-c22";
		reg = <1>;
		interrupt-parent = <&gpio4>;
		interrupts = <RK_PC3 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&eth_phy_reset_pin>;
		realtek,led-data = <0xae00>;
	};
};

&pcie2x1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pcie_reset_h>;
	reset-gpios = <&gpio4 RK_PC6 GPIO_ACTIVE_HIGH>;
	status = "okay";

	pcie@0,0 {
		reg = <0x00000000 0 0 0 0>;
		#address-cells = <3>;
		#size-cells = <2>;

		rtl8168: pcie@1,0 {
			compatible = "pci10ec,8168";
			reg = <0x000000 0 0 0 0>;
			realtek,led-data = <0x870>;
		};
	};
};

&pinctrl {
	gpio-leds {
		lan_led_pin: lan-led-pin {
			rockchip,pins = <3 RK_PC2 RK_FUNC_GPIO &pcfg_pull_none>;
		};

		power_led_pin: power-led-pin {
			rockchip,pins = <0 RK_PB7 RK_FUNC_GPIO &pcfg_pull_none>;
		};

		wan_led_pin: wan-led-pin {
			rockchip,pins = <3 RK_PC3 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	gmac {
		eth_phy_reset_pin: eth-phy-reset-pin {
			rockchip,pins = <4 RK_PC2 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	pcie {
		pcie_reset_h: pcie-reset-h {
			rockchip,pins = <4 RK_PC6 RK_FUNC_GPIO &pcfg_pull_down>;
		};
	};

	pmic {
		pmic_int: pmic-int {
			rockchip,pins = <0 RK_PA3 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	rockchip-key {
		reset_button_pin: reset-button-pin {
			rockchip,pins = <0 RK_PC2 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	rtc {
		hym8563_int: hym8563-int {
			rockchip,pins = <0 RK_PD3 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	usb {
		vcc5v0_usb_host_en: vcc5v0-usb-host-en {
			rockchip,pins = <0 RK_PA6 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};
};

&pmu_io_domains {
	status = "okay";
	pmuio1-supply = <&vcc3v3_pmu>;
	pmuio2-supply = <&vcc3v3_pmu>;
	vccio1-supply = <&vccio_acodec>;
	vccio2-supply = <&vcc_1v8>;
	vccio3-supply = <&vccio_sd>;
	vccio4-supply = <&vcc_3v3>;
	vccio5-supply = <&vcc_1v8>;
	vccio6-supply = <&vcc_3v3>;
	vccio7-supply = <&vcc_3v3>;
};

&sdhci {
	bus-width = <8>;
	max-frequency = <200000000>;
	non-removable;
	pinctrl-names = "default";
	pinctrl-0 = <&emmc_bus8 &emmc_clk &emmc_cmd &emmc_datastrobe>;
	status = "okay";
};

&sdmmc0 {
	bus-width = <4>;
	cap-mmc-highspeed;
	cap-sd-highspeed;
	disable-wp;
	max-frequency = <150000000>;
	no-sdio;
	no-mmc;
	pinctrl-names = "default";
	pinctrl-0 = <&sdmmc0_bus4 &sdmmc0_clk &sdmmc0_cmd &sdmmc0_det>;
	sd-uhs-sdr50;
	vmmc-supply = <&vcc3v3_sd>;
	vqmmc-supply = <&vccio_sd>;
	status = "okay";
};

&tsadc {
	status = "okay";
};

&uart2 {
	status = "okay";
};

&usb2phy0 {
	status = "okay";
};

&usb2phy0_host {
	phy-supply = <&vcc5v0_usb>;
	status = "okay";
};

&usb2phy0_otg {
	status = "okay";
};

&usb_host0_xhci {
	extcon = <&usb2phy0>;
	status = "okay";
};

&usb_host1_xhci {
	status = "okay";
};

&vop {
	assigned-clocks = <&cru DCLK_VOP0>, <&cru DCLK_VOP1>;
	assigned-clock-parents = <&pmucru PLL_HPLL>, <&cru PLL_VPLL>;
	status = "okay";
};

&vop_mmu {
	status = "okay";
};
