From a6118ebc98ec0081064ccc01d0d23f029a504d71 Mon Sep 17 00:00:00 2001
From: Christian Marangi <ansuelsmth@gmail.com>
Date: Wed, 4 Dec 2024 01:49:09 +0100
Subject: [PATCH] arm64: dts: qcom: Add label to EDMA port for IPQ9574 RDP433

Add label to EDMA port for IPQ9574 RDP433 board.

Signed-off-by: Christian Marangi <ansuelsmth@gmail.com>
---
 arch/arm64/boot/dts/qcom/ipq9574-rdp433.dts | 6 ++++++
 1 file changed, 6 insertions(+)

--- a/arch/arm64/boot/dts/qcom/ipq9574-rdp433.dts
+++ b/arch/arm64/boot/dts/qcom/ipq9574-rdp433.dts
@@ -161,6 +161,7 @@
 			reg = <1>;
 			phy-mode = "qsgmii";
 			managed = "in-band-status";
+			label = "lan1";
 			phy-handle = <&phy0>;
 			pcs-handle = <&pcsuniphy0_ch0>;
 			clocks = <&nsscc NSS_CC_PORT1_MAC_CLK>,
@@ -181,6 +182,7 @@
 			reg = <2>;
 			phy-mode = "qsgmii";
 			managed = "in-band-status";
+			label = "lan2";
 			phy-handle = <&phy1>;
 			pcs-handle = <&pcsuniphy0_ch1>;
 			clocks = <&nsscc NSS_CC_PORT2_MAC_CLK>,
@@ -201,6 +203,7 @@
 			reg = <3>;
 			phy-mode = "qsgmii";
 			managed = "in-band-status";
+			label = "lan3";
 			phy-handle = <&phy2>;
 			pcs-handle = <&pcsuniphy0_ch2>;
 			clocks = <&nsscc NSS_CC_PORT3_MAC_CLK>,
@@ -221,6 +224,7 @@
 			reg = <4>;
 			phy-mode = "qsgmii";
 			managed = "in-band-status";
+			label = "lan4";
 			phy-handle = <&phy3>;
 			pcs-handle = <&pcsuniphy0_ch3>;
 			clocks = <&nsscc NSS_CC_PORT4_MAC_CLK>,
@@ -241,6 +245,7 @@
 			reg = <5>;
 			phy-mode = "usxgmii";
 			managed = "in-band-status";
+			label = "lan5";
 			phy-handle = <&phy4>;
 			pcs-handle = <&pcsuniphy1_ch0>;
 			clocks = <&nsscc NSS_CC_PORT5_MAC_CLK>,
@@ -261,6 +266,7 @@
 			reg = <6>;
 			phy-mode = "usxgmii";
 			managed = "in-band-status";
+			label = "wan";
 			phy-handle = <&phy5>;
 			pcs-handle = <&pcsuniphy2_ch0>;
 			clocks = <&nsscc NSS_CC_PORT6_MAC_CLK>,
