From d8be616ac9444f9dfef9e027fccad8c379b49433 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.com>
Date: Fri, 8 Dec 2023 15:29:38 +0000
Subject: [PATCH 0788/1085] ARM: dts: bcm2712: PWM references include polarity

Increase #pwm-cells to 3 to allow for the extra polarity word.

Signed-off-by: Phil Elwell <phil@raspberrypi.com>
---
 arch/arm/boot/dts/broadcom/bcm2712.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/broadcom/bcm2712.dtsi
+++ b/arch/arm/boot/dts/broadcom/bcm2712.dtsi
@@ -628,7 +628,7 @@
 		pwm_aon: pwm@7d517a80 {
 			compatible = "brcm,bcm7038-pwm";
 			reg = <0x7d517a80 0x28>;
-			#pwm-cells = <2>;
+			#pwm-cells = <3>;
 			clocks = <&clk_27MHz>;
 		};
 
