From d14f3a4f1feabb6bb5935bf3b275a1e6bf2208eb Mon Sep 17 00:00:00 2001
From: Marcin Juszkiewicz <marcin.juszkiewicz@linaro.org>
Date: Thu, 29 Aug 2024 14:26:53 +0200
Subject: [PATCH] arm64: dts: rockchip: prepare NanoPC-T6 for LTS board

FriendlyELEC introduced a second version of NanoPC-T6 SBC.

Create common include file and make NanoPC-T6 use it. Following
patches will add LTS version.

Signed-off-by: Marcin Juszkiewicz <marcin.juszkiewicz@linaro.org>
Link: https://lore.kernel.org/r/20240829-friendlyelec-nanopc-t6-lts-v6-2-edff247e8c02@linaro.org
Signed-off-by: Heiko Stuebner <heiko@sntech.de>
---
 .../boot/dts/rockchip/rk3588-nanopc-t6.dts    | 932 +----------------
 .../boot/dts/rockchip/rk3588-nanopc-t6.dtsi   | 945 ++++++++++++++++++
 2 files changed, 947 insertions(+), 930 deletions(-)
 create mode 100644 arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dtsi

--- a/arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dts
@@ -2,944 +2,16 @@
 /*
  * Copyright (c) 2021 Rockchip Electronics Co., Ltd.
  * Copyright (c) 2023 Thomas McKahan
+ * Copyright (c) 2024 Linaro Ltd.
  *
  */
 
 /dts-v1/;
 
-#include <dt-bindings/gpio/gpio.h>
-#include <dt-bindings/pinctrl/rockchip.h>
-#include <dt-bindings/usb/pd.h>
-#include "rk3588.dtsi"
+#include "rk3588-nanopc-t6.dtsi"
 
 / {
 	model = "FriendlyElec NanoPC-T6";
 	compatible = "friendlyarm,nanopc-t6", "rockchip,rk3588";
 
-	aliases {
-		mmc0 = &sdhci;
-		mmc1 = &sdmmc;
-	};
-
-	chosen {
-		stdout-path = "serial2:1500000n8";
-	};
-
-	leds {
-		compatible = "gpio-leds";
-
-		sys_led: led-0 {
-			gpios = <&gpio2 RK_PB7 GPIO_ACTIVE_HIGH>;
-			label = "system-led";
-			linux,default-trigger = "heartbeat";
-			pinctrl-names = "default";
-			pinctrl-0 = <&sys_led_pin>;
-		};
-
-		usr_led: led-1 {
-			gpios = <&gpio2 RK_PC0 GPIO_ACTIVE_HIGH>;
-			label = "user-led";
-			pinctrl-names = "default";
-			pinctrl-0 = <&usr_led_pin>;
-		};
-	};
-
-	sound {
-		compatible = "simple-audio-card";
-		pinctrl-names = "default";
-		pinctrl-0 = <&hp_det>;
-
-		simple-audio-card,name = "realtek,rt5616-codec";
-		simple-audio-card,format = "i2s";
-		simple-audio-card,mclk-fs = <256>;
-
-		simple-audio-card,hp-det-gpio = <&gpio1 RK_PC4 GPIO_ACTIVE_LOW>;
-		simple-audio-card,hp-pin-name = "Headphones";
-
-		simple-audio-card,widgets =
-			"Headphone", "Headphones",
-			"Microphone", "Microphone Jack";
-		simple-audio-card,routing =
-			"Headphones", "HPOL",
-			"Headphones", "HPOR",
-			"MIC1", "Microphone Jack",
-			"Microphone Jack", "micbias1";
-
-		simple-audio-card,cpu {
-			sound-dai = <&i2s0_8ch>;
-		};
-		simple-audio-card,codec {
-			sound-dai = <&rt5616>;
-		};
-	};
-
-	vcc12v_dcin: vcc12v-dcin-regulator {
-		compatible = "regulator-fixed";
-		regulator-name = "vcc12v_dcin";
-		regulator-always-on;
-		regulator-boot-on;
-		regulator-min-microvolt = <12000000>;
-		regulator-max-microvolt = <12000000>;
-	};
-
-	/* vcc5v0_sys powers peripherals */
-	vcc5v0_sys: vcc5v0-sys-regulator {
-		compatible = "regulator-fixed";
-		regulator-name = "vcc5v0_sys";
-		regulator-always-on;
-		regulator-boot-on;
-		regulator-min-microvolt = <5000000>;
-		regulator-max-microvolt = <5000000>;
-		vin-supply = <&vcc12v_dcin>;
-	};
-
-	/* vcc4v0_sys powers the RK806, RK860's */
-	vcc4v0_sys: vcc4v0-sys-regulator {
-		compatible = "regulator-fixed";
-		regulator-name = "vcc4v0_sys";
-		regulator-always-on;
-		regulator-boot-on;
-		regulator-min-microvolt = <4000000>;
-		regulator-max-microvolt = <4000000>;
-		vin-supply = <&vcc12v_dcin>;
-	};
-
-	vcc_1v1_nldo_s3: vcc-1v1-nldo-s3-regulator {
-		compatible = "regulator-fixed";
-		regulator-name = "vcc-1v1-nldo-s3";
-		regulator-always-on;
-		regulator-boot-on;
-		regulator-min-microvolt = <1100000>;
-		regulator-max-microvolt = <1100000>;
-		vin-supply = <&vcc4v0_sys>;
-	};
-
-	vcc_3v3_pcie20: vcc3v3-pcie20-regulator {
-		compatible = "regulator-fixed";
-		regulator-name = "vcc_3v3_pcie20";
-		regulator-always-on;
-		regulator-boot-on;
-		regulator-min-microvolt = <3300000>;
-		regulator-max-microvolt = <3300000>;
-		vin-supply = <&vcc_3v3_s3>;
-	};
-
-	vbus5v0_typec: vbus5v0-typec-regulator {
-		compatible = "regulator-fixed";
-		enable-active-high;
-		gpio = <&gpio1 RK_PD2 GPIO_ACTIVE_HIGH>;
-		pinctrl-names = "default";
-		pinctrl-0 = <&typec5v_pwren>;
-		regulator-name = "vbus5v0_typec";
-		regulator-min-microvolt = <5000000>;
-		regulator-max-microvolt = <5000000>;
-		vin-supply = <&vcc5v0_sys>;
-	};
-
-	vcc3v3_pcie2x1l0: vcc3v3-pcie2x1l0-regulator {
-		compatible = "regulator-fixed";
-		enable-active-high;
-		gpio = <&gpio4 RK_PC2 GPIO_ACTIVE_HIGH>;
-		pinctrl-names = "default";
-		pinctrl-0 = <&pcie_m2_1_pwren>;
-		regulator-name = "vcc3v3_pcie2x1l0";
-		regulator-min-microvolt = <3300000>;
-		regulator-max-microvolt = <3300000>;
-		vin-supply = <&vcc5v0_sys>;
-	};
-
-	vcc3v3_pcie30: vcc3v3-pcie30-regulator {
-		compatible = "regulator-fixed";
-		enable-active-high;
-		gpios = <&gpio2 RK_PC5 GPIO_ACTIVE_HIGH>;
-		pinctrl-names = "default";
-		pinctrl-0 = <&pcie_m2_0_pwren>;
-		regulator-name = "vcc3v3_pcie30";
-		regulator-min-microvolt = <3300000>;
-		regulator-max-microvolt = <3300000>;
-		vin-supply = <&vcc5v0_sys>;
-	};
-
-	vcc3v3_sd_s0: vcc3v3-sd-s0-regulator {
-		compatible = "regulator-fixed";
-		enable-active-low;
-		gpio = <&gpio4 RK_PA5 GPIO_ACTIVE_LOW>;
-		regulator-boot-on;
-		regulator-max-microvolt = <3300000>;
-		regulator-min-microvolt = <3300000>;
-		regulator-name = "vcc3v3_sd_s0";
-		vin-supply = <&vcc_3v3_s3>;
-	};
-
-	vdd_4g_3v3: vdd-4g-3v3-regulator {
-		compatible = "regulator-fixed";
-		enable-active-high;
-		gpio = <&gpio4 RK_PC6 GPIO_ACTIVE_HIGH>;
-		pinctrl-names = "default";
-		pinctrl-0 = <&pin_4g_lte_pwren>;
-		regulator-name = "vdd_4g_3v3";
-		regulator-min-microvolt = <3300000>;
-		regulator-max-microvolt = <3300000>;
-		vin-supply = <&vcc5v0_sys>;
-	};
-};
-
-&combphy0_ps {
-	status = "okay";
-};
-
-&combphy1_ps {
-	status = "okay";
-};
-
-&combphy2_psu {
-	status = "okay";
-};
-
-&cpu_l0 {
-	cpu-supply = <&vdd_cpu_lit_s0>;
-};
-
-&cpu_l1 {
-	cpu-supply = <&vdd_cpu_lit_s0>;
-};
-
-&cpu_l2 {
-	cpu-supply = <&vdd_cpu_lit_s0>;
-};
-
-&cpu_l3 {
-	cpu-supply = <&vdd_cpu_lit_s0>;
-};
-
-&cpu_b0{
-	cpu-supply = <&vdd_cpu_big0_s0>;
-};
-
-&cpu_b1{
-	cpu-supply = <&vdd_cpu_big0_s0>;
-};
-
-&cpu_b2{
-	cpu-supply = <&vdd_cpu_big1_s0>;
-};
-
-&cpu_b3{
-	cpu-supply = <&vdd_cpu_big1_s0>;
-};
-
-&gpio0 {
-	gpio-line-names = /* GPIO0 A0-A7 */
-			  "", "", "", "",
-			  "", "", "", "",
-			  /* GPIO0 B0-B7 */
-			  "", "", "", "",
-			  "", "", "", "",
-			  /* GPIO0 C0-C7 */
-			  "", "", "", "",
-			  "HEADER_10", "HEADER_08", "HEADER_32", "",
-			  /* GPIO0 D0-D7 */
-			  "", "", "", "",
-			  "", "", "", "";
-};
-
-&gpio1 {
-	gpio-line-names = /* GPIO1 A0-A7 */
-			  "HEADER_27", "HEADER_28", "", "",
-			  "", "", "", "HEADER_15",
-			  /* GPIO1 B0-B7 */
-			  "HEADER_26", "HEADER_21", "HEADER_19", "HEADER_23",
-			  "HEADER_24", "HEADER_22", "", "",
-			  /* GPIO1 C0-C7 */
-			  "", "", "", "",
-			  "", "", "", "",
-			  /* GPIO1 D0-D7 */
-			  "", "", "", "",
-			  "", "", "HEADER_05", "HEADER_03";
-};
-
-&gpio2 {
-	gpio-line-names = /* GPIO2 A0-A7 */
-			  "", "", "", "",
-			  "", "", "", "",
-			  /* GPIO2 B0-B7 */
-			  "", "", "", "",
-			  "", "", "", "",
-			  /* GPIO2 C0-C7 */
-			  "", "CSI1_11", "CSI1_12", "",
-			  "", "", "", "",
-			  /* GPIO2 D0-D7 */
-			  "", "", "", "",
-			  "", "", "", "";
-};
-
-&gpio3 {
-	gpio-line-names = /* GPIO3 A0-A7 */
-			  "HEADER_35", "HEADER_38", "HEADER_40", "HEADER_36",
-			  "HEADER_37", "", "DSI0_12", "",
-			  /* GPIO3 B0-B7 */
-			  "HEADER_33", "DSI0_10", "HEADER_07", "HEADER_16",
-			  "HEADER_18", "HEADER_29", "HEADER_31", "HEADER_12",
-			  /* GPIO3 C0-C7 */
-			  "DSI0_08", "DSI0_14", "HEADER_11", "HEADER_13",
-			  "", "", "", "",
-			  /* GPIO3 D0-D7 */
-			  "", "", "", "",
-			  "", "DSI1_10", "", "";
-};
-
-&gpio4 {
-	gpio-line-names = /* GPIO4 A0-A7 */
-			  "DSI1_08", "DSI1_14", "", "DSI1_12",
-			  "", "", "", "",
-			  /* GPIO4 B0-B7 */
-			  "", "", "", "",
-			  "", "", "", "",
-			  /* GPIO4 C0-C7 */
-			  "", "", "", "",
-			  "CSI0_11", "CSI0_12", "", "",
-			  /* GPIO4 D0-D7 */
-			  "", "", "", "",
-			  "", "", "", "";
-};
-
-&i2c0 {
-	pinctrl-names = "default";
-	pinctrl-0 = <&i2c0m2_xfer>;
-	status = "okay";
-
-	vdd_cpu_big0_s0: regulator@42 {
-		compatible = "rockchip,rk8602";
-		reg = <0x42>;
-		fcs,suspend-voltage-selector = <1>;
-		regulator-name = "vdd_cpu_big0_s0";
-		regulator-always-on;
-		regulator-boot-on;
-		regulator-min-microvolt = <550000>;
-		regulator-max-microvolt = <1050000>;
-		regulator-ramp-delay = <2300>;
-		vin-supply = <&vcc4v0_sys>;
-
-		regulator-state-mem {
-			regulator-off-in-suspend;
-		};
-	};
-
-	vdd_cpu_big1_s0: regulator@43 {
-		compatible = "rockchip,rk8603", "rockchip,rk8602";
-		reg = <0x43>;
-		fcs,suspend-voltage-selector = <1>;
-		regulator-name = "vdd_cpu_big1_s0";
-		regulator-always-on;
-		regulator-boot-on;
-		regulator-min-microvolt = <550000>;
-		regulator-max-microvolt = <1050000>;
-		regulator-ramp-delay = <2300>;
-		vin-supply = <&vcc4v0_sys>;
-
-		regulator-state-mem {
-			regulator-off-in-suspend;
-		};
-	};
-};
-
-&i2c2 {
-	status = "okay";
-
-	vdd_npu_s0: regulator@42 {
-		compatible = "rockchip,rk8602";
-		reg = <0x42>;
-		rockchip,suspend-voltage-selector = <1>;
-		regulator-name = "vdd_npu_s0";
-		regulator-always-on;
-		regulator-boot-on;
-		regulator-min-microvolt = <550000>;
-		regulator-max-microvolt = <950000>;
-		regulator-ramp-delay = <2300>;
-		vin-supply = <&vcc4v0_sys>;
-
-		regulator-state-mem {
-			regulator-off-in-suspend;
-		};
-	};
-};
-
-&i2c6 {
-	clock-frequency = <200000>;
-	status = "okay";
-
-	fusb302: typec-portc@22 {
-		compatible = "fcs,fusb302";
-		reg = <0x22>;
-		interrupt-parent = <&gpio0>;
-		interrupts = <RK_PD3 IRQ_TYPE_LEVEL_LOW>;
-		pinctrl-0 = <&usbc0_int>;
-		pinctrl-names = "default";
-		vbus-supply = <&vbus5v0_typec>;
-
-		connector {
-			compatible = "usb-c-connector";
-			data-role = "dual";
-			label = "USB-C";
-			power-role = "dual";
-			try-power-role = "sink";
-			source-pdos = <PDO_FIXED(5000, 2000, PDO_FIXED_USB_COMM)>;
-			sink-pdos = <PDO_FIXED(5000, 3000, PDO_FIXED_USB_COMM)>;
-			op-sink-microwatt = <1000000>;
-		};
-	};
-
-	hym8563: rtc@51 {
-		compatible = "haoyu,hym8563";
-		reg = <0x51>;
-		#clock-cells = <0>;
-		clock-output-names = "hym8563";
-		pinctrl-names = "default";
-		pinctrl-0 = <&hym8563_int>;
-		interrupt-parent = <&gpio0>;
-		interrupts = <RK_PB0 IRQ_TYPE_LEVEL_LOW>;
-		wakeup-source;
-	};
-};
-
-&i2c7 {
-	clock-frequency = <200000>;
-	status = "okay";
-
-	rt5616: codec@1b {
-		compatible = "realtek,rt5616";
-		reg = <0x1b>;
-		clocks = <&cru I2S0_8CH_MCLKOUT>;
-		clock-names = "mclk";
-		#sound-dai-cells = <0>;
-		assigned-clocks = <&cru I2S0_8CH_MCLKOUT>;
-		assigned-clock-rates = <12288000>;
-
-		port {
-			rt5616_p0_0: endpoint {
-				remote-endpoint = <&i2s0_8ch_p0_0>;
-			};
-		};
-	};
-
-	/* connected with MIPI-CSI1 */
-};
-
-&i2c8 {
-	pinctrl-0 = <&i2c8m2_xfer>;
-};
-
-&i2s0_8ch {
-	pinctrl-names = "default";
-	pinctrl-0 = <&i2s0_lrck
-		     &i2s0_mclk
-		     &i2s0_sclk
-		     &i2s0_sdi0
-		     &i2s0_sdo0>;
-	status = "okay";
-
-	i2s0_8ch_p0: port {
-		i2s0_8ch_p0_0: endpoint {
-			dai-format = "i2s";
-			mclk-fs = <256>;
-			remote-endpoint = <&rt5616_p0_0>;
-		};
-	};
-};
-
-&pcie2x1l0 {
-	reset-gpios = <&gpio4 RK_PB3 GPIO_ACTIVE_HIGH>;
-	vpcie3v3-supply = <&vcc_3v3_pcie20>;
-	pinctrl-names = "default";
-	pinctrl-0 = <&pcie2_0_rst>;
-	status = "okay";
-};
-
-&pcie2x1l1 {
-	reset-gpios = <&gpio4 RK_PA2 GPIO_ACTIVE_HIGH>;
-	vpcie3v3-supply = <&vcc3v3_pcie2x1l0>;
-	pinctrl-names = "default";
-	pinctrl-0 = <&pcie2_1_rst>;
-	status = "okay";
-};
-
-&pcie2x1l2 {
-	reset-gpios = <&gpio4 RK_PA4 GPIO_ACTIVE_HIGH>;
-	vpcie3v3-supply = <&vcc_3v3_pcie20>;
-	pinctrl-names = "default";
-	pinctrl-0 = <&pcie2_2_rst>;
-	status = "okay";
-};
-
-&pcie30phy {
-	status = "okay";
-};
-
-&pcie3x4 {
-	reset-gpios = <&gpio4 RK_PB6 GPIO_ACTIVE_HIGH>;
-	vpcie3v3-supply = <&vcc3v3_pcie30>;
-	status = "okay";
-};
-
-&pinctrl {
-	gpio-leds {
-		sys_led_pin: sys-led-pin {
-			rockchip,pins = <2 RK_PB7 RK_FUNC_GPIO &pcfg_pull_none>;
-		};
-
-		usr_led_pin: usr-led-pin {
-			rockchip,pins = <2 RK_PC0 RK_FUNC_GPIO &pcfg_pull_none>;
-		};
-	};
-
-	headphone {
-		hp_det: hp-det {
-			rockchip,pins = <1 RK_PC4 RK_FUNC_GPIO &pcfg_pull_none>;
-		};
-	};
-
-	hym8563 {
-		hym8563_int: hym8563-int {
-			rockchip,pins = <0 RK_PB0 RK_FUNC_GPIO &pcfg_pull_up>;
-		};
-	};
-
-	pcie {
-		pcie2_0_rst: pcie2-0-rst {
-			rockchip,pins = <4 RK_PB3 RK_FUNC_GPIO &pcfg_pull_none>;
-		};
-
-		pcie2_1_rst: pcie2-1-rst {
-			rockchip,pins = <4 RK_PA2 RK_FUNC_GPIO &pcfg_pull_none>;
-		};
-
-		pcie2_2_rst: pcie2-2-rst {
-			rockchip,pins = <4 RK_PA4 RK_FUNC_GPIO &pcfg_pull_none>;
-		};
-
-		pcie_m2_0_pwren: pcie-m20-pwren {
-			rockchip,pins = <2 RK_PC5 RK_FUNC_GPIO &pcfg_pull_none>;
-		};
-
-		pcie_m2_1_pwren: pcie-m21-pwren {
-			rockchip,pins = <4 RK_PC2 RK_FUNC_GPIO &pcfg_pull_none>;
-		};
-	};
-
-	usb {
-		pin_4g_lte_pwren: 4g-lte-pwren {
-			rockchip,pins = <4 RK_PC6 RK_FUNC_GPIO &pcfg_pull_none>;
-		};
-
-		typec5v_pwren: typec5v-pwren {
-			rockchip,pins = <1 RK_PD2 RK_FUNC_GPIO &pcfg_pull_none>;
-		};
-
-		usbc0_int: usbc0-int {
-			rockchip,pins = <0 RK_PD3 RK_FUNC_GPIO &pcfg_pull_up>;
-		};
-	};
-};
-
-&pwm1 {
-	pinctrl-0 = <&pwm1m1_pins>;
-	status = "okay";
-};
-
-&saradc {
-	vref-supply = <&avcc_1v8_s0>;
-	status = "okay";
-};
-
-&sdhci {
-	bus-width = <8>;
-	no-sdio;
-	no-sd;
-	non-removable;
-	max-frequency = <200000000>;
-	mmc-hs400-1_8v;
-	mmc-hs400-enhanced-strobe;
-	status = "okay";
-};
-
-&sdmmc {
-	bus-width = <4>;
-	cap-mmc-highspeed;
-	cap-sd-highspeed;
-	cd-gpios = <&gpio0 RK_PA4 GPIO_ACTIVE_LOW>;
-	disable-wp;
-	no-mmc;
-	no-sdio;
-	sd-uhs-sdr104;
-	vmmc-supply = <&vcc3v3_sd_s0>;
-	vqmmc-supply = <&vccio_sd_s0>;
-	status = "okay";
-};
-
-&spi2 {
-	status = "okay";
-	assigned-clocks = <&cru CLK_SPI2>;
-	assigned-clock-rates = <200000000>;
-	pinctrl-names = "default";
-	pinctrl-0 = <&spi2m2_cs0 &spi2m2_pins>;
-	num-cs = <1>;
-
-	pmic@0 {
-		compatible = "rockchip,rk806";
-		spi-max-frequency = <1000000>;
-		reg = <0x0>;
-
-		interrupt-parent = <&gpio0>;
-		interrupts = <7 IRQ_TYPE_LEVEL_LOW>;
-
-		pinctrl-names = "default";
-		pinctrl-0 = <&pmic_pins>, <&rk806_dvs1_null>,
-			    <&rk806_dvs2_null>, <&rk806_dvs3_null>;
-
-		system-power-controller;
-
-		vcc1-supply = <&vcc4v0_sys>;
-		vcc2-supply = <&vcc4v0_sys>;
-		vcc3-supply = <&vcc4v0_sys>;
-		vcc4-supply = <&vcc4v0_sys>;
-		vcc5-supply = <&vcc4v0_sys>;
-		vcc6-supply = <&vcc4v0_sys>;
-		vcc7-supply = <&vcc4v0_sys>;
-		vcc8-supply = <&vcc4v0_sys>;
-		vcc9-supply = <&vcc4v0_sys>;
-		vcc10-supply = <&vcc4v0_sys>;
-		vcc11-supply = <&vcc_2v0_pldo_s3>;
-		vcc12-supply = <&vcc4v0_sys>;
-		vcc13-supply = <&vcc_1v1_nldo_s3>;
-		vcc14-supply = <&vcc_1v1_nldo_s3>;
-		vcca-supply = <&vcc4v0_sys>;
-
-		gpio-controller;
-		#gpio-cells = <2>;
-
-		rk806_dvs1_null: dvs1-null-pins {
-			pins = "gpio_pwrctrl1";
-			function = "pin_fun0";
-		};
-
-		rk806_dvs2_null: dvs2-null-pins {
-			pins = "gpio_pwrctrl2";
-			function = "pin_fun0";
-		};
-
-		rk806_dvs3_null: dvs3-null-pins {
-			pins = "gpio_pwrctrl3";
-			function = "pin_fun0";
-		};
-
-		regulators {
-			vdd_gpu_s0: vdd_gpu_mem_s0: dcdc-reg1 {
-				regulator-boot-on;
-				regulator-min-microvolt = <550000>;
-				regulator-max-microvolt = <950000>;
-				regulator-ramp-delay = <12500>;
-				regulator-name = "vdd_gpu_s0";
-				regulator-enable-ramp-delay = <400>;
-
-				regulator-state-mem {
-					regulator-off-in-suspend;
-				};
-			};
-
-			vdd_cpu_lit_s0: vdd_cpu_lit_mem_s0: dcdc-reg2 {
-				regulator-always-on;
-				regulator-boot-on;
-				regulator-min-microvolt = <550000>;
-				regulator-max-microvolt = <950000>;
-				regulator-ramp-delay = <12500>;
-				regulator-name = "vdd_cpu_lit_s0";
-
-				regulator-state-mem {
-					regulator-off-in-suspend;
-				};
-			};
-
-			vdd_log_s0: dcdc-reg3 {
-				regulator-always-on;
-				regulator-boot-on;
-				regulator-min-microvolt = <675000>;
-				regulator-max-microvolt = <750000>;
-				regulator-ramp-delay = <12500>;
-				regulator-name = "vdd_log_s0";
-
-				regulator-state-mem {
-					regulator-off-in-suspend;
-					regulator-suspend-microvolt = <750000>;
-				};
-			};
-
-			vdd_vdenc_s0: vdd_vdenc_mem_s0: dcdc-reg4 {
-				regulator-always-on;
-				regulator-boot-on;
-				regulator-min-microvolt = <550000>;
-				regulator-max-microvolt = <950000>;
-				regulator-init-microvolt = <750000>;
-				regulator-ramp-delay = <12500>;
-				regulator-name = "vdd_vdenc_s0";
-
-				regulator-state-mem {
-					regulator-off-in-suspend;
-				};
-			};
-
-			vdd_ddr_s0: dcdc-reg5 {
-				regulator-always-on;
-				regulator-boot-on;
-				regulator-min-microvolt = <675000>;
-				regulator-max-microvolt = <900000>;
-				regulator-ramp-delay = <12500>;
-				regulator-name = "vdd_ddr_s0";
-
-				regulator-state-mem {
-					regulator-off-in-suspend;
-					regulator-suspend-microvolt = <850000>;
-				};
-			};
-
-			vdd2_ddr_s3: dcdc-reg6 {
-				regulator-always-on;
-				regulator-boot-on;
-				regulator-name = "vdd2_ddr_s3";
-
-				regulator-state-mem {
-					regulator-on-in-suspend;
-				};
-			};
-
-			vcc_2v0_pldo_s3: dcdc-reg7 {
-				regulator-always-on;
-				regulator-boot-on;
-				regulator-min-microvolt = <2000000>;
-				regulator-max-microvolt = <2000000>;
-				regulator-ramp-delay = <12500>;
-				regulator-name = "vdd_2v0_pldo_s3";
-
-				regulator-state-mem {
-					regulator-on-in-suspend;
-					regulator-suspend-microvolt = <2000000>;
-				};
-			};
-
-			vcc_3v3_s3: dcdc-reg8 {
-				regulator-always-on;
-				regulator-boot-on;
-				regulator-min-microvolt = <3300000>;
-				regulator-max-microvolt = <3300000>;
-				regulator-name = "vcc_3v3_s3";
-
-				regulator-state-mem {
-					regulator-on-in-suspend;
-					regulator-suspend-microvolt = <3300000>;
-				};
-			};
-
-			vddq_ddr_s0: dcdc-reg9 {
-				regulator-always-on;
-				regulator-boot-on;
-				regulator-name = "vddq_ddr_s0";
-
-				regulator-state-mem {
-					regulator-off-in-suspend;
-				};
-			};
-
-			vcc_1v8_s3: dcdc-reg10 {
-				regulator-always-on;
-				regulator-boot-on;
-				regulator-min-microvolt = <1800000>;
-				regulator-max-microvolt = <1800000>;
-				regulator-name = "vcc_1v8_s3";
-
-				regulator-state-mem {
-					regulator-on-in-suspend;
-					regulator-suspend-microvolt = <1800000>;
-				};
-			};
-
-			avcc_1v8_s0: pldo-reg1 {
-				regulator-always-on;
-				regulator-boot-on;
-				regulator-min-microvolt = <1800000>;
-				regulator-max-microvolt = <1800000>;
-				regulator-name = "avcc_1v8_s0";
-
-				regulator-state-mem {
-					regulator-off-in-suspend;
-				};
-			};
-
-			vcc_1v8_s0: pldo-reg2 {
-				regulator-always-on;
-				regulator-boot-on;
-				regulator-min-microvolt = <1800000>;
-				regulator-max-microvolt = <1800000>;
-				regulator-name = "vcc_1v8_s0";
-
-				regulator-state-mem {
-					regulator-off-in-suspend;
-					regulator-suspend-microvolt = <1800000>;
-				};
-			};
-
-			avdd_1v2_s0: pldo-reg3 {
-				regulator-always-on;
-				regulator-boot-on;
-				regulator-min-microvolt = <1200000>;
-				regulator-max-microvolt = <1200000>;
-				regulator-name = "avdd_1v2_s0";
-
-				regulator-state-mem {
-					regulator-off-in-suspend;
-				};
-			};
-
-			vcc_3v3_s0: pldo-reg4 {
-				regulator-always-on;
-				regulator-boot-on;
-				regulator-min-microvolt = <3300000>;
-				regulator-max-microvolt = <3300000>;
-				regulator-ramp-delay = <12500>;
-				regulator-name = "vcc_3v3_s0";
-
-				regulator-state-mem {
-					regulator-off-in-suspend;
-				};
-			};
-
-			vccio_sd_s0: pldo-reg5 {
-				regulator-always-on;
-				regulator-boot-on;
-				regulator-min-microvolt = <1800000>;
-				regulator-max-microvolt = <3300000>;
-				regulator-ramp-delay = <12500>;
-				regulator-name = "vccio_sd_s0";
-
-				regulator-state-mem {
-					regulator-off-in-suspend;
-				};
-			};
-
-			pldo6_s3: pldo-reg6 {
-				regulator-always-on;
-				regulator-boot-on;
-				regulator-min-microvolt = <1800000>;
-				regulator-max-microvolt = <1800000>;
-				regulator-name = "pldo6_s3";
-
-				regulator-state-mem {
-					regulator-on-in-suspend;
-					regulator-suspend-microvolt = <1800000>;
-				};
-			};
-
-			vdd_0v75_s3: nldo-reg1 {
-				regulator-always-on;
-				regulator-boot-on;
-				regulator-min-microvolt = <750000>;
-				regulator-max-microvolt = <750000>;
-				regulator-name = "vdd_0v75_s3";
-
-				regulator-state-mem {
-					regulator-on-in-suspend;
-					regulator-suspend-microvolt = <750000>;
-				};
-			};
-
-			vdd_ddr_pll_s0: nldo-reg2 {
-				regulator-always-on;
-				regulator-boot-on;
-				regulator-min-microvolt = <850000>;
-				regulator-max-microvolt = <850000>;
-				regulator-name = "vdd_ddr_pll_s0";
-
-				regulator-state-mem {
-					regulator-off-in-suspend;
-					regulator-suspend-microvolt = <850000>;
-				};
-			};
-
-			avdd_0v75_s0: nldo-reg3 {
-				regulator-always-on;
-				regulator-boot-on;
-				regulator-min-microvolt = <750000>;
-				regulator-max-microvolt = <750000>;
-				regulator-name = "avdd_0v75_s0";
-
-				regulator-state-mem {
-					regulator-off-in-suspend;
-				};
-			};
-
-			vdd_0v85_s0: nldo-reg4 {
-				regulator-always-on;
-				regulator-boot-on;
-				regulator-min-microvolt = <850000>;
-				regulator-max-microvolt = <850000>;
-				regulator-name = "vdd_0v85_s0";
-
-				regulator-state-mem {
-					regulator-off-in-suspend;
-				};
-			};
-
-			vdd_0v75_s0: nldo-reg5 {
-				regulator-always-on;
-				regulator-boot-on;
-				regulator-min-microvolt = <750000>;
-				regulator-max-microvolt = <750000>;
-				regulator-name = "vdd_0v75_s0";
-
-				regulator-state-mem {
-					regulator-off-in-suspend;
-				};
-			};
-		};
-	};
-};
-
-&tsadc {
-	status = "okay";
-};
-
-&uart2 {
-	pinctrl-0 = <&uart2m0_xfer>;
-	status = "okay";
-};
-
-&u2phy2_host {
-	phy-supply = <&vdd_4g_3v3>;
-	status = "okay";
-};
-
-&u2phy3_host {
-	status = "okay";
-};
-
-&u2phy2 {
-	status = "okay";
-};
-
-&u2phy3 {
-	status = "okay";
-};
-
-&usb_host0_ehci {
-	status = "okay";
-};
-
-&usb_host0_ohci {
-	status = "okay";
-};
-
-&usb_host1_ehci {
-	status = "okay";
-};
-
-&usb_host1_ohci {
-	status = "okay";
 };
--- /dev/null
+++ b/arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dtsi
@@ -0,0 +1,945 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Copyright (c) 2021 Rockchip Electronics Co., Ltd.
+ * Copyright (c) 2023 Thomas McKahan
+ *
+ */
+
+/dts-v1/;
+
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/pinctrl/rockchip.h>
+#include <dt-bindings/usb/pd.h>
+#include "rk3588.dtsi"
+
+/ {
+	model = "FriendlyElec NanoPC-T6";
+	compatible = "friendlyarm,nanopc-t6", "rockchip,rk3588";
+
+	aliases {
+		mmc0 = &sdhci;
+		mmc1 = &sdmmc;
+	};
+
+	chosen {
+		stdout-path = "serial2:1500000n8";
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		sys_led: led-0 {
+			gpios = <&gpio2 RK_PB7 GPIO_ACTIVE_HIGH>;
+			label = "system-led";
+			linux,default-trigger = "heartbeat";
+			pinctrl-names = "default";
+			pinctrl-0 = <&sys_led_pin>;
+		};
+
+		usr_led: led-1 {
+			gpios = <&gpio2 RK_PC0 GPIO_ACTIVE_HIGH>;
+			label = "user-led";
+			pinctrl-names = "default";
+			pinctrl-0 = <&usr_led_pin>;
+		};
+	};
+
+	sound {
+		compatible = "simple-audio-card";
+		pinctrl-names = "default";
+		pinctrl-0 = <&hp_det>;
+
+		simple-audio-card,name = "realtek,rt5616-codec";
+		simple-audio-card,format = "i2s";
+		simple-audio-card,mclk-fs = <256>;
+
+		simple-audio-card,hp-det-gpio = <&gpio1 RK_PC4 GPIO_ACTIVE_LOW>;
+		simple-audio-card,hp-pin-name = "Headphones";
+
+		simple-audio-card,widgets =
+			"Headphone", "Headphones",
+			"Microphone", "Microphone Jack";
+		simple-audio-card,routing =
+			"Headphones", "HPOL",
+			"Headphones", "HPOR",
+			"MIC1", "Microphone Jack",
+			"Microphone Jack", "micbias1";
+
+		simple-audio-card,cpu {
+			sound-dai = <&i2s0_8ch>;
+		};
+		simple-audio-card,codec {
+			sound-dai = <&rt5616>;
+		};
+	};
+
+	vcc12v_dcin: vcc12v-dcin-regulator {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc12v_dcin";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <12000000>;
+		regulator-max-microvolt = <12000000>;
+	};
+
+	/* vcc5v0_sys powers peripherals */
+	vcc5v0_sys: vcc5v0-sys-regulator {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc5v0_sys";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		vin-supply = <&vcc12v_dcin>;
+	};
+
+	/* vcc4v0_sys powers the RK806, RK860's */
+	vcc4v0_sys: vcc4v0-sys-regulator {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc4v0_sys";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <4000000>;
+		regulator-max-microvolt = <4000000>;
+		vin-supply = <&vcc12v_dcin>;
+	};
+
+	vcc_1v1_nldo_s3: vcc-1v1-nldo-s3-regulator {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc-1v1-nldo-s3";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <1100000>;
+		regulator-max-microvolt = <1100000>;
+		vin-supply = <&vcc4v0_sys>;
+	};
+
+	vcc_3v3_pcie20: vcc3v3-pcie20-regulator {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc_3v3_pcie20";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		vin-supply = <&vcc_3v3_s3>;
+	};
+
+	vbus5v0_typec: vbus5v0-typec-regulator {
+		compatible = "regulator-fixed";
+		enable-active-high;
+		gpio = <&gpio1 RK_PD2 GPIO_ACTIVE_HIGH>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&typec5v_pwren>;
+		regulator-name = "vbus5v0_typec";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		vin-supply = <&vcc5v0_sys>;
+	};
+
+	vcc3v3_pcie2x1l0: vcc3v3-pcie2x1l0-regulator {
+		compatible = "regulator-fixed";
+		enable-active-high;
+		gpio = <&gpio4 RK_PC2 GPIO_ACTIVE_HIGH>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&pcie_m2_1_pwren>;
+		regulator-name = "vcc3v3_pcie2x1l0";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		vin-supply = <&vcc5v0_sys>;
+	};
+
+	vcc3v3_pcie30: vcc3v3-pcie30-regulator {
+		compatible = "regulator-fixed";
+		enable-active-high;
+		gpios = <&gpio2 RK_PC5 GPIO_ACTIVE_HIGH>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&pcie_m2_0_pwren>;
+		regulator-name = "vcc3v3_pcie30";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		vin-supply = <&vcc5v0_sys>;
+	};
+
+	vcc3v3_sd_s0: vcc3v3-sd-s0-regulator {
+		compatible = "regulator-fixed";
+		enable-active-low;
+		gpio = <&gpio4 RK_PA5 GPIO_ACTIVE_LOW>;
+		regulator-boot-on;
+		regulator-max-microvolt = <3300000>;
+		regulator-min-microvolt = <3300000>;
+		regulator-name = "vcc3v3_sd_s0";
+		vin-supply = <&vcc_3v3_s3>;
+	};
+
+	vdd_4g_3v3: vdd-4g-3v3-regulator {
+		compatible = "regulator-fixed";
+		enable-active-high;
+		gpio = <&gpio4 RK_PC6 GPIO_ACTIVE_HIGH>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&pin_4g_lte_pwren>;
+		regulator-name = "vdd_4g_3v3";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		vin-supply = <&vcc5v0_sys>;
+	};
+};
+
+&combphy0_ps {
+	status = "okay";
+};
+
+&combphy1_ps {
+	status = "okay";
+};
+
+&combphy2_psu {
+	status = "okay";
+};
+
+&cpu_l0 {
+	cpu-supply = <&vdd_cpu_lit_s0>;
+};
+
+&cpu_l1 {
+	cpu-supply = <&vdd_cpu_lit_s0>;
+};
+
+&cpu_l2 {
+	cpu-supply = <&vdd_cpu_lit_s0>;
+};
+
+&cpu_l3 {
+	cpu-supply = <&vdd_cpu_lit_s0>;
+};
+
+&cpu_b0 {
+	cpu-supply = <&vdd_cpu_big0_s0>;
+};
+
+&cpu_b1 {
+	cpu-supply = <&vdd_cpu_big0_s0>;
+};
+
+&cpu_b2 {
+	cpu-supply = <&vdd_cpu_big1_s0>;
+};
+
+&cpu_b3 {
+	cpu-supply = <&vdd_cpu_big1_s0>;
+};
+
+&gpio0 {
+	gpio-line-names = /* GPIO0 A0-A7 */
+			  "", "", "", "",
+			  "", "", "", "",
+			  /* GPIO0 B0-B7 */
+			  "", "", "", "",
+			  "", "", "", "",
+			  /* GPIO0 C0-C7 */
+			  "", "", "", "",
+			  "HEADER_10", "HEADER_08", "HEADER_32", "",
+			  /* GPIO0 D0-D7 */
+			  "", "", "", "",
+			  "", "", "", "";
+};
+
+&gpio1 {
+	gpio-line-names = /* GPIO1 A0-A7 */
+			  "HEADER_27", "HEADER_28", "", "",
+			  "", "", "", "HEADER_15",
+			  /* GPIO1 B0-B7 */
+			  "HEADER_26", "HEADER_21", "HEADER_19", "HEADER_23",
+			  "HEADER_24", "HEADER_22", "", "",
+			  /* GPIO1 C0-C7 */
+			  "", "", "", "",
+			  "", "", "", "",
+			  /* GPIO1 D0-D7 */
+			  "", "", "", "",
+			  "", "", "HEADER_05", "HEADER_03";
+};
+
+&gpio2 {
+	gpio-line-names = /* GPIO2 A0-A7 */
+			  "", "", "", "",
+			  "", "", "", "",
+			  /* GPIO2 B0-B7 */
+			  "", "", "", "",
+			  "", "", "", "",
+			  /* GPIO2 C0-C7 */
+			  "", "CSI1_11", "CSI1_12", "",
+			  "", "", "", "",
+			  /* GPIO2 D0-D7 */
+			  "", "", "", "",
+			  "", "", "", "";
+};
+
+&gpio3 {
+	gpio-line-names = /* GPIO3 A0-A7 */
+			  "HEADER_35", "HEADER_38", "HEADER_40", "HEADER_36",
+			  "HEADER_37", "", "DSI0_12", "",
+			  /* GPIO3 B0-B7 */
+			  "HEADER_33", "DSI0_10", "HEADER_07", "HEADER_16",
+			  "HEADER_18", "HEADER_29", "HEADER_31", "HEADER_12",
+			  /* GPIO3 C0-C7 */
+			  "DSI0_08", "DSI0_14", "HEADER_11", "HEADER_13",
+			  "", "", "", "",
+			  /* GPIO3 D0-D7 */
+			  "", "", "", "",
+			  "", "DSI1_10", "", "";
+};
+
+&gpio4 {
+	gpio-line-names = /* GPIO4 A0-A7 */
+			  "DSI1_08", "DSI1_14", "", "DSI1_12",
+			  "", "", "", "",
+			  /* GPIO4 B0-B7 */
+			  "", "", "", "",
+			  "", "", "", "",
+			  /* GPIO4 C0-C7 */
+			  "", "", "", "",
+			  "CSI0_11", "CSI0_12", "", "",
+			  /* GPIO4 D0-D7 */
+			  "", "", "", "",
+			  "", "", "", "";
+};
+
+&i2c0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c0m2_xfer>;
+	status = "okay";
+
+	vdd_cpu_big0_s0: regulator@42 {
+		compatible = "rockchip,rk8602";
+		reg = <0x42>;
+		fcs,suspend-voltage-selector = <1>;
+		regulator-name = "vdd_cpu_big0_s0";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <550000>;
+		regulator-max-microvolt = <1050000>;
+		regulator-ramp-delay = <2300>;
+		vin-supply = <&vcc4v0_sys>;
+
+		regulator-state-mem {
+			regulator-off-in-suspend;
+		};
+	};
+
+	vdd_cpu_big1_s0: regulator@43 {
+		compatible = "rockchip,rk8603", "rockchip,rk8602";
+		reg = <0x43>;
+		fcs,suspend-voltage-selector = <1>;
+		regulator-name = "vdd_cpu_big1_s0";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <550000>;
+		regulator-max-microvolt = <1050000>;
+		regulator-ramp-delay = <2300>;
+		vin-supply = <&vcc4v0_sys>;
+
+		regulator-state-mem {
+			regulator-off-in-suspend;
+		};
+	};
+};
+
+&i2c2 {
+	status = "okay";
+
+	vdd_npu_s0: regulator@42 {
+		compatible = "rockchip,rk8602";
+		reg = <0x42>;
+		rockchip,suspend-voltage-selector = <1>;
+		regulator-name = "vdd_npu_s0";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <550000>;
+		regulator-max-microvolt = <950000>;
+		regulator-ramp-delay = <2300>;
+		vin-supply = <&vcc4v0_sys>;
+
+		regulator-state-mem {
+			regulator-off-in-suspend;
+		};
+	};
+};
+
+&i2c6 {
+	clock-frequency = <200000>;
+	status = "okay";
+
+	fusb302: typec-portc@22 {
+		compatible = "fcs,fusb302";
+		reg = <0x22>;
+		interrupt-parent = <&gpio0>;
+		interrupts = <RK_PD3 IRQ_TYPE_LEVEL_LOW>;
+		pinctrl-0 = <&usbc0_int>;
+		pinctrl-names = "default";
+		vbus-supply = <&vbus5v0_typec>;
+
+		connector {
+			compatible = "usb-c-connector";
+			data-role = "dual";
+			label = "USB-C";
+			power-role = "dual";
+			try-power-role = "sink";
+			source-pdos = <PDO_FIXED(5000, 2000, PDO_FIXED_USB_COMM)>;
+			sink-pdos = <PDO_FIXED(5000, 3000, PDO_FIXED_USB_COMM)>;
+			op-sink-microwatt = <1000000>;
+		};
+	};
+
+	hym8563: rtc@51 {
+		compatible = "haoyu,hym8563";
+		reg = <0x51>;
+		#clock-cells = <0>;
+		clock-output-names = "hym8563";
+		pinctrl-names = "default";
+		pinctrl-0 = <&hym8563_int>;
+		interrupt-parent = <&gpio0>;
+		interrupts = <RK_PB0 IRQ_TYPE_LEVEL_LOW>;
+		wakeup-source;
+	};
+};
+
+&i2c7 {
+	clock-frequency = <200000>;
+	status = "okay";
+
+	rt5616: codec@1b {
+		compatible = "realtek,rt5616";
+		reg = <0x1b>;
+		clocks = <&cru I2S0_8CH_MCLKOUT>;
+		clock-names = "mclk";
+		#sound-dai-cells = <0>;
+		assigned-clocks = <&cru I2S0_8CH_MCLKOUT>;
+		assigned-clock-rates = <12288000>;
+
+		port {
+			rt5616_p0_0: endpoint {
+				remote-endpoint = <&i2s0_8ch_p0_0>;
+			};
+		};
+	};
+
+	/* connected with MIPI-CSI1 */
+};
+
+&i2c8 {
+	pinctrl-0 = <&i2c8m2_xfer>;
+};
+
+&i2s0_8ch {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s0_lrck
+		     &i2s0_mclk
+		     &i2s0_sclk
+		     &i2s0_sdi0
+		     &i2s0_sdo0>;
+	status = "okay";
+
+	i2s0_8ch_p0: port {
+		i2s0_8ch_p0_0: endpoint {
+			dai-format = "i2s";
+			mclk-fs = <256>;
+			remote-endpoint = <&rt5616_p0_0>;
+		};
+	};
+};
+
+&pcie2x1l0 {
+	reset-gpios = <&gpio4 RK_PB3 GPIO_ACTIVE_HIGH>;
+	vpcie3v3-supply = <&vcc_3v3_pcie20>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&pcie2_0_rst>;
+	status = "okay";
+};
+
+&pcie2x1l1 {
+	reset-gpios = <&gpio4 RK_PA2 GPIO_ACTIVE_HIGH>;
+	vpcie3v3-supply = <&vcc3v3_pcie2x1l0>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&pcie2_1_rst>;
+	status = "okay";
+};
+
+&pcie2x1l2 {
+	reset-gpios = <&gpio4 RK_PA4 GPIO_ACTIVE_HIGH>;
+	vpcie3v3-supply = <&vcc_3v3_pcie20>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&pcie2_2_rst>;
+	status = "okay";
+};
+
+&pcie30phy {
+	status = "okay";
+};
+
+&pcie3x4 {
+	reset-gpios = <&gpio4 RK_PB6 GPIO_ACTIVE_HIGH>;
+	vpcie3v3-supply = <&vcc3v3_pcie30>;
+	status = "okay";
+};
+
+&pinctrl {
+	gpio-leds {
+		sys_led_pin: sys-led-pin {
+			rockchip,pins = <2 RK_PB7 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		usr_led_pin: usr-led-pin {
+			rockchip,pins = <2 RK_PC0 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	headphone {
+		hp_det: hp-det {
+			rockchip,pins = <1 RK_PC4 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	hym8563 {
+		hym8563_int: hym8563-int {
+			rockchip,pins = <0 RK_PB0 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+	};
+
+	pcie {
+		pcie2_0_rst: pcie2-0-rst {
+			rockchip,pins = <4 RK_PB3 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		pcie2_1_rst: pcie2-1-rst {
+			rockchip,pins = <4 RK_PA2 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		pcie2_2_rst: pcie2-2-rst {
+			rockchip,pins = <4 RK_PA4 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		pcie_m2_0_pwren: pcie-m20-pwren {
+			rockchip,pins = <2 RK_PC5 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		pcie_m2_1_pwren: pcie-m21-pwren {
+			rockchip,pins = <4 RK_PC2 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	usb {
+		pin_4g_lte_pwren: 4g-lte-pwren {
+			rockchip,pins = <4 RK_PC6 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		typec5v_pwren: typec5v-pwren {
+			rockchip,pins = <1 RK_PD2 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		usbc0_int: usbc0-int {
+			rockchip,pins = <0 RK_PD3 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+	};
+};
+
+&pwm1 {
+	pinctrl-0 = <&pwm1m1_pins>;
+	status = "okay";
+};
+
+&saradc {
+	vref-supply = <&avcc_1v8_s0>;
+	status = "okay";
+};
+
+&sdhci {
+	bus-width = <8>;
+	no-sdio;
+	no-sd;
+	non-removable;
+	max-frequency = <200000000>;
+	mmc-hs400-1_8v;
+	mmc-hs400-enhanced-strobe;
+	status = "okay";
+};
+
+&sdmmc {
+	bus-width = <4>;
+	cap-mmc-highspeed;
+	cap-sd-highspeed;
+	cd-gpios = <&gpio0 RK_PA4 GPIO_ACTIVE_LOW>;
+	disable-wp;
+	no-mmc;
+	no-sdio;
+	sd-uhs-sdr104;
+	vmmc-supply = <&vcc3v3_sd_s0>;
+	vqmmc-supply = <&vccio_sd_s0>;
+	status = "okay";
+};
+
+&spi2 {
+	status = "okay";
+	assigned-clocks = <&cru CLK_SPI2>;
+	assigned-clock-rates = <200000000>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi2m2_cs0 &spi2m2_pins>;
+	num-cs = <1>;
+
+	pmic@0 {
+		compatible = "rockchip,rk806";
+		spi-max-frequency = <1000000>;
+		reg = <0x0>;
+
+		interrupt-parent = <&gpio0>;
+		interrupts = <7 IRQ_TYPE_LEVEL_LOW>;
+
+		pinctrl-names = "default";
+		pinctrl-0 = <&pmic_pins>, <&rk806_dvs1_null>,
+			    <&rk806_dvs2_null>, <&rk806_dvs3_null>;
+
+		system-power-controller;
+
+		vcc1-supply = <&vcc4v0_sys>;
+		vcc2-supply = <&vcc4v0_sys>;
+		vcc3-supply = <&vcc4v0_sys>;
+		vcc4-supply = <&vcc4v0_sys>;
+		vcc5-supply = <&vcc4v0_sys>;
+		vcc6-supply = <&vcc4v0_sys>;
+		vcc7-supply = <&vcc4v0_sys>;
+		vcc8-supply = <&vcc4v0_sys>;
+		vcc9-supply = <&vcc4v0_sys>;
+		vcc10-supply = <&vcc4v0_sys>;
+		vcc11-supply = <&vcc_2v0_pldo_s3>;
+		vcc12-supply = <&vcc4v0_sys>;
+		vcc13-supply = <&vcc_1v1_nldo_s3>;
+		vcc14-supply = <&vcc_1v1_nldo_s3>;
+		vcca-supply = <&vcc4v0_sys>;
+
+		gpio-controller;
+		#gpio-cells = <2>;
+
+		rk806_dvs1_null: dvs1-null-pins {
+			pins = "gpio_pwrctrl1";
+			function = "pin_fun0";
+		};
+
+		rk806_dvs2_null: dvs2-null-pins {
+			pins = "gpio_pwrctrl2";
+			function = "pin_fun0";
+		};
+
+		rk806_dvs3_null: dvs3-null-pins {
+			pins = "gpio_pwrctrl3";
+			function = "pin_fun0";
+		};
+
+		regulators {
+			vdd_gpu_s0: vdd_gpu_mem_s0: dcdc-reg1 {
+				regulator-boot-on;
+				regulator-min-microvolt = <550000>;
+				regulator-max-microvolt = <950000>;
+				regulator-ramp-delay = <12500>;
+				regulator-name = "vdd_gpu_s0";
+				regulator-enable-ramp-delay = <400>;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vdd_cpu_lit_s0: vdd_cpu_lit_mem_s0: dcdc-reg2 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <550000>;
+				regulator-max-microvolt = <950000>;
+				regulator-ramp-delay = <12500>;
+				regulator-name = "vdd_cpu_lit_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vdd_log_s0: dcdc-reg3 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <675000>;
+				regulator-max-microvolt = <750000>;
+				regulator-ramp-delay = <12500>;
+				regulator-name = "vdd_log_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+					regulator-suspend-microvolt = <750000>;
+				};
+			};
+
+			vdd_vdenc_s0: vdd_vdenc_mem_s0: dcdc-reg4 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <550000>;
+				regulator-max-microvolt = <950000>;
+				regulator-init-microvolt = <750000>;
+				regulator-ramp-delay = <12500>;
+				regulator-name = "vdd_vdenc_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vdd_ddr_s0: dcdc-reg5 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <675000>;
+				regulator-max-microvolt = <900000>;
+				regulator-ramp-delay = <12500>;
+				regulator-name = "vdd_ddr_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+					regulator-suspend-microvolt = <850000>;
+				};
+			};
+
+			vdd2_ddr_s3: dcdc-reg6 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-name = "vdd2_ddr_s3";
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+				};
+			};
+
+			vcc_2v0_pldo_s3: dcdc-reg7 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <2000000>;
+				regulator-max-microvolt = <2000000>;
+				regulator-ramp-delay = <12500>;
+				regulator-name = "vdd_2v0_pldo_s3";
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <2000000>;
+				};
+			};
+
+			vcc_3v3_s3: dcdc-reg8 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc_3v3_s3";
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <3300000>;
+				};
+			};
+
+			vddq_ddr_s0: dcdc-reg9 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-name = "vddq_ddr_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcc_1v8_s3: dcdc-reg10 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-name = "vcc_1v8_s3";
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1800000>;
+				};
+			};
+
+			avcc_1v8_s0: pldo-reg1 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-name = "avcc_1v8_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcc_1v8_s0: pldo-reg2 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-name = "vcc_1v8_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+					regulator-suspend-microvolt = <1800000>;
+				};
+			};
+
+			avdd_1v2_s0: pldo-reg3 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1200000>;
+				regulator-max-microvolt = <1200000>;
+				regulator-name = "avdd_1v2_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcc_3v3_s0: pldo-reg4 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-ramp-delay = <12500>;
+				regulator-name = "vcc_3v3_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vccio_sd_s0: pldo-reg5 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-ramp-delay = <12500>;
+				regulator-name = "vccio_sd_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			pldo6_s3: pldo-reg6 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-name = "pldo6_s3";
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1800000>;
+				};
+			};
+
+			vdd_0v75_s3: nldo-reg1 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <750000>;
+				regulator-max-microvolt = <750000>;
+				regulator-name = "vdd_0v75_s3";
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <750000>;
+				};
+			};
+
+			vdd_ddr_pll_s0: nldo-reg2 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <850000>;
+				regulator-max-microvolt = <850000>;
+				regulator-name = "vdd_ddr_pll_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+					regulator-suspend-microvolt = <850000>;
+				};
+			};
+
+			avdd_0v75_s0: nldo-reg3 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <750000>;
+				regulator-max-microvolt = <750000>;
+				regulator-name = "avdd_0v75_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vdd_0v85_s0: nldo-reg4 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <850000>;
+				regulator-max-microvolt = <850000>;
+				regulator-name = "vdd_0v85_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vdd_0v75_s0: nldo-reg5 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <750000>;
+				regulator-max-microvolt = <750000>;
+				regulator-name = "vdd_0v75_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+		};
+	};
+};
+
+&tsadc {
+	status = "okay";
+};
+
+&uart2 {
+	pinctrl-0 = <&uart2m0_xfer>;
+	status = "okay";
+};
+
+&u2phy2_host {
+	phy-supply = <&vdd_4g_3v3>;
+	status = "okay";
+};
+
+&u2phy3_host {
+	status = "okay";
+};
+
+&u2phy2 {
+	status = "okay";
+};
+
+&u2phy3 {
+	status = "okay";
+};
+
+&usb_host0_ehci {
+	status = "okay";
+};
+
+&usb_host0_ohci {
+	status = "okay";
+};
+
+&usb_host1_ehci {
+	status = "okay";
+};
+
+&usb_host1_ohci {
+	status = "okay";
+};
