From a6bb7d4e4abbcefcd00e37835df1c4e64b2dc732 Mon Sep 17 00:00:00 2001
From: Lee Jackson <lee.jackson@arducam.com>
Date: Wed, 10 Jan 2024 08:52:54 +0800
Subject: [PATCH 0822/1085] drivers: media: imx519: Add V4L2_CID_LINK_FREQ
 control

Add V4L2_CID_LINK_FREQ as a read-only control with a value of 408 Mhz.
This will be used by the CFE driver to corretly setup the DPHY timing
parameters in the CSI-2 block.

Signed-off-by: Lee Jackson <lee.jackson@arducam.com>
---
 drivers/media/i2c/imx519.c | 14 ++++++++++++++
 1 file changed, 14 insertions(+)

--- a/drivers/media/i2c/imx519.c
+++ b/drivers/media/i2c/imx519.c
@@ -145,6 +145,10 @@ struct imx519_mode {
 	struct imx519_reg_list reg_list;
 };
 
+static const s64 imx519_link_freq_menu[] = {
+	IMX519_DEFAULT_LINK_FREQ,
+};
+
 static const struct imx519_reg mode_common_regs[] = {
 	{0x0100, 0x00},
 	{0x0136, 0x18},
@@ -1819,6 +1823,7 @@ static int imx519_init_controls(struct i
 	struct v4l2_ctrl_handler *ctrl_hdlr;
 	struct i2c_client *client = v4l2_get_subdevdata(&imx519->sd);
 	struct v4l2_fwnode_device_properties props;
+	struct v4l2_ctrl *link_freq;
 	unsigned int i;
 	int ret;
 
@@ -1837,6 +1842,15 @@ static int imx519_init_controls(struct i
 					       IMX519_PIXEL_RATE, 1,
 					       IMX519_PIXEL_RATE);
 
+	/* LINK_FREQ is also read only */
+	link_freq =
+		v4l2_ctrl_new_int_menu(ctrl_hdlr, &imx519_ctrl_ops,
+				       V4L2_CID_LINK_FREQ,
+				       ARRAY_SIZE(imx519_link_freq_menu) - 1, 0,
+				       imx519_link_freq_menu);
+	if (link_freq)
+		link_freq->flags |= V4L2_CTRL_FLAG_READ_ONLY;
+
 	/*
 	 * Create the controls here, but mode specific limits are setup
 	 * in the imx519_set_framing_limits() call below.
