// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/pinctrl/rockchip.h>
#include <dt-bindings/soc/rockchip,vop2.h>
#include "rk3568.dtsi"

/ {
	aliases {
		mmc0 = &sdmmc0;
		mmc1 = &sdhci;
	};

	chosen {
		stdout-path = "serial2:1500000n8";
	};

	hdmi-con {
		compatible = "hdmi-connector";
		type = "a";

		port {
			hdmi_con_in: endpoint {
				remote-endpoint = <&hdmi_out_con>;
			};
		};
	};

	dc_12v: dc-12v-regulator {
		compatible = "regulator-fixed";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <12000000>;
		regulator-max-microvolt = <12000000>;
		regulator-name = "dc_12v";
	};

	vcc3v3_sys: vcc3v3-sys-regulator {
		compatible = "regulator-fixed";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-name = "vcc3v3_sys";
		vin-supply = <&dc_12v>;
	};

	vcc5v0_sys: vcc5v0-sys-regulator {
		compatible = "regulator-fixed";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		regulator-name = "vcc5v0_sys";
		vin-supply = <&dc_12v>;
	};

	vcc5v0_usb_host: vcc5v0-usb-host-regulator {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio0 RK_PA5 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&vcc5v0_usb_host_en>;
		regulator-always-on;
		regulator-boot-on;
		regulator-name = "vcc5v0_usb_host";
	};

	vcc5v0_usb_otg: vcc5v0-usb-otg-regulator {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio0 RK_PA6 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&vcc5v0_usb_otg_en>;
		regulator-always-on;
		regulator-boot-on;
		regulator-name = "vcc5v0_usb_otg";
	};
};

&combphy0 {
	status = "okay";
};

&combphy1 {
	status = "okay";
};

&combphy2 {
	status = "okay";
};

&cpu0 {
	cpu-supply = <&vdd_cpu>;
};

&cpu1 {
	cpu-supply = <&vdd_cpu>;
};

&cpu2 {
	cpu-supply = <&vdd_cpu>;
};

&cpu3 {
	cpu-supply = <&vdd_cpu>;
};

&gpu {
	mali-supply = <&vdd_gpu>;
	status = "okay";
};

&hdmi {
	avdd-0v9-supply = <&vdda0v9_image>;
	avdd-1v8-supply = <&vcca1v8_image>;
	status = "okay";
};

&hdmi_in {
	hdmi_in_vp0: endpoint {
		remote-endpoint = <&vp0_out_hdmi>;
	};
};

&hdmi_out {
	hdmi_out_con: endpoint {
		remote-endpoint = <&hdmi_con_in>;
	};
};

&hdmi_sound {
	status = "okay";
};

&i2c0 {
	status = "okay";

	vdd_cpu: regulator@1c {
		compatible = "tcs,tcs4525";
		reg = <0x1c>;
		fcs,suspend-voltage-selector = <1>;
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <712500>;
		regulator-max-microvolt = <1390000>;
		regulator-name = "vdd_cpu";
		regulator-ramp-delay = <2300>;
		vin-supply = <&vcc5v0_sys>;

		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	rk809: pmic@20 {
		compatible = "rockchip,rk809";
		reg = <0x20>;
		interrupt-parent = <&gpio0>;
		interrupts = <RK_PA3 IRQ_TYPE_LEVEL_LOW>;
		#clock-cells = <1>;
		pinctrl-names = "default";
		pinctrl-0 = <&pmic_int>;
		rockchip,system-power-controller;
		wakeup-source;

		vcc1-supply = <&vcc3v3_sys>;
		vcc2-supply = <&vcc3v3_sys>;
		vcc3-supply = <&vcc3v3_sys>;
		vcc4-supply = <&vcc3v3_sys>;
		vcc5-supply = <&vcc3v3_sys>;
		vcc6-supply = <&vcc3v3_sys>;
		vcc7-supply = <&vcc3v3_sys>;
		vcc8-supply = <&vcc3v3_sys>;
		vcc9-supply = <&vcc3v3_sys>;

		regulators {
			vdd_logic: DCDC_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-init-microvolt = <900000>;
				regulator-initial-mode = <0x2>;
				regulator-min-microvolt = <500000>;
				regulator-max-microvolt = <1350000>;
				regulator-name = "vdd_logic";
				regulator-ramp-delay = <6001>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_gpu: DCDC_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-init-microvolt = <900000>;
				regulator-initial-mode = <0x2>;
				regulator-min-microvolt = <500000>;
				regulator-max-microvolt = <1350000>;
				regulator-name = "vdd_gpu";
				regulator-ramp-delay = <6001>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_ddr: DCDC_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-initial-mode = <0x2>;
				regulator-name = "vcc_ddr";

				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vdd_npu: DCDC_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-init-microvolt = <900000>;
				regulator-initial-mode = <0x2>;
				regulator-min-microvolt = <500000>;
				regulator-max-microvolt = <1350000>;
				regulator-name = "vdd_npu";
				regulator-ramp-delay = <6001>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_1v8: DCDC_REG5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc_1v8";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdda0v9_image: LDO_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <900000>;
				regulator-max-microvolt = <900000>;
				regulator-name = "vdda0v9_image";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdda_0v9: LDO_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <900000>;
				regulator-max-microvolt = <900000>;
				regulator-name = "vdda_0v9";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdda0v9_pmu: LDO_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <900000>;
				regulator-max-microvolt = <900000>;
				regulator-name = "vdda0v9_pmu";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <900000>;
				};
			};

			vccio_acodec: LDO_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vccio_acodec";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vccio_sd: LDO_REG5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vccio_sd";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc3v3_pmu: LDO_REG6 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc3v3_pmu";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcca_1v8: LDO_REG7 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcca_1v8";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcca1v8_pmu: LDO_REG8 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcca1v8_pmu";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcca1v8_image: LDO_REG9 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcca1v8_image";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_3v3: SWITCH_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc_3v3";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc3v3_sd: SWITCH_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc3v3_sd";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};
		};
	};
};

&i2s0_8ch {
	status = "okay";
};

&pinctrl {
	pmic {
		pmic_int: pmic_int {
			rockchip,pins = <0 RK_PA3 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};
};

&pmu_io_domains {
	pmuio1-supply = <&vcc3v3_pmu>;
	pmuio2-supply = <&vcc3v3_pmu>;
	vccio1-supply = <&vccio_acodec>;
	vccio2-supply = <&vcc_1v8>;
	vccio3-supply = <&vccio_sd>;
	vccio4-supply = <&vcc_1v8>;
	vccio5-supply = <&vcc_3v3>;
	vccio6-supply = <&vcc_1v8>;
	vccio7-supply = <&vcc_3v3>;
	status = "okay";
};

&saradc {
	vref-supply = <&vcca_1v8>;
	status = "okay";
};

&sdhci {
	bus-width = <8>;
	max-frequency = <200000000>;
	non-removable;
	pinctrl-names = "default";
	pinctrl-0 = <&emmc_bus8 &emmc_clk &emmc_cmd &emmc_datastrobe>;
	status = "okay";
};

&sdmmc0 {
	bus-width = <4>;
	cap-sd-highspeed;
	cd-gpios = <&gpio0 RK_PA4 GPIO_ACTIVE_LOW>;
	disable-wp;
	pinctrl-names = "default";
	pinctrl-0 = <&sdmmc0_bus4 &sdmmc0_clk &sdmmc0_cmd &sdmmc0_det>;
	sd-uhs-sdr104;
	vmmc-supply = <&vcc3v3_sd>;
	vqmmc-supply = <&vccio_sd>;
	status = "okay";
};

&tsadc {
	rockchip,hw-tshut-mode = <1>;
	rockchip,hw-tshut-polarity = <0>;
	status = "okay";
};

&uart2 {
	status = "okay";
};

&usb_host0_ehci {
	status = "okay";
};

&usb_host0_ohci {
	status = "okay";
};

&usb_host0_xhci {
	dr_mode = "host";
	status = "okay";
};

&usb_host1_ehci {
	status = "okay";
};

&usb_host1_ohci {
	status = "okay";
};

&usb_host1_xhci {
	status = "okay";
};

&usb2phy0 {
	status = "okay";
};

&usb2phy0_host {
	phy-supply = <&vcc5v0_usb_host>;
	status = "okay";
};

&usb2phy0_otg {
	phy-supply = <&vcc5v0_usb_otg>;
	status = "okay";
};

&usb2phy1 {
	status = "okay";
};

&usb2phy1_host {
	phy-supply = <&vcc5v0_usb_host>;
	status = "okay";
};

&usb2phy1_otg {
	phy-supply = <&vcc5v0_usb_host>;
	status = "okay";
};

&vop {
	assigned-clocks = <&cru DCLK_VOP0>, <&cru DCLK_VOP1>;
	assigned-clock-parents = <&pmucru PLL_HPLL>, <&cru PLL_VPLL>;
	status = "okay";
};

&vop_mmu {
	status = "okay";
};

&vp0 {
	vp0_out_hdmi: endpoint@ROCKCHIP_VOP2_EP_HDMI0 {
		reg = <ROCKCHIP_VOP2_EP_HDMI0>;
		remote-endpoint = <&hdmi_in_vp0>;
	};
};
