// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "glinet,gl-mt1300", "mediatek,mt7621-soc";
	model = "GL.iNet GL-MT1300";

	aliases {
		led-boot = &led_run;
		led-failsafe = &led_run;
		led-running = &led_run;
		led-upgrade = &led_run;
		label-mac-device = &gmac1;
	};

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		switch {
			label = "switch";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
			linux,input-type = <EV_SW>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_run: run {
			label = "blue:run";
			gpios = <&gpio 14 GPIO_ACTIVE_HIGH>;
		};

		system {
			label = "white:system";
			gpios = <&gpio 13 GPIO_ACTIVE_HIGH>;
		};
	};
};

&i2c {
	status = "okay";
};

&sdhci {
	status = "okay";
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <50000000>;
		broken-flash-reset;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					eeprom_factory_0: eeprom@0 {
						reg = <0x0 0x4da8>;
					};

					macaddr_factory_4000: macaddr@4000 {
						compatible = "mac-base";
						reg = <0x4000 0x6>;
						#nvmem-cell-cells = <1>;
					};
				};
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0x1fb0000>;
			};
		};
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&eeprom_factory_0>;
		nvmem-cell-names = "eeprom";
	};
};

&gmac0 {
	nvmem-cells = <&macaddr_factory_4000 1>;
	nvmem-cell-names = "mac-address";
};

&gmac1 {
	status = "okay";
	label = "wan";
	phy-handle = <&ethphy4>;

	nvmem-cells = <&macaddr_factory_4000 0>;
	nvmem-cell-names = "mac-address";
};

&ethphy4 {
	/delete-property/ interrupts;
};

&switch0 {
	ports {
		port@2 {
			status = "okay";
			label = "lan1";
		};

		port@3 {
			status = "okay";
			label = "lan2";
		};
	};
};

&uartlite3 {
	status = "okay";
};

&state_default {
	gpio {
		group = "wdt", "jtag";
		function = "gpio";
	};
};
