From 594356bf1518872a1dcc077d0342c88c93f14b57 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.com>
Date: Mon, 27 Nov 2023 12:16:04 +0000
Subject: [PATCH 0750/1085] ASoC: dwc: Permit sample rates up to 384kHz

The BCM2835 I2S block advertises clock rates up to 384kHz, and there's
no reason why RP1's DWC I2S block shouldn't do the same.

See: https://github.com/raspberrypi/linux/issues/5748

Signed-off-by: Phil Elwell <phil@raspberrypi.com>
---
 sound/soc/dwc/dwc-i2s.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/sound/soc/dwc/dwc-i2s.c
+++ b/sound/soc/dwc/dwc-i2s.c
@@ -796,7 +796,7 @@ static int dw_configure_dai_by_dt(struct
 	u32 idx2;
 	int ret;
 
-	ret = dw_configure_dai(dev, dw_i2s_dai, SNDRV_PCM_RATE_8000_192000);
+	ret = dw_configure_dai(dev, dw_i2s_dai, SNDRV_PCM_RATE_8000_384000);
 	if (ret < 0)
 		return ret;
 
