// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

/dts-v1/;

#include "ipq6018.dtsi"
#include "ipq6018-cp-cpu.dtsi"
#include "ipq6018-ess.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	model = "TP-Link EAP610-Outdoor";
	compatible = "tplink,eap610-outdoor", "qcom,ipq6018";

	aliases {
		serial0 = &blsp1_uart3;
		led-boot = &led_sys_green;
		led-failsafe = &led_sys_amber;
		led-running = &led_sys_green;
		led-upgrade = &led_sys_amber;
	};

	chosen {
		stdout-path = "serial0:115200n8";
		bootargs-append = " ubi.block=0,rootfs root=/dev/ubiblock0_1";
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&tlmm 9 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_sys_amber: led-0 {
			function = "system";
			color = <LED_COLOR_ID_AMBER>;
			gpios = <&tlmm 35 GPIO_ACTIVE_HIGH>;
		};

		led_sys_green: led-1 {
			function = "system";
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&tlmm 37 GPIO_ACTIVE_HIGH>;
		};
	};

	gpio-restart {
		compatible = "gpio-restart";
		gpios = <&tlmm 61 GPIO_ACTIVE_LOW>;
		open-source;
	};
};

&blsp1_uart3 {
	pinctrl-0 = <&serial_3_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&tlmm {
	mdio_pins: mdio-pins {
		mdc {
			pins = "gpio64";
			function = "mdc";
			drive-strength = <8>;
			bias-pull-up;
		};

		mdio {
			pins = "gpio65";
			function = "mdio";
			drive-strength = <8>;
			bias-pull-up;
		};
	};

	led_enable {
		gpio-hog;
		output-high;
		gpios = <36 GPIO_ACTIVE_HIGH>;
		line-name = "enable-leds";
	};
};

&dp5 {
	phy-handle = <&rtl8211f_4>;
	phy-mode = "sgmii";
	label = "lan";
	status = "okay";
};

&edma {
	status = "okay";
};

&mdio {
	pinctrl-0 = <&mdio_pins>;
	pinctrl-names = "default";
	reset-gpios = <&tlmm 77 GPIO_ACTIVE_LOW>;
	reset-delay-us = <10000>;
	reset-post-delay-us = <50000>;
	status = "okay";

	rtl8211f_4: ethernet-phy@4 {
		reg = <4>;
	};
};

&switch {
	switch_lan_bmp = <ESS_PORT5>;
	switch_mac_mode1 = <MAC_MODE_SGMII_CHANNEL0>;
	status = "okay";

	qcom,port_phyinfo {
		port@4 {
			port_id = <5>;
			phy_address = <4>;
		};
	};
};

&qpic_bam {
	status = "okay";
};

&qpic_nand {
	status = "okay";

	nand@0 {
		reg = <0>;

		nand-ecc-strength = <4>;
		nand-ecc-step-size = <512>;
		nand-bus-width = <8>;
	};
};

&wifi {
	ieee80211-freq-limit = <2402000 5835000>;
	qcom,ath11k-calibration-variant = "TP-Link-EAP610-Outdoor";
	status = "okay";
};
