From 81a8e9e192d53ce8b5cafd47190d6c6826519d09 Mon Sep 17 00:00:00 2001
From: Daniel Schwierzeck <daniel.schwierzeck@gmail.com>
Date: Wed, 7 Nov 2012 14:58:59 +0100
Subject: sf: spansion: fix device IDs and sector architecture for S25FL256S

Signed-off-by: Daniel Schwierzeck <daniel.schwierzeck@gmail.com>

--- a/drivers/mtd/spi/spansion.c
+++ b/drivers/mtd/spi/spansion.c
@@ -97,11 +97,18 @@ static const struct spansion_spi_flash_p
 		.name = "S25FL129P_64K",
 	},
 	{
-		.idcode1 = 0x2019,
+		.idcode1 = 0x0219,
 		.idcode2 = 0x4d01,
 		.pages_per_sector = 256,
 		.nr_sectors = 512,
-		.name = "S25FL256S",
+		.name = "S25FL256S_64K",
+	},
+	{
+		.idcode1 = 0x0219,
+		.idcode2 = 0x4d00,
+		.pages_per_sector = 1024,
+		.nr_sectors = 128,
+		.name = "S25FL256S_256K",
 	},
 };
 
