From: Felix Fietkau <nbd@nbd.name>
Date: Sat, 26 Dec 2020 14:23:47 +0100
Subject: [PATCH] mac80211: remove legacy minstrel rate control

Now that minstrel_ht supports legacy rates, it is no longer needed

Signed-off-by: Felix Fietkau <nbd@nbd.name>
---
 delete mode 100644 net/mac80211/rc80211_minstrel.c
 delete mode 100644 net/mac80211/rc80211_minstrel.h
 delete mode 100644 net/mac80211/rc80211_minstrel_debugfs.c

--- a/net/mac80211/Makefile
+++ b/net/mac80211/Makefile
@@ -55,11 +55,9 @@ mac80211-$(CONFIG_PM) += pm.o
 CFLAGS_trace.o := -I$(src)
 
 rc80211_minstrel-y := \
-	rc80211_minstrel.o \
 	rc80211_minstrel_ht.o
 
 rc80211_minstrel-$(CPTCFG_MAC80211_DEBUGFS) += \
-	rc80211_minstrel_debugfs.o \
 	rc80211_minstrel_ht_debugfs.o
 
 mac80211-$(CPTCFG_MAC80211_RC_MINSTREL) += $(rc80211_minstrel-y)
--- a/net/mac80211/rc80211_minstrel.c
+++ /dev/null
@@ -1,574 +0,0 @@
-/*
- * Copyright (C) 2008 Felix Fietkau <nbd@openwrt.org>
- *
- * This program is free software; you can redistribute it and/or modify
- * it under the terms of the GNU General Public License version 2 as
- * published by the Free Software Foundation.
- *
- * Based on minstrel.c:
- *   Copyright (C) 2005-2007 Derek Smithies <derek@indranet.co.nz>
- *   Sponsored by Indranet Technologies Ltd
- *
- * Based on sample.c:
- *   Copyright (c) 2005 John Bicket
- *   All rights reserved.
- *
- *   Redistribution and use in source and binary forms, with or without
- *   modification, are permitted provided that the following conditions
- *   are met:
- *   1. Redistributions of source code must retain the above copyright
- *      notice, this list of conditions and the following disclaimer,
- *      without modification.
- *   2. Redistributions in binary form must reproduce at minimum a disclaimer
- *      similar to the "NO WARRANTY" disclaimer below ("Disclaimer") and any
- *      redistribution must be conditioned upon including a substantially
- *      similar Disclaimer requirement for further binary redistribution.
- *   3. Neither the names of the above-listed copyright holders nor the names
- *      of any contributors may be used to endorse or promote products derived
- *      from this software without specific prior written permission.
- *
- *   Alternatively, this software may be distributed under the terms of the
- *   GNU General Public License ("GPL") version 2 as published by the Free
- *   Software Foundation.
- *
- *   NO WARRANTY
- *   THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
- *   ``AS IS'' AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
- *   LIMITED TO, THE IMPLIED WARRANTIES OF NONINFRINGEMENT, MERCHANTIBILITY
- *   AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL
- *   THE COPYRIGHT HOLDERS OR CONTRIBUTORS BE LIABLE FOR SPECIAL, EXEMPLARY,
- *   OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
- *   SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
- *   INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER
- *   IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
- *   ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF
- *   THE POSSIBILITY OF SUCH DAMAGES.
- */
-#include <linux/netdevice.h>
-#include <linux/types.h>
-#include <linux/skbuff.h>
-#include <linux/debugfs.h>
-#include <linux/random.h>
-#include <linux/ieee80211.h>
-#include <linux/slab.h>
-#include <net/mac80211.h>
-#include "rate.h"
-#include "rc80211_minstrel.h"
-
-#define SAMPLE_TBL(_mi, _idx, _col) \
-		_mi->sample_table[(_idx * SAMPLE_COLUMNS) + _col]
-
-/* convert mac80211 rate index to local array index */
-static inline int
-rix_to_ndx(struct minstrel_sta_info *mi, int rix)
-{
-	int i = rix;
-	for (i = rix; i >= 0; i--)
-		if (mi->r[i].rix == rix)
-			break;
-	return i;
-}
-
-/* return current EMWA throughput */
-int minstrel_get_tp_avg(struct minstrel_rate *mr, int prob_avg)
-{
-	int usecs;
-
-	usecs = mr->perfect_tx_time;
-	if (!usecs)
-		usecs = 1000000;
-
-	/* reset thr. below 10% success */
-	if (mr->stats.prob_avg < MINSTREL_FRAC(10, 100))
-		return 0;
-
-	if (prob_avg > MINSTREL_FRAC(90, 100))
-		return MINSTREL_TRUNC(100000 * (MINSTREL_FRAC(90, 100) / usecs));
-	else
-		return MINSTREL_TRUNC(100000 * (prob_avg / usecs));
-}
-
-/* find & sort topmost throughput rates */
-static inline void
-minstrel_sort_best_tp_rates(struct minstrel_sta_info *mi, int i, u8 *tp_list)
-{
-	int j;
-	struct minstrel_rate_stats *tmp_mrs;
-	struct minstrel_rate_stats *cur_mrs = &mi->r[i].stats;
-
-	for (j = MAX_THR_RATES; j > 0; --j) {
-		tmp_mrs = &mi->r[tp_list[j - 1]].stats;
-		if (minstrel_get_tp_avg(&mi->r[i], cur_mrs->prob_avg) <=
-		    minstrel_get_tp_avg(&mi->r[tp_list[j - 1]], tmp_mrs->prob_avg))
-			break;
-	}
-
-	if (j < MAX_THR_RATES - 1)
-		memmove(&tp_list[j + 1], &tp_list[j], MAX_THR_RATES - (j + 1));
-	if (j < MAX_THR_RATES)
-		tp_list[j] = i;
-}
-
-static void
-minstrel_set_rate(struct minstrel_sta_info *mi, struct ieee80211_sta_rates *ratetbl,
-		  int offset, int idx)
-{
-	struct minstrel_rate *r = &mi->r[idx];
-
-	ratetbl->rate[offset].idx = r->rix;
-	ratetbl->rate[offset].count = r->adjusted_retry_count;
-	ratetbl->rate[offset].count_cts = r->retry_count_cts;
-	ratetbl->rate[offset].count_rts = r->stats.retry_count_rtscts;
-}
-
-static void
-minstrel_update_rates(struct minstrel_priv *mp, struct minstrel_sta_info *mi)
-{
-	struct ieee80211_sta_rates *ratetbl;
-	int i = 0;
-
-	ratetbl = kzalloc(sizeof(*ratetbl), GFP_ATOMIC);
-	if (!ratetbl)
-		return;
-
-	/* Start with max_tp_rate */
-	minstrel_set_rate(mi, ratetbl, i++, mi->max_tp_rate[0]);
-
-	if (mp->hw->max_rates >= 3) {
-		/* At least 3 tx rates supported, use max_tp_rate2 next */
-		minstrel_set_rate(mi, ratetbl, i++, mi->max_tp_rate[1]);
-	}
-
-	if (mp->hw->max_rates >= 2) {
-		/* At least 2 tx rates supported, use max_prob_rate next */
-		minstrel_set_rate(mi, ratetbl, i++, mi->max_prob_rate);
-	}
-
-	/* Use lowest rate last */
-	ratetbl->rate[i].idx = mi->lowest_rix;
-	ratetbl->rate[i].count = mp->max_retry;
-	ratetbl->rate[i].count_cts = mp->max_retry;
-	ratetbl->rate[i].count_rts = mp->max_retry;
-
-	rate_control_set_rates(mp->hw, mi->sta, ratetbl);
-}
-
-/*
-* Recalculate statistics and counters of a given rate
-*/
-void
-minstrel_calc_rate_stats(struct minstrel_priv *mp,
-			 struct minstrel_rate_stats *mrs)
-{
-	unsigned int cur_prob;
-
-	if (unlikely(mrs->attempts > 0)) {
-		mrs->sample_skipped = 0;
-		cur_prob = MINSTREL_FRAC(mrs->success, mrs->attempts);
-		if (mp->new_avg) {
-			minstrel_filter_avg_add(&mrs->prob_avg,
-						&mrs->prob_avg_1, cur_prob);
-		} else if (unlikely(!mrs->att_hist)) {
-			mrs->prob_avg = cur_prob;
-		} else {
-			/*update exponential weighted moving avarage */
-			mrs->prob_avg = minstrel_ewma(mrs->prob_avg,
-						      cur_prob,
-						      EWMA_LEVEL);
-		}
-		mrs->att_hist += mrs->attempts;
-		mrs->succ_hist += mrs->success;
-	} else {
-		mrs->sample_skipped++;
-	}
-
-	mrs->last_success = mrs->success;
-	mrs->last_attempts = mrs->attempts;
-	mrs->success = 0;
-	mrs->attempts = 0;
-}
-
-static void
-minstrel_update_stats(struct minstrel_priv *mp, struct minstrel_sta_info *mi)
-{
-	u8 tmp_tp_rate[MAX_THR_RATES];
-	u8 tmp_prob_rate = 0;
-	int i, tmp_cur_tp, tmp_prob_tp;
-
-	for (i = 0; i < MAX_THR_RATES; i++)
-	    tmp_tp_rate[i] = 0;
-
-	for (i = 0; i < mi->n_rates; i++) {
-		struct minstrel_rate *mr = &mi->r[i];
-		struct minstrel_rate_stats *mrs = &mi->r[i].stats;
-		struct minstrel_rate_stats *tmp_mrs = &mi->r[tmp_prob_rate].stats;
-
-		/* Update statistics of success probability per rate */
-		minstrel_calc_rate_stats(mp, mrs);
-
-		/* Sample less often below the 10% chance of success.
-		 * Sample less often above the 95% chance of success. */
-		if (mrs->prob_avg > MINSTREL_FRAC(95, 100) ||
-		    mrs->prob_avg < MINSTREL_FRAC(10, 100)) {
-			mr->adjusted_retry_count = mrs->retry_count >> 1;
-			if (mr->adjusted_retry_count > 2)
-				mr->adjusted_retry_count = 2;
-			mr->sample_limit = 4;
-		} else {
-			mr->sample_limit = -1;
-			mr->adjusted_retry_count = mrs->retry_count;
-		}
-		if (!mr->adjusted_retry_count)
-			mr->adjusted_retry_count = 2;
-
-		minstrel_sort_best_tp_rates(mi, i, tmp_tp_rate);
-
-		/* To determine the most robust rate (max_prob_rate) used at
-		 * 3rd mmr stage we distinct between two cases:
-		 * (1) if any success probabilitiy >= 95%, out of those rates
-		 * choose the maximum throughput rate as max_prob_rate
-		 * (2) if all success probabilities < 95%, the rate with
-		 * highest success probability is chosen as max_prob_rate */
-		if (mrs->prob_avg >= MINSTREL_FRAC(95, 100)) {
-			tmp_cur_tp = minstrel_get_tp_avg(mr, mrs->prob_avg);
-			tmp_prob_tp = minstrel_get_tp_avg(&mi->r[tmp_prob_rate],
-							  tmp_mrs->prob_avg);
-			if (tmp_cur_tp >= tmp_prob_tp)
-				tmp_prob_rate = i;
-		} else {
-			if (mrs->prob_avg >= tmp_mrs->prob_avg)
-				tmp_prob_rate = i;
-		}
-	}
-
-	/* Assign the new rate set */
-	memcpy(mi->max_tp_rate, tmp_tp_rate, sizeof(mi->max_tp_rate));
-	mi->max_prob_rate = tmp_prob_rate;
-
-#ifdef CPTCFG_MAC80211_DEBUGFS
-	/* use fixed index if set */
-	if (mp->fixed_rate_idx != -1) {
-		mi->max_tp_rate[0] = mp->fixed_rate_idx;
-		mi->max_tp_rate[1] = mp->fixed_rate_idx;
-		mi->max_prob_rate = mp->fixed_rate_idx;
-	}
-#endif
-
-	/* Reset update timer */
-	mi->last_stats_update = jiffies;
-
-	minstrel_update_rates(mp, mi);
-}
-
-static void
-minstrel_tx_status(void *priv, struct ieee80211_supported_band *sband,
-		   void *priv_sta, struct ieee80211_tx_status *st)
-{
-	struct ieee80211_tx_info *info = st->info;
-	struct minstrel_priv *mp = priv;
-	struct minstrel_sta_info *mi = priv_sta;
-	struct ieee80211_tx_rate *ar = info->status.rates;
-	int i, ndx;
-	int success;
-
-	success = !!(info->flags & IEEE80211_TX_STAT_ACK);
-
-	for (i = 0; i < IEEE80211_TX_MAX_RATES; i++) {
-		if (ar[i].idx < 0 || !ar[i].count)
-			break;
-
-		ndx = rix_to_ndx(mi, ar[i].idx);
-		if (ndx < 0)
-			continue;
-
-		mi->r[ndx].stats.attempts += ar[i].count;
-
-		if ((i != IEEE80211_TX_MAX_RATES - 1) && (ar[i + 1].idx < 0))
-			mi->r[ndx].stats.success += success;
-	}
-
-	if (time_after(jiffies, mi->last_stats_update +
-				mp->update_interval / (mp->new_avg ? 2 : 1)))
-		minstrel_update_stats(mp, mi);
-}
-
-
-static inline unsigned int
-minstrel_get_retry_count(struct minstrel_rate *mr,
-			 struct ieee80211_tx_info *info)
-{
-	u8 retry = mr->adjusted_retry_count;
-
-	if (info->control.use_rts)
-		retry = max_t(u8, 2, min(mr->stats.retry_count_rtscts, retry));
-	else if (info->control.use_cts_prot)
-		retry = max_t(u8, 2, min(mr->retry_count_cts, retry));
-	return retry;
-}
-
-
-static int
-minstrel_get_next_sample(struct minstrel_sta_info *mi)
-{
-	unsigned int sample_ndx;
-	sample_ndx = SAMPLE_TBL(mi, mi->sample_row, mi->sample_column);
-	mi->sample_row++;
-	if ((int) mi->sample_row >= mi->n_rates) {
-		mi->sample_row = 0;
-		mi->sample_column++;
-		if (mi->sample_column >= SAMPLE_COLUMNS)
-			mi->sample_column = 0;
-	}
-	return sample_ndx;
-}
-
-static void
-minstrel_get_rate(void *priv, struct ieee80211_sta *sta,
-		  void *priv_sta, struct ieee80211_tx_rate_control *txrc)
-{
-	struct sk_buff *skb = txrc->skb;
-	struct ieee80211_tx_info *info = IEEE80211_SKB_CB(skb);
-	struct minstrel_sta_info *mi = priv_sta;
-	struct minstrel_priv *mp = priv;
-	struct ieee80211_tx_rate *rate = &info->control.rates[0];
-	struct minstrel_rate *msr, *mr;
-	unsigned int ndx;
-	bool mrr_capable;
-	bool prev_sample;
-	int delta;
-	int sampling_ratio;
-
-	/* check multi-rate-retry capabilities & adjust lookaround_rate */
-	mrr_capable = mp->has_mrr &&
-		      !txrc->rts &&
-		      !txrc->bss_conf->use_cts_prot;
-	if (mrr_capable)
-		sampling_ratio = mp->lookaround_rate_mrr;
-	else
-		sampling_ratio = mp->lookaround_rate;
-
-	/* increase sum packet counter */
-	mi->total_packets++;
-
-#ifdef CPTCFG_MAC80211_DEBUGFS
-	if (mp->fixed_rate_idx != -1)
-		return;
-#endif
-
-	/* Don't use EAPOL frames for sampling on non-mrr hw */
-	if (mp->hw->max_rates == 1 &&
-	    (info->control.flags & IEEE80211_TX_CTRL_PORT_CTRL_PROTO))
-		return;
-
-	delta = (mi->total_packets * sampling_ratio / 100) -
-			mi->sample_packets;
-
-	/* delta < 0: no sampling required */
-	prev_sample = mi->prev_sample;
-	mi->prev_sample = false;
-	if (delta < 0 || (!mrr_capable && prev_sample))
-		return;
-
-	if (mi->total_packets >= 10000) {
-		mi->sample_packets = 0;
-		mi->total_packets = 0;
-	} else if (delta > mi->n_rates * 2) {
-		/* With multi-rate retry, not every planned sample
-		 * attempt actually gets used, due to the way the retry
-		 * chain is set up - [max_tp,sample,prob,lowest] for
-		 * sample_rate < max_tp.
-		 *
-		 * If there's too much sampling backlog and the link
-		 * starts getting worse, minstrel would start bursting
-		 * out lots of sampling frames, which would result
-		 * in a large throughput loss. */
-		mi->sample_packets += (delta - mi->n_rates * 2);
-	}
-
-	/* get next random rate sample */
-	ndx = minstrel_get_next_sample(mi);
-	msr = &mi->r[ndx];
-	mr = &mi->r[mi->max_tp_rate[0]];
-
-	/* Decide if direct ( 1st mrr stage) or indirect (2nd mrr stage)
-	 * rate sampling method should be used.
-	 * Respect such rates that are not sampled for 20 interations.
-	 */
-	if (msr->perfect_tx_time < mr->perfect_tx_time ||
-	    msr->stats.sample_skipped >= 20) {
-		if (!msr->sample_limit)
-			return;
-
-		mi->sample_packets++;
-		if (msr->sample_limit > 0)
-			msr->sample_limit--;
-	}
-
-	/* If we're not using MRR and the sampling rate already
-	 * has a probability of >95%, we shouldn't be attempting
-	 * to use it, as this only wastes precious airtime */
-	if (!mrr_capable &&
-	   (mi->r[ndx].stats.prob_avg > MINSTREL_FRAC(95, 100)))
-		return;
-
-	mi->prev_sample = true;
-
-	rate->idx = mi->r[ndx].rix;
-	rate->count = minstrel_get_retry_count(&mi->r[ndx], info);
-	info->flags |= IEEE80211_TX_CTL_RATE_CTRL_PROBE;
-}
-
-
-static void
-calc_rate_durations(enum nl80211_band band,
-		    struct minstrel_rate *d,
-		    struct ieee80211_rate *rate,
-		    struct cfg80211_chan_def *chandef)
-{
-	int erp = !!(rate->flags & IEEE80211_RATE_ERP_G);
-	int shift = ieee80211_chandef_get_shift(chandef);
-
-	d->perfect_tx_time = ieee80211_frame_duration(band, 1200,
-			DIV_ROUND_UP(rate->bitrate, 1 << shift), erp, 1,
-			shift);
-	d->ack_time = ieee80211_frame_duration(band, 10,
-			DIV_ROUND_UP(rate->bitrate, 1 << shift), erp, 1,
-			shift);
-}
-
-static void
-init_sample_table(struct minstrel_sta_info *mi)
-{
-	unsigned int i, col, new_idx;
-	u8 rnd[8];
-
-	mi->sample_column = 0;
-	mi->sample_row = 0;
-	memset(mi->sample_table, 0xff, SAMPLE_COLUMNS * mi->n_rates);
-
-	for (col = 0; col < SAMPLE_COLUMNS; col++) {
-		prandom_bytes(rnd, sizeof(rnd));
-		for (i = 0; i < mi->n_rates; i++) {
-			new_idx = (i + rnd[i & 7]) % mi->n_rates;
-			while (SAMPLE_TBL(mi, new_idx, col) != 0xff)
-				new_idx = (new_idx + 1) % mi->n_rates;
-
-			SAMPLE_TBL(mi, new_idx, col) = i;
-		}
-	}
-}
-
-static void
-minstrel_rate_init(void *priv, struct ieee80211_supported_band *sband,
-		   struct cfg80211_chan_def *chandef,
-		   struct ieee80211_sta *sta, void *priv_sta)
-{
-	struct minstrel_sta_info *mi = priv_sta;
-	struct minstrel_priv *mp = priv;
-	struct ieee80211_rate *ctl_rate;
-	unsigned int i, n = 0;
-	unsigned int t_slot = 9; /* FIXME: get real slot time */
-	u32 rate_flags;
-
-	mi->sta = sta;
-	mi->lowest_rix = rate_lowest_index(sband, sta);
-	ctl_rate = &sband->bitrates[mi->lowest_rix];
-	mi->sp_ack_dur = ieee80211_frame_duration(sband->band, 10,
-				ctl_rate->bitrate,
-				!!(ctl_rate->flags & IEEE80211_RATE_ERP_G), 1,
-				ieee80211_chandef_get_shift(chandef));
-
-	rate_flags = ieee80211_chandef_rate_flags(&mp->hw->conf.chandef);
-	memset(mi->max_tp_rate, 0, sizeof(mi->max_tp_rate));
-	mi->max_prob_rate = 0;
-
-	for (i = 0; i < sband->n_bitrates; i++) {
-		struct minstrel_rate *mr = &mi->r[n];
-		struct minstrel_rate_stats *mrs = &mi->r[n].stats;
-		unsigned int tx_time = 0, tx_time_cts = 0, tx_time_rtscts = 0;
-		unsigned int tx_time_single;
-		unsigned int cw = mp->cw_min;
-		int shift;
-
-		if (!rate_supported(sta, sband->band, i))
-			continue;
-		if ((rate_flags & sband->bitrates[i].flags) != rate_flags)
-			continue;
-
-		n++;
-		memset(mr, 0, sizeof(*mr));
-		memset(mrs, 0, sizeof(*mrs));
-
-		mr->rix = i;
-		shift = ieee80211_chandef_get_shift(chandef);
-		mr->bitrate = DIV_ROUND_UP(sband->bitrates[i].bitrate,
-					   (1 << shift) * 5);
-		calc_rate_durations(sband->band, mr, &sband->bitrates[i],
-				    chandef);
-
-		/* calculate maximum number of retransmissions before
-		 * fallback (based on maximum segment size) */
-		mr->sample_limit = -1;
-		mrs->retry_count = 1;
-		mr->retry_count_cts = 1;
-		mrs->retry_count_rtscts = 1;
-		tx_time = mr->perfect_tx_time + mi->sp_ack_dur;
-		do {
-			/* add one retransmission */
-			tx_time_single = mr->ack_time + mr->perfect_tx_time;
-
-			/* contention window */
-			tx_time_single += (t_slot * cw) >> 1;
-			cw = min((cw << 1) | 1, mp->cw_max);
-
-			tx_time += tx_time_single;
-			tx_time_cts += tx_time_single + mi->sp_ack_dur;
-			tx_time_rtscts += tx_time_single + 2 * mi->sp_ack_dur;
-			if ((tx_time_cts < mp->segment_size) &&
-				(mr->retry_count_cts < mp->max_retry))
-				mr->retry_count_cts++;
-			if ((tx_time_rtscts < mp->segment_size) &&
-				(mrs->retry_count_rtscts < mp->max_retry))
-				mrs->retry_count_rtscts++;
-		} while ((tx_time < mp->segment_size) &&
-				(++mr->stats.retry_count < mp->max_retry));
-		mr->adjusted_retry_count = mrs->retry_count;
-		if (!(sband->bitrates[i].flags & IEEE80211_RATE_ERP_G))
-			mr->retry_count_cts = mrs->retry_count;
-	}
-
-	for (i = n; i < sband->n_bitrates; i++) {
-		struct minstrel_rate *mr = &mi->r[i];
-		mr->rix = -1;
-	}
-
-	mi->n_rates = n;
-	mi->last_stats_update = jiffies;
-
-	init_sample_table(mi);
-	minstrel_update_rates(mp, mi);
-}
-
-static u32 minstrel_get_expected_throughput(void *priv_sta)
-{
-	struct minstrel_sta_info *mi = priv_sta;
-	struct minstrel_rate_stats *tmp_mrs;
-	int idx = mi->max_tp_rate[0];
-	int tmp_cur_tp;
-
-	/* convert pkt per sec in kbps (1200 is the average pkt size used for
-	 * computing cur_tp
-	 */
-	tmp_mrs = &mi->r[idx].stats;
-	tmp_cur_tp = minstrel_get_tp_avg(&mi->r[idx], tmp_mrs->prob_avg) * 10;
-	tmp_cur_tp = tmp_cur_tp * 1200 * 8 / 1024;
-
-	return tmp_cur_tp;
-}
-
-const struct rate_control_ops mac80211_minstrel = {
-	.tx_status_ext = minstrel_tx_status,
-	.get_rate = minstrel_get_rate,
-	.rate_init = minstrel_rate_init,
-	.get_expected_throughput = minstrel_get_expected_throughput,
-};
--- a/net/mac80211/rc80211_minstrel.h
+++ /dev/null
@@ -1,185 +0,0 @@
-/* SPDX-License-Identifier: GPL-2.0-only */
-/*
- * Copyright (C) 2008 Felix Fietkau <nbd@openwrt.org>
- */
-
-#ifndef __RC_MINSTREL_H
-#define __RC_MINSTREL_H
-
-#define EWMA_LEVEL	96	/* ewma weighting factor [/EWMA_DIV] */
-#define EWMA_DIV	128
-#define SAMPLE_COLUMNS	10	/* number of columns in sample table */
-
-/* scaled fraction values */
-#define MINSTREL_SCALE  12
-#define MINSTREL_FRAC(val, div) (((val) << MINSTREL_SCALE) / div)
-#define MINSTREL_TRUNC(val) ((val) >> MINSTREL_SCALE)
-
-/* number of highest throughput rates to consider*/
-#define MAX_THR_RATES 4
-
-/*
- * Coefficients for moving average with noise filter (period=16),
- * scaled by 10 bits
- *
- * a1 = exp(-pi * sqrt(2) / period)
- * coeff2 = 2 * a1 * cos(sqrt(2) * 2 * pi / period)
- * coeff3 = -sqr(a1)
- * coeff1 = 1 - coeff2 - coeff3
- */
-#define MINSTREL_AVG_COEFF1		(MINSTREL_FRAC(1, 1) - \
-					 MINSTREL_AVG_COEFF2 - \
-					 MINSTREL_AVG_COEFF3)
-#define MINSTREL_AVG_COEFF2		0x00001499
-#define MINSTREL_AVG_COEFF3		-0x0000092e
-
-/*
- * Perform EWMA (Exponentially Weighted Moving Average) calculation
- */
-static inline int
-minstrel_ewma(int old, int new, int weight)
-{
-	int diff, incr;
-
-	diff = new - old;
-	incr = (EWMA_DIV - weight) * diff / EWMA_DIV;
-
-	return old + incr;
-}
-
-static inline int minstrel_filter_avg_add(u16 *prev_1, u16 *prev_2, s32 in)
-{
-	s32 out_1 = *prev_1;
-	s32 out_2 = *prev_2;
-	s32 val;
-
-	if (!in)
-		in += 1;
-
-	if (!out_1) {
-		val = out_1 = in;
-		goto out;
-	}
-
-	val = MINSTREL_AVG_COEFF1 * in;
-	val += MINSTREL_AVG_COEFF2 * out_1;
-	val += MINSTREL_AVG_COEFF3 * out_2;
-	val >>= MINSTREL_SCALE;
-
-	if (val > 1 << MINSTREL_SCALE)
-		val = 1 << MINSTREL_SCALE;
-	if (val < 0)
-		val = 1;
-
-out:
-	*prev_2 = out_1;
-	*prev_1 = val;
-
-	return val;
-}
-
-struct minstrel_rate_stats {
-	/* current / last sampling period attempts/success counters */
-	u16 attempts, last_attempts;
-	u16 success, last_success;
-
-	/* total attempts/success counters */
-	u32 att_hist, succ_hist;
-
-	/* prob_avg - moving average of prob */
-	u16 prob_avg;
-	u16 prob_avg_1;
-
-	/* maximum retry counts */
-	u8 retry_count;
-	u8 retry_count_rtscts;
-
-	u8 sample_skipped;
-	bool retry_updated;
-};
-
-struct minstrel_rate {
-	int bitrate;
-
-	s8 rix;
-	u8 retry_count_cts;
-	u8 adjusted_retry_count;
-
-	unsigned int perfect_tx_time;
-	unsigned int ack_time;
-
-	int sample_limit;
-
-	struct minstrel_rate_stats stats;
-};
-
-struct minstrel_sta_info {
-	struct ieee80211_sta *sta;
-
-	unsigned long last_stats_update;
-	unsigned int sp_ack_dur;
-	unsigned int rate_avg;
-
-	unsigned int lowest_rix;
-
-	u8 max_tp_rate[MAX_THR_RATES];
-	u8 max_prob_rate;
-	unsigned int total_packets;
-	unsigned int sample_packets;
-
-	unsigned int sample_row;
-	unsigned int sample_column;
-
-	int n_rates;
-	struct minstrel_rate *r;
-	bool prev_sample;
-
-	/* sampling table */
-	u8 *sample_table;
-};
-
-struct minstrel_priv {
-	struct ieee80211_hw *hw;
-	bool has_mrr;
-	bool new_avg;
-	u32 sample_switch;
-	unsigned int cw_min;
-	unsigned int cw_max;
-	unsigned int max_retry;
-	unsigned int segment_size;
-	unsigned int update_interval;
-	unsigned int lookaround_rate;
-	unsigned int lookaround_rate_mrr;
-
-	u8 cck_rates[4];
-	u8 ofdm_rates[NUM_NL80211_BANDS][8];
-
-#ifdef CPTCFG_MAC80211_DEBUGFS
-	/*
-	 * enable fixed rate processing per RC
-	 *   - write static index to debugfs:ieee80211/phyX/rc/fixed_rate_idx
-	 *   - write -1 to enable RC processing again
-	 *   - setting will be applied on next update
-	 */
-	u32 fixed_rate_idx;
-#endif
-};
-
-struct minstrel_debugfs_info {
-	size_t len;
-	char buf[];
-};
-
-extern const struct rate_control_ops mac80211_minstrel;
-void minstrel_add_sta_debugfs(void *priv, void *priv_sta, struct dentry *dir);
-
-/* Recalculate success probabilities and counters for a given rate using EWMA */
-void minstrel_calc_rate_stats(struct minstrel_priv *mp,
-			      struct minstrel_rate_stats *mrs);
-int minstrel_get_tp_avg(struct minstrel_rate *mr, int prob_avg);
-
-/* debugfs */
-int minstrel_stats_open(struct inode *inode, struct file *file);
-int minstrel_stats_csv_open(struct inode *inode, struct file *file);
-
-#endif
--- a/net/mac80211/rc80211_minstrel_debugfs.c
+++ /dev/null
@@ -1,172 +0,0 @@
-/*
- * Copyright (C) 2008 Felix Fietkau <nbd@openwrt.org>
- *
- * This program is free software; you can redistribute it and/or modify
- * it under the terms of the GNU General Public License version 2 as
- * published by the Free Software Foundation.
- *
- * Based on minstrel.c:
- *   Copyright (C) 2005-2007 Derek Smithies <derek@indranet.co.nz>
- *   Sponsored by Indranet Technologies Ltd
- *
- * Based on sample.c:
- *   Copyright (c) 2005 John Bicket
- *   All rights reserved.
- *
- *   Redistribution and use in source and binary forms, with or without
- *   modification, are permitted provided that the following conditions
- *   are met:
- *   1. Redistributions of source code must retain the above copyright
- *      notice, this list of conditions and the following disclaimer,
- *      without modification.
- *   2. Redistributions in binary form must reproduce at minimum a disclaimer
- *      similar to the "NO WARRANTY" disclaimer below ("Disclaimer") and any
- *      redistribution must be conditioned upon including a substantially
- *      similar Disclaimer requirement for further binary redistribution.
- *   3. Neither the names of the above-listed copyright holders nor the names
- *      of any contributors may be used to endorse or promote products derived
- *      from this software without specific prior written permission.
- *
- *   Alternatively, this software may be distributed under the terms of the
- *   GNU General Public License ("GPL") version 2 as published by the Free
- *   Software Foundation.
- *
- *   NO WARRANTY
- *   THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
- *   ``AS IS'' AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
- *   LIMITED TO, THE IMPLIED WARRANTIES OF NONINFRINGEMENT, MERCHANTIBILITY
- *   AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL
- *   THE COPYRIGHT HOLDERS OR CONTRIBUTORS BE LIABLE FOR SPECIAL, EXEMPLARY,
- *   OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
- *   SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
- *   INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER
- *   IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
- *   ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF
- *   THE POSSIBILITY OF SUCH DAMAGES.
- */
-#include <linux/netdevice.h>
-#include <linux/types.h>
-#include <linux/skbuff.h>
-#include <linux/debugfs.h>
-#include <linux/ieee80211.h>
-#include <linux/slab.h>
-#include <linux/export.h>
-#include <net/mac80211.h>
-#include "rc80211_minstrel.h"
-
-int
-minstrel_stats_open(struct inode *inode, struct file *file)
-{
-	struct minstrel_sta_info *mi = inode->i_private;
-	struct minstrel_debugfs_info *ms;
-	unsigned int i, tp_max, tp_avg, eprob;
-	char *p;
-
-	ms = kmalloc(2048, GFP_KERNEL);
-	if (!ms)
-		return -ENOMEM;
-
-	file->private_data = ms;
-	p = ms->buf;
-	p += sprintf(p, "\n");
-	p += sprintf(p,
-		     "best   __________rate_________    ____statistics___    ____last_____    ______sum-of________\n");
-	p += sprintf(p,
-		     "rate  [name idx airtime max_tp]  [avg(tp) avg(prob)]  [retry|suc|att]  [#success | #attempts]\n");
-
-	for (i = 0; i < mi->n_rates; i++) {
-		struct minstrel_rate *mr = &mi->r[i];
-		struct minstrel_rate_stats *mrs = &mi->r[i].stats;
-
-		*(p++) = (i == mi->max_tp_rate[0]) ? 'A' : ' ';
-		*(p++) = (i == mi->max_tp_rate[1]) ? 'B' : ' ';
-		*(p++) = (i == mi->max_tp_rate[2]) ? 'C' : ' ';
-		*(p++) = (i == mi->max_tp_rate[3]) ? 'D' : ' ';
-		*(p++) = (i == mi->max_prob_rate) ? 'P' : ' ';
-
-		p += sprintf(p, " %3u%s ", mr->bitrate / 2,
-				(mr->bitrate & 1 ? ".5" : "  "));
-		p += sprintf(p, "%3u  ", i);
-		p += sprintf(p, "%6u ", mr->perfect_tx_time);
-
-		tp_max = minstrel_get_tp_avg(mr, MINSTREL_FRAC(100,100));
-		tp_avg = minstrel_get_tp_avg(mr, mrs->prob_avg);
-		eprob = MINSTREL_TRUNC(mrs->prob_avg * 1000);
-
-		p += sprintf(p, "%4u.%1u    %4u.%1u     %3u.%1u"
-				"     %3u   %3u %-3u   "
-				"%9llu   %-9llu\n",
-				tp_max / 10, tp_max % 10,
-				tp_avg / 10, tp_avg % 10,
-				eprob / 10, eprob % 10,
-				mrs->retry_count,
-				mrs->last_success,
-				mrs->last_attempts,
-				(unsigned long long)mrs->succ_hist,
-				(unsigned long long)mrs->att_hist);
-	}
-	p += sprintf(p, "\nTotal packet count::    ideal %d      "
-			"lookaround %d\n\n",
-			mi->total_packets - mi->sample_packets,
-			mi->sample_packets);
-	ms->len = p - ms->buf;
-
-	WARN_ON(ms->len + sizeof(*ms) > 2048);
-
-	return 0;
-}
-
-int
-minstrel_stats_csv_open(struct inode *inode, struct file *file)
-{
-	struct minstrel_sta_info *mi = inode->i_private;
-	struct minstrel_debugfs_info *ms;
-	unsigned int i, tp_max, tp_avg, eprob;
-	char *p;
-
-	ms = kmalloc(2048, GFP_KERNEL);
-	if (!ms)
-		return -ENOMEM;
-
-	file->private_data = ms;
-	p = ms->buf;
-
-	for (i = 0; i < mi->n_rates; i++) {
-		struct minstrel_rate *mr = &mi->r[i];
-		struct minstrel_rate_stats *mrs = &mi->r[i].stats;
-
-		p += sprintf(p, "%s" ,((i == mi->max_tp_rate[0]) ? "A" : ""));
-		p += sprintf(p, "%s" ,((i == mi->max_tp_rate[1]) ? "B" : ""));
-		p += sprintf(p, "%s" ,((i == mi->max_tp_rate[2]) ? "C" : ""));
-		p += sprintf(p, "%s" ,((i == mi->max_tp_rate[3]) ? "D" : ""));
-		p += sprintf(p, "%s" ,((i == mi->max_prob_rate) ? "P" : ""));
-
-		p += sprintf(p, ",%u%s", mr->bitrate / 2,
-				(mr->bitrate & 1 ? ".5," : ","));
-		p += sprintf(p, "%u,", i);
-		p += sprintf(p, "%u,",mr->perfect_tx_time);
-
-		tp_max = minstrel_get_tp_avg(mr, MINSTREL_FRAC(100,100));
-		tp_avg = minstrel_get_tp_avg(mr, mrs->prob_avg);
-		eprob = MINSTREL_TRUNC(mrs->prob_avg * 1000);
-
-		p += sprintf(p, "%u.%u,%u.%u,%u.%u,%u,%u,%u,"
-				"%llu,%llu,%d,%d\n",
-				tp_max / 10, tp_max % 10,
-				tp_avg / 10, tp_avg % 10,
-				eprob / 10, eprob % 10,
-				mrs->retry_count,
-				mrs->last_success,
-				mrs->last_attempts,
-				(unsigned long long)mrs->succ_hist,
-				(unsigned long long)mrs->att_hist,
-				mi->total_packets - mi->sample_packets,
-				mi->sample_packets);
-
-	}
-	ms->len = p - ms->buf;
-
-	WARN_ON(ms->len + sizeof(*ms) > 2048);
-
-	return 0;
-}
--- a/net/mac80211/rc80211_minstrel_ht.c
+++ b/net/mac80211/rc80211_minstrel_ht.c
@@ -13,7 +13,6 @@
 #include <net/mac80211.h>
 #include "rate.h"
 #include "sta_info.h"
-#include "rc80211_minstrel.h"
 #include "rc80211_minstrel_ht.h"
 
 #define AVG_AMPDU_SIZE	16
@@ -716,6 +715,83 @@ out:
 	mi->sample_mode = MINSTREL_SAMPLE_ACTIVE;
 }
 
+static inline int
+minstrel_ewma(int old, int new, int weight)
+{
+	int diff, incr;
+
+	diff = new - old;
+	incr = (EWMA_DIV - weight) * diff / EWMA_DIV;
+
+	return old + incr;
+}
+
+static inline int minstrel_filter_avg_add(u16 *prev_1, u16 *prev_2, s32 in)
+{
+	s32 out_1 = *prev_1;
+	s32 out_2 = *prev_2;
+	s32 val;
+
+	if (!in)
+		in += 1;
+
+	if (!out_1) {
+		val = out_1 = in;
+		goto out;
+	}
+
+	val = MINSTREL_AVG_COEFF1 * in;
+	val += MINSTREL_AVG_COEFF2 * out_1;
+	val += MINSTREL_AVG_COEFF3 * out_2;
+	val >>= MINSTREL_SCALE;
+
+	if (val > 1 << MINSTREL_SCALE)
+		val = 1 << MINSTREL_SCALE;
+	if (val < 0)
+		val = 1;
+
+out:
+	*prev_2 = out_1;
+	*prev_1 = val;
+
+	return val;
+}
+
+/*
+* Recalculate statistics and counters of a given rate
+*/
+static void
+minstrel_ht_calc_rate_stats(struct minstrel_priv *mp,
+			    struct minstrel_rate_stats *mrs)
+{
+	unsigned int cur_prob;
+
+	if (unlikely(mrs->attempts > 0)) {
+		mrs->sample_skipped = 0;
+		cur_prob = MINSTREL_FRAC(mrs->success, mrs->attempts);
+		if (mp->new_avg) {
+			minstrel_filter_avg_add(&mrs->prob_avg,
+						&mrs->prob_avg_1, cur_prob);
+		} else if (unlikely(!mrs->att_hist)) {
+			mrs->prob_avg = cur_prob;
+		} else {
+			/*update exponential weighted moving avarage */
+			mrs->prob_avg = minstrel_ewma(mrs->prob_avg,
+						      cur_prob,
+						      EWMA_LEVEL);
+		}
+		mrs->att_hist += mrs->attempts;
+		mrs->succ_hist += mrs->success;
+	} else {
+		mrs->sample_skipped++;
+	}
+
+	mrs->last_success = mrs->success;
+	mrs->last_attempts = mrs->attempts;
+	mrs->success = 0;
+	mrs->attempts = 0;
+}
+
 /*
  * Update rate statistics and select new primary rates
  *
@@ -808,7 +884,7 @@ minstrel_ht_update_stats(struct minstrel
 
 			mrs = &mg->rates[i];
 			mrs->retry_updated = false;
-			minstrel_calc_rate_stats(mp, mrs);
+			minstrel_ht_calc_rate_stats(mp, mrs);
 			cur_prob = mrs->prob_avg;
 
 			if (minstrel_ht_get_tp_avg(mi, group, i, cur_prob) == 0)
@@ -960,8 +1036,7 @@ minstrel_ht_tx_status(void *priv, struct
                       void *priv_sta, struct ieee80211_tx_status *st)
 {
 	struct ieee80211_tx_info *info = st->info;
-	struct minstrel_ht_sta_priv *msp = priv_sta;
-	struct minstrel_ht_sta *mi = &msp->ht;
+	struct minstrel_ht_sta *mi = priv_sta;
 	struct ieee80211_tx_rate *ar = info->status.rates;
 	struct minstrel_rate_stats *rate, *rate2, *rate_sample = NULL;
 	struct minstrel_priv *mp = priv;
@@ -1372,8 +1447,7 @@ minstrel_ht_get_rate(void *priv, struct
 	const struct mcs_group *sample_group;
 	struct ieee80211_tx_info *info = IEEE80211_SKB_CB(txrc->skb);
 	struct ieee80211_tx_rate *rate = &info->status.rates[0];
-	struct minstrel_ht_sta_priv *msp = priv_sta;
-	struct minstrel_ht_sta *mi = &msp->ht;
+	struct minstrel_ht_sta *mi = priv_sta;
 	struct minstrel_priv *mp = priv;
 	int sample_idx;
 
@@ -1484,8 +1558,7 @@ minstrel_ht_update_caps(void *priv, stru
 			struct ieee80211_sta *sta, void *priv_sta)
 {
 	struct minstrel_priv *mp = priv;
-	struct minstrel_ht_sta_priv *msp = priv_sta;
-	struct minstrel_ht_sta *mi = &msp->ht;
+	struct minstrel_ht_sta *mi = priv_sta;
 	struct ieee80211_mcs_info *mcs = &sta->ht_cap.mcs;
 	u16 ht_cap = sta->ht_cap.cap;
 	struct ieee80211_sta_vht_cap *vht_cap = &sta->vht_cap;
@@ -1647,7 +1720,7 @@ static void *
 minstrel_ht_alloc_sta(void *priv, struct ieee80211_sta *sta, gfp_t gfp)
 {
 	struct ieee80211_supported_band *sband;
-	struct minstrel_ht_sta_priv *msp;
+	struct minstrel_ht_sta *mi;
 	struct minstrel_priv *mp = priv;
 	struct ieee80211_hw *hw = mp->hw;
 	int max_rates = 0;
@@ -1659,35 +1732,13 @@ minstrel_ht_alloc_sta(void *priv, struct
 			max_rates = sband->n_bitrates;
 	}
 
-	msp = kzalloc(sizeof(*msp), gfp);
-	if (!msp)
-		return NULL;
-
-	msp->ratelist = kcalloc(max_rates, sizeof(struct minstrel_rate), gfp);
-	if (!msp->ratelist)
-		goto error;
-
-	msp->sample_table = kmalloc_array(max_rates, SAMPLE_COLUMNS, gfp);
-	if (!msp->sample_table)
-		goto error1;
-
-	return msp;
-
-error1:
-	kfree(msp->ratelist);
-error:
-	kfree(msp);
-	return NULL;
+	return kzalloc(sizeof(*mi), gfp);
 }
 
 static void
 minstrel_ht_free_sta(void *priv, struct ieee80211_sta *sta, void *priv_sta)
 {
-	struct minstrel_ht_sta_priv *msp = priv_sta;
-
-	kfree(msp->sample_table);
-	kfree(msp->ratelist);
-	kfree(msp);
+	kfree(priv_sta);
 }
 
 static void
@@ -1768,12 +1819,6 @@ minstrel_ht_alloc(struct ieee80211_hw *h
 	mp->cw_min = 15;
 	mp->cw_max = 1023;
 
-	/* number of packets (in %) to use for sampling other rates
-	 * sample less often for non-mrr packets, because the overhead
-	 * is much higher than with mrr */
-	mp->lookaround_rate = 5;
-	mp->lookaround_rate_mrr = 10;
-
 	/* maximum time that the hw is allowed to stay in one MRR segment */
 	mp->segment_size = 6000;
 
@@ -1821,8 +1866,7 @@ minstrel_ht_free(void *priv)
 
 static u32 minstrel_ht_get_expected_throughput(void *priv_sta)
 {
-	struct minstrel_ht_sta_priv *msp = priv_sta;
-	struct minstrel_ht_sta *mi = &msp->ht;
+	struct minstrel_ht_sta *mi = priv_sta;
 	int i, j, prob, tp_avg;
 
 	i = mi->max_tp_rate[0] / MCS_GROUP_RATES;
--- a/net/mac80211/rc80211_minstrel_ht.h
+++ b/net/mac80211/rc80211_minstrel_ht.h
@@ -6,6 +6,33 @@
 #ifndef __RC_MINSTREL_HT_H
 #define __RC_MINSTREL_HT_H
 
+/* number of highest throughput rates to consider*/
+#define MAX_THR_RATES 4
+#define SAMPLE_COLUMNS	10	/* number of columns in sample table */
+
+/* scaled fraction values */
+#define MINSTREL_SCALE  12
+#define MINSTREL_FRAC(val, div) (((val) << MINSTREL_SCALE) / div)
+#define MINSTREL_TRUNC(val) ((val) >> MINSTREL_SCALE)
+
+#define EWMA_LEVEL	96	/* ewma weighting factor [/EWMA_DIV] */
+#define EWMA_DIV	128
+
+/*
+ * Coefficients for moving average with noise filter (period=16),
+ * scaled by 10 bits
+ *
+ * a1 = exp(-pi * sqrt(2) / period)
+ * coeff2 = 2 * a1 * cos(sqrt(2) * 2 * pi / period)
+ * coeff3 = -sqr(a1)
+ * coeff1 = 1 - coeff2 - coeff3
+ */
+#define MINSTREL_AVG_COEFF1		(MINSTREL_FRAC(1, 1) - \
+					 MINSTREL_AVG_COEFF2 - \
+					 MINSTREL_AVG_COEFF3)
+#define MINSTREL_AVG_COEFF2		0x00001499
+#define MINSTREL_AVG_COEFF3		-0x0000092e
+
 /*
  * The number of streams can be changed to 2 to reduce code
  * size and memory footprint.
@@ -30,6 +57,32 @@
 
 #define MCS_GROUP_RATES		10
 
+struct minstrel_priv {
+	struct ieee80211_hw *hw;
+	bool has_mrr;
+	bool new_avg;
+	u32 sample_switch;
+	unsigned int cw_min;
+	unsigned int cw_max;
+	unsigned int max_retry;
+	unsigned int segment_size;
+	unsigned int update_interval;
+
+	u8 cck_rates[4];
+	u8 ofdm_rates[NUM_NL80211_BANDS][8];
+
+#ifdef CPTCFG_MAC80211_DEBUGFS
+	/*
+	 * enable fixed rate processing per RC
+	 *   - write static index to debugfs:ieee80211/phyX/rc/fixed_rate_idx
+	 *   - write -1 to enable RC processing again
+	 *   - setting will be applied on next update
+	 */
+	u32 fixed_rate_idx;
+#endif
+};
+
+
 struct mcs_group {
 	u16 flags;
 	u8 streams;
@@ -42,6 +95,26 @@ extern const s16 minstrel_cck_bitrates[4
 extern const s16 minstrel_ofdm_bitrates[8];
 extern const struct mcs_group minstrel_mcs_groups[];
 
+struct minstrel_rate_stats {
+	/* current / last sampling period attempts/success counters */
+	u16 attempts, last_attempts;
+	u16 success, last_success;
+
+	/* total attempts/success counters */
+	u32 att_hist, succ_hist;
+
+	/* prob_avg - moving average of prob */
+	u16 prob_avg;
+	u16 prob_avg_1;
+
+	/* maximum retry counts */
+	u8 retry_count;
+	u8 retry_count_rtscts;
+
+	u8 sample_skipped;
+	bool retry_updated;
+};
+
 struct minstrel_mcs_group_data {
 	u8 index;
 	u8 column;
@@ -111,12 +184,6 @@ struct minstrel_ht_sta {
 	struct minstrel_mcs_group_data groups[MINSTREL_GROUPS_NB];
 };
 
-struct minstrel_ht_sta_priv {
-	struct minstrel_ht_sta ht;
-	void *ratelist;
-	void *sample_table;
-};
-
 void minstrel_ht_add_sta_debugfs(void *priv, void *priv_sta, struct dentry *dir);
 int minstrel_ht_get_tp_avg(struct minstrel_ht_sta *mi, int group, int rate,
 			   int prob_avg);
--- a/net/mac80211/rc80211_minstrel_ht_debugfs.c
+++ b/net/mac80211/rc80211_minstrel_ht_debugfs.c
@@ -9,9 +9,13 @@
 #include <linux/ieee80211.h>
 #include <linux/export.h>
 #include <net/mac80211.h>
-#include "rc80211_minstrel.h"
 #include "rc80211_minstrel_ht.h"
 
+struct minstrel_debugfs_info {
+	size_t len;
+	char buf[];
+};
+
 static ssize_t
 minstrel_stats_read(struct file *file, char __user *buf, size_t len, loff_t *ppos)
 {
@@ -127,8 +131,7 @@ minstrel_ht_stats_dump(struct minstrel_h
 static int
 minstrel_ht_stats_open(struct inode *inode, struct file *file)
 {
-	struct minstrel_ht_sta_priv *msp = inode->i_private;
-	struct minstrel_ht_sta *mi = &msp->ht;
+	struct minstrel_ht_sta *mi = inode->i_private;
 	struct minstrel_debugfs_info *ms;
 	unsigned int i;
 	char *p;
@@ -276,8 +279,7 @@ minstrel_ht_stats_csv_dump(struct minstr
 static int
 minstrel_ht_stats_csv_open(struct inode *inode, struct file *file)
 {
-	struct minstrel_ht_sta_priv *msp = inode->i_private;
-	struct minstrel_ht_sta *mi = &msp->ht;
+	struct minstrel_ht_sta *mi = inode->i_private;
 	struct minstrel_debugfs_info *ms;
 	unsigned int i;
 	char *p;
@@ -313,10 +315,8 @@ static const struct file_operations mins
 void
 minstrel_ht_add_sta_debugfs(void *priv, void *priv_sta, struct dentry *dir)
 {
-	struct minstrel_ht_sta_priv *msp = priv_sta;
-
-	debugfs_create_file("rc_stats", 0444, dir, msp,
+	debugfs_create_file("rc_stats", 0444, dir, priv_sta,
 			    &minstrel_ht_stat_fops);
-	debugfs_create_file("rc_stats_csv", 0444, dir, msp,
+	debugfs_create_file("rc_stats_csv", 0444, dir, priv_sta,
 			    &minstrel_ht_stat_csv_fops);
 }
