From d3e5e7f3a4e6f61e8c380b9a610212267ee72dbd Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?=C3=81lvaro=20Fern=C3=A1ndez=20Rojas?= <noltari@gmail.com>
Date: Sat, 20 Feb 2021 19:24:50 +0100
Subject: [PATCH] hwrng: iproc: set quality to 1000
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This allows khwrngd to make use of iproc-rng200.

Signed-off-by: Álvaro Fernández Rojas <noltari@gmail.com>
---
 drivers/char/hw_random/iproc-rng200.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/char/hw_random/iproc-rng200.c
+++ b/drivers/char/hw_random/iproc-rng200.c
@@ -270,6 +270,7 @@ static int iproc_rng200_probe(struct pla
 
 	priv->rng.name = pdev->name;
 	priv->rng.cleanup = iproc_rng200_cleanup;
+	priv->rng.quality = 1000;
 
 	if (of_device_is_compatible(dev->of_node, "brcm,bcm2711-rng200")) {
 		priv->rng.init = bcm2711_rng200_init;
