From a8254fa4ba60b85829b6e5ede6564f81cd70d59f Mon Sep 17 00:00:00 2001
From: YueHaibing <yuehaibing@huawei.com>
Date: Tue, 11 Sep 2018 11:24:04 +0800
Subject: [PATCH] brcmfmac: remove set but not used variables 'sfdoff' and
 'pad_size'

Fixes gcc '-Wunused-but-set-variable' warning:

drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c: In function 'brcmf_sdio_rxglom':
drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c:1466:11: warning:
 variable 'sfdoff' set but not used [-Wunused-but-set-variable]

drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c: In function 'brcmf_sdio_bus_preinit':
drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c:3408:7: warning:
 variable 'pad_size' set but not used [-Wunused-but-set-variable]

Signed-off-by: YueHaibing <yuehaibing@huawei.com>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---
 drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c | 5 +----
 1 file changed, 1 insertion(+), 4 deletions(-)

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
@@ -1480,7 +1480,7 @@ static u8 brcmf_sdio_rxglom(struct brcmf
 	struct sk_buff *pfirst, *pnext;
 
 	int errcode;
-	u8 doff, sfdoff;
+	u8 doff;
 
 	struct brcmf_sdio_hdrinfo rd_new;
 
@@ -1614,7 +1614,6 @@ static u8 brcmf_sdio_rxglom(struct brcmf
 
 		/* Remove superframe header, remember offset */
 		skb_pull(pfirst, rd_new.dat_offset);
-		sfdoff = rd_new.dat_offset;
 		num = 0;
 
 		/* Validate all the subframe headers */
@@ -3428,7 +3427,6 @@ static int brcmf_sdio_bus_preinit(struct
 	struct brcmf_sdio_dev *sdiodev = bus_if->bus_priv.sdio;
 	struct brcmf_sdio *bus = sdiodev->bus;
 	struct brcmf_core *core = bus->sdio_core;
-	uint pad_size;
 	u32 value;
 	int err;
 
@@ -3469,7 +3467,6 @@ static int brcmf_sdio_bus_preinit(struct
 	if (sdiodev->sg_support) {
 		bus->txglom = false;
 		value = 1;
-		pad_size = bus->sdiodev->func2->cur_blksize << 1;
 		err = brcmf_iovar_data_set(bus->sdiodev->dev, "bus:rxglom",
 					   &value, sizeof(u32));
 		if (err < 0) {
