From 7ae46019667c122c3e2a5a291b2cd5b62df524f9 Mon Sep 17 00:00:00 2001
From: Lukas Rusak <lorusak@gmail.com>
Date: Fri, 29 Jun 2018 10:13:59 -0700
Subject: [PATCH 338/454] arm: dts: bcm2710-rpi-3-b-plus: fix hpd gpio pin

Signed-off-by: Lukas Rusak <lorusak@gmail.com>
---
 arch/arm/boot/dts/bcm2710-rpi-3-b-plus.dts | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/bcm2710-rpi-3-b-plus.dts
+++ b/arch/arm/boot/dts/bcm2710-rpi-3-b-plus.dts
@@ -162,7 +162,7 @@
 };
 
 &hdmi {
-	hpd-gpios = <&expgpio 4 GPIO_ACTIVE_LOW>;
+	hpd-gpios = <&gpio 28 GPIO_ACTIVE_LOW>;
 };
 
 &audio {
