From 523c96b2a6127bdc1ebe4a35d59bc458cd77fe02 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.org>
Date: Wed, 11 Apr 2018 11:18:43 +0100
Subject: [PATCH 335/454] defconfig: Enable Unicam driver and various sources
 on Pi platforms.

Enable:
	VIDEO_V4L2_SUBDEV_API=y
	VIDEO_BCM2835_UNICAM=m
	VIDEO_TC358743=m
	VIDEO_ADV7180=m
	VIDEO_OV5647=m
so that we can receive CSI data from these devices.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.org>
---
 arch/arm/configs/bcm2709_defconfig | 5 +++++
 arch/arm/configs/bcmrpi_defconfig  | 5 +++++
 2 files changed, 10 insertions(+)

--- a/arch/arm/configs/bcm2709_defconfig
+++ b/arch/arm/configs/bcm2709_defconfig
@@ -697,6 +697,7 @@ CONFIG_MEDIA_ANALOG_TV_SUPPORT=y
 CONFIG_MEDIA_DIGITAL_TV_SUPPORT=y
 CONFIG_MEDIA_RADIO_SUPPORT=y
 CONFIG_MEDIA_CONTROLLER=y
+CONFIG_VIDEO_V4L2_SUBDEV_API=y
 CONFIG_MEDIA_USB_SUPPORT=y
 CONFIG_USB_VIDEO_CLASS=m
 CONFIG_USB_M5602=m
@@ -815,6 +816,7 @@ CONFIG_VIDEO_EM28XX_V4L2=m
 CONFIG_VIDEO_EM28XX_ALSA=m
 CONFIG_VIDEO_EM28XX_DVB=m
 CONFIG_V4L_PLATFORM_DRIVERS=y
+CONFIG_VIDEO_BCM2835_UNICAM=m
 CONFIG_RADIO_SI470X=y
 CONFIG_USB_SI470X=m
 CONFIG_I2C_SI470X=m
@@ -834,10 +836,13 @@ CONFIG_RADIO_WL128X=m
 # CONFIG_MEDIA_SUBDRV_AUTOSELECT is not set
 CONFIG_VIDEO_UDA1342=m
 CONFIG_VIDEO_SONY_BTF_MPX=m
+CONFIG_VIDEO_ADV7180=m
+CONFIG_VIDEO_TC358743=m
 CONFIG_VIDEO_TVP5150=m
 CONFIG_VIDEO_TW2804=m
 CONFIG_VIDEO_TW9903=m
 CONFIG_VIDEO_TW9906=m
+CONFIG_VIDEO_OV5647=m
 CONFIG_VIDEO_OV7640=m
 CONFIG_VIDEO_MT9V011=m
 CONFIG_DRM=m
--- a/arch/arm/configs/bcmrpi_defconfig
+++ b/arch/arm/configs/bcmrpi_defconfig
@@ -690,6 +690,7 @@ CONFIG_MEDIA_ANALOG_TV_SUPPORT=y
 CONFIG_MEDIA_DIGITAL_TV_SUPPORT=y
 CONFIG_MEDIA_RADIO_SUPPORT=y
 CONFIG_MEDIA_CONTROLLER=y
+CONFIG_VIDEO_V4L2_SUBDEV_API=y
 CONFIG_MEDIA_USB_SUPPORT=y
 CONFIG_USB_VIDEO_CLASS=m
 CONFIG_USB_M5602=m
@@ -808,6 +809,7 @@ CONFIG_VIDEO_EM28XX_V4L2=m
 CONFIG_VIDEO_EM28XX_ALSA=m
 CONFIG_VIDEO_EM28XX_DVB=m
 CONFIG_V4L_PLATFORM_DRIVERS=y
+CONFIG_VIDEO_BCM2835_UNICAM=m
 CONFIG_RADIO_SI470X=y
 CONFIG_USB_SI470X=m
 CONFIG_I2C_SI470X=m
@@ -827,10 +829,13 @@ CONFIG_RADIO_WL128X=m
 # CONFIG_MEDIA_SUBDRV_AUTOSELECT is not set
 CONFIG_VIDEO_UDA1342=m
 CONFIG_VIDEO_SONY_BTF_MPX=m
+CONFIG_VIDEO_ADV7180=m
+CONFIG_VIDEO_TC358743=m
 CONFIG_VIDEO_TVP5150=m
 CONFIG_VIDEO_TW2804=m
 CONFIG_VIDEO_TW9903=m
 CONFIG_VIDEO_TW9906=m
+CONFIG_VIDEO_OV5647=m
 CONFIG_VIDEO_OV7640=m
 CONFIG_VIDEO_MT9V011=m
 CONFIG_DRM=m
