From 84a10b20192ae300833b1f630f078ed8825bbfa9 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Tue, 12 Jun 2018 10:16:07 +0100
Subject: [PATCH 312/454] config: Add CONFIG_SPI_GPIO

See: https://github.com/raspberrypi/linux/pull/2318

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/configs/bcm2709_defconfig | 1 +
 arch/arm/configs/bcmrpi_defconfig  | 1 +
 2 files changed, 2 insertions(+)

--- a/arch/arm/configs/bcm2709_defconfig
+++ b/arch/arm/configs/bcm2709_defconfig
@@ -618,6 +618,7 @@ CONFIG_I2C_TINY_USB=m
 CONFIG_SPI=y
 CONFIG_SPI_BCM2835=m
 CONFIG_SPI_BCM2835AUX=m
+CONFIG_SPI_GPIO=m
 CONFIG_SPI_SPIDEV=m
 CONFIG_SPI_SLAVE=y
 CONFIG_PPS=m
--- a/arch/arm/configs/bcmrpi_defconfig
+++ b/arch/arm/configs/bcmrpi_defconfig
@@ -613,6 +613,7 @@ CONFIG_I2C_TINY_USB=m
 CONFIG_SPI=y
 CONFIG_SPI_BCM2835=m
 CONFIG_SPI_BCM2835AUX=m
+CONFIG_SPI_GPIO=m
 CONFIG_SPI_SPIDEV=m
 CONFIG_SPI_SLAVE=y
 CONFIG_PPS=m
