From 182f9c510f98a2cefec44762a35cd5c00fd98709 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Tue, 2 Jan 2024 19:32:25 +0000
Subject: [PATCH 0811/1085] drm/vc4: Fixup of patches adding debugfs functions

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/gpu/drm/vc4/vc4_hvs.c | 12 ++++++------
 1 file changed, 6 insertions(+), 6 deletions(-)

--- a/drivers/gpu/drm/vc4/vc4_hvs.c
+++ b/drivers/gpu/drm/vc4/vc4_hvs.c
@@ -221,8 +221,8 @@ static int vc4_hvs_debugfs_dlist(struct
 
 static int vc6_hvs_debugfs_dlist(struct seq_file *m, void *data)
 {
-	struct drm_info_node *node = m->private;
-	struct drm_device *dev = node->minor->dev;
+	struct drm_debugfs_entry *entry = m->private;
+	struct drm_device *dev = entry->dev;
 	struct vc4_dev *vc4 = to_vc4_dev(dev);
 	struct vc4_hvs *hvs = vc4->hvs;
 	struct drm_printer p = drm_seq_file_printer(m);
@@ -270,8 +270,8 @@ static int vc6_hvs_debugfs_dlist(struct
 
 static int vc5_hvs_debugfs_gamma(struct seq_file *m, void *data)
 {
-	struct drm_info_node *node = m->private;
-	struct drm_device *dev = node->minor->dev;
+	struct drm_debugfs_entry *entry = m->private;
+	struct drm_device *dev = entry->dev;
 	struct vc4_dev *vc4 = to_vc4_dev(dev);
 	struct vc4_hvs *hvs = vc4->hvs;
 	struct drm_printer p = drm_seq_file_printer(m);
@@ -349,8 +349,8 @@ static int vc5_hvs_debugfs_gamma(struct
 
 static int vc4_hvs_debugfs_dlist_allocs(struct seq_file *m, void *data)
 {
-	struct drm_info_node *node = m->private;
-	struct drm_device *dev = node->minor->dev;
+	struct drm_debugfs_entry *entry = m->private;
+	struct drm_device *dev = entry->dev;
 	struct vc4_dev *vc4 = to_vc4_dev(dev);
 	struct vc4_hvs *hvs = vc4->hvs;
 	struct drm_printer p = drm_seq_file_printer(m);
