From: Sumit Gupta <sumitg@nvidia.com>
To: <catalin.marinas@arm.com>, <linux-arm-kernel@lists.infradead.org>,
	<linux-kernel@vger.kernel.org>
Cc: <will.deacon@arm.com>, <suzuki.poulose@arm.com>,
	<james.morse@arm.com>, <mark.rutland@arm.com>,
	<yang.shi@linaro.org>, <julien.grall@arm.com>,
	<steve.capper@linaro.org>, <bbasu@nvidia.com>,
	<linux-tegra@vger.kernel.org>, Sumit Gupta <sumitg@nvidia.com>
Subject: [PATCH] arm64: cpuinfo: Add "model name" in /proc/cpuinfo for 64bit tasks also
Date: Mon, 29 Aug 2016 14:32:25 +0530
Message-ID: <1472461345-28219-1-git-send-email-sumitg@nvidia.com> (raw)

Removed restriction of displaying model name for 32 bit tasks only.
Because of this Processor details were not displayed in
"System setting -> Details" in Ubuntu model name display is generic
and can be printed for 64 bit also.

model name : ARMv8 Processor rev X (v8l)

Signed-off-by: Sumit Gupta <sumitg@nvidia.com>
---
 arch/arm64/kernel/cpuinfo.c | 3 +--
 1 file changed, 1 insertion(+), 2 deletions(-)

--- a/arch/arm64/kernel/cpuinfo.c
+++ b/arch/arm64/kernel/cpuinfo.c
@@ -189,9 +189,8 @@ static int c_show(struct seq_file *m, vo
 		 * "processor".  Give glibc what it expects.
 		 */
 		seq_printf(m, "processor\t: %d\n", i);
-		if (compat)
-			seq_printf(m, "model name\t: ARMv8 Processor rev %d (%s)\n",
-				   MIDR_REVISION(midr), COMPAT_ELF_PLATFORM);
+		seq_printf(m, "model name\t: ARMv8 Processor rev %d (%s)\n",
+			   MIDR_REVISION(midr), COMPAT_ELF_PLATFORM);
 
 		seq_printf(m, "BogoMIPS\t: %lu.%02lu\n",
 			   loops_per_jiffy / (500000UL/HZ),
