From acadf3a63b39ad03167a633fa3cea8c0fc2ab87f Mon Sep 17 00:00:00 2001
From: Nick Morrow <usbwifi2024@gmail.com>
Date: Thu, 7 Nov 2024 08:28:46 +0800
Subject: [PATCH 6/6] wifi: rtw88: Add additional USB IDs for RTL8812BU

Add three additional USB IDs found in
https://github.com/morrownr/88x2bu-20210702
to support more RTL8812BU devices.

Signed-off-by: Nick Morrow <usbwifi2024@gmail.com>
Signed-off-by: Zenm Chen <zenmchen@gmail.com>
Signed-off-by: Mikhail Novosyolov <m.novosyolov@rosalinux.ru>
---
 drivers/net/wireless/realtek/rtw88/rtw8822bu.c | 6 ++++++
 1 file changed, 6 insertions(+)

--- a/drivers/net/wireless/realtek/rtw88/rtw8822bu.c
+++ b/drivers/net/wireless/realtek/rtw88/rtw8822bu.c
@@ -67,6 +67,12 @@ static const struct usb_device_id rtw_88
 	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* LiteOn */
 	{ USB_DEVICE_AND_INTERFACE_INFO(0x20f4, 0x808a, 0xff, 0xff, 0xff),
 	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* TRENDnet TEW-808UBM */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x20f4, 0x805a, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* TRENDnet TEW-805UBH */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x056e, 0x4011, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* ELECOM WDB-867DU3S */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x2c4e, 0x0107, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* Mercusys MA30H */
 	{},
 };
 MODULE_DEVICE_TABLE(usb, rtw_8822bu_id_table);
